APIs in Category: fcp | Cluster-Mode API version 1.15

fcp-adapter-config-down fcp-adapter-config-up fcp-adapter-get-iter fcp-adapter-set-speed fcp-adapter-stats-get-iter fcp-initiator-get-iter fcp-interface-get-iter fcp-port-name-get-iter fcp-service-get-iter fcp-wwpnalias-get-iter

NetApp Manage ONTAP

fcp-adapter-config-down | [top]

> Bring a Fibre Channel target adapter offline. The adapter may not be offline immediately after the call returns, it may take up to a few seconds for the adapter to change state. In Data ONTAP 7-Mode, if the FCP service is not running then all adapters are automatically offlined. They cannot be brought online again until FCP service is started. adapter to change state. In Data ONTAP Cluster-Mode, offlining an adapter will operationally disable all FCP logical interfaces (LIFs) hosted by the adapter.

> Input Name | Range | Type | Description
> fcp-adapter |  | string | FC adapter to bring offline.
> node |  | string | The name of the storage system node where the adapter is installed.

> Errno | Description
> EINTERNALERROR |  |
> EADAPTERNOTFOUND |  |
> EADAPTERINVALIDTYPE |  |
> EADAPTERPARTNER |  |
> ENOTSTARTED |  |
> ENTAPI_EINVAL |  |

> License
> fcp

fcp-adapter-config-up | [top]

> Bring a Fibre Channel target adapter online. The adapter may not be online immediately after the call returns, it may take up to a few seconds for the adapter to initialize. In Data ONTAP 7-Mode, if the FCP service is not running then all adapters are automatically offlined. They cannot be brought online again until FCP service is started. In Data ONTAP Cluster-Mode, offlining an adapter will operationally disable all FCP logical interfaces (LIFs) hosted by the adapter.

> Input Name | Range | Type | Description
> fcp-adapter |  | string | FC adapter to bring online.
> node |  | string | The name of the storage system node where the adapter is installed.

> Errno | Description
> EINTERNALERROR |  |
> EADAPTERNOTFOUND |  |
> EADAPTERINVALIDTYPE |  |
> EADAPTERPARTNER |  |
> ENOTSTARTED |  |
> EONTAPI_EINVAL |  |

> License
> fcp

fcp-adapter-get-iter | [top]

> Iterate over the list of physical FC adapters.

> Input Name | Range | Type | Description
> desired-attributes |  | fcp-config-adapter-info optional | Specify the attributes that should be returned. If not present, all attributes for which information is available will be returned. If present, only the desired attributes for which information is available will be returned.
> max-records | [1..100] | integer optional | The maximum number of records to return in this call. Default: 20
> query |  | fcp-config-adapter-info optional | A query that specifies which objects to return. A query could be specified on any number of attributes in the FC Adapter object. All FC Adapter objects matching this query up to 'max-records' will be returned.
> tag |  | string optional | Specify the tag from the last call. It is usually not specified for the first call. For subsequent calls, copy values from the 'next-tag' obtained from the previous call.
> Output Name | Range | Type | Description
> attributes-list |  | fcp-config-adapter-info[] optional | The list of attributes of FC Adapter objects.
> next-tag |  | string optional | Tag for the next call. Not present when there are no more FC Adapter objects to return.
> num-records | [0..100] | integer | The number of records returned in this call.

> Errno | Description
> EINTERNALERROR |  |

fcp-adapter-set-speed | [top]

> Sets the speed on the Fibre Channel target adapter. It can be configured to run at 1Gb, 2Gb, 4Gb, or to autonegotiate. Note only 4Gb adapters support the 4Gb speed. If the adapter is online it must be brought offline before setting the speed, and then online in order for a new speed to take effect. This may temporarily disrupt fcp service on the target adapter.

> Input Name | Range | Type | Description
> fcp-adapter |  | string | FC Target adapter
> node |  | string | The name of the storage system node where the adapter is installed.
> speed |  | string | Link speed (in Gb). Possible values: "1", "2", "4", or "auto" (autonegotiate speed).

> Errno | Description
> EINTERNALERROR |  |
> EADAPTERNOTFOUND |  |
> EADAPTERINVALIDTYPE |  |
> EADAPTERPARTNER |  |
> ENOTSTARTED |  |
> EONTAPI_EINVAL |  |

> License
> fcp

fcp-adapter-stats-get-iter | [top]

> Iterate over a list of fcp objects.

> Input Name | Range | Type | Description
> desired-attributes |  | fcp-adapter-stats-info optional | Specify the attributes that should be returned. If not present, all attributes for which information is available will be returned. If present, only the desired attributes for which information is available will be returned.
> max-records | [1..100] | integer optional | The maximum number of records to return in this call. Default: 20
> query |  | fcp-adapter-stats-info optional | A query that specifies which objects to return. A query could be specified on any number of attributes in the fcp object. All fcp objects matching this query up to 'max-records' will be returned.
> tag |  | string optional | Specify the tag from the last call. It is usually not specified for the first call. For subsequent calls, copy values from the 'next-tag' obtained from the previous call.
> Output Name | Range | Type | Description
> attributes-list |  | fcp-adapter-stats-info[] optional | The list of attributes of fcp objects.
> next-tag |  | string optional | Tag for the next call. Not present when there are no more fcp objects to return.
> num-records | [0..100] | integer | The number of records returned in this call.

> Errno | Description
> EINTERNALERROR |  |

fcp-initiator-get-iter | [top]

> List all initiators connected to FCP target LIFs.

> Input Name | Range | Type | Description
> desired-attributes |  | fcp-adapter-initiators-info optional | Specify the attributes that should be returned. If not present, all attributes for which information is available will be returned. If present, only the desired attributes for which information is available will be returned.
> max-records | [1..100] | integer optional | The maximum number of records to return in this call. Default: 20
> query |  | fcp-adapter-initiators-info optional | A query that specifies which objects to return. A query could be specified on any number of attributes in the connected FCP initiator object. All connected FCP initiator objects matching this query up to 'max-records' will be returned.
> tag |  | string optional | Specify the tag from the last call. It is usually not specified for the first call. For subsequent calls, copy values from the 'next-tag' obtained from the previous call.
> Output Name | Range | Type | Description
> attributes-list |  | fcp-adapter-initiators-info[] optional | The list of attributes of connected FCP initiator objects.
> next-tag |  | string optional | Tag for the next call. Not present when there are no more connected FCP initiator objects to return.
> num-records | [0..100] | integer | The number of records returned in this call.

> Errno | Description
> EINTERNALERROR |  |

fcp-interface-get-iter | [top]

> Iterate over a list of FCP Target Logical Interfaces (LIF).

> Input Name | Range | Type | Description
> desired-attributes |  | fcp-interface-info optional | Specify the attributes that should be returned. If not present, all attributes for which information is available will be returned. If present, only the desired attributes for which information is available will be returned.
> max-records | [1..100] | integer optional | The maximum number of records to return in this call. Default: 20
> query |  | fcp-interface-info optional | A query that specifies which objects to return. A query could be specified on any number of attributes in the FCP data LIF object. All FCP data LIF objects matching this query up to 'max-records' will be returned.
> tag |  | string optional | Specify the tag from the last call. It is usually not specified for the first call. For subsequent calls, copy values from the 'next-tag' obtained from the previous call.
> Output Name | Range | Type | Description
> attributes-list |  | fcp-interface-info[] optional | The list of attributes of FCP data LIF objects.
> next-tag |  | string optional | Tag for the next call. Not present when there are no more FCP data LIF objects to return.
> num-records | [0..100] | integer | The number of records returned in this call.

> Errno | Description
> EINTERNALERROR |  |

fcp-port-name-get-iter | [top]

> Iterate over the list of valid Fibre Channel target port names on a Vserver's FCP LIFs.

> Input Name | Range | Type | Description
> desired-attributes |  | fcp-port-name-info optional | Specify the attributes that should be returned. If not present, all attributes for which information is available will be returned. If present, only the desired attributes for which information is available will be returned.
> max-records | [1..100] | integer optional | The maximum number of records to return in this call. Default: 20
> query |  | fcp-port-name-info optional | A query that specifies which objects to return. A query could be specified on any number of attributes in the Fibre Channel target port name object. All Fibre Channel target port name objects matching this query up to 'max-records' will be returned.
> tag |  | string optional | Specify the tag from the last call. It is usually not specified for the first call. For subsequent calls, copy values from the 'next-tag' obtained from the previous call.
> Output Name | Range | Type | Description
> attributes-list |  | fcp-port-name-info[] optional | The list of attributes of Fibre Channel target port name objects.
> next-tag |  | string optional | Tag for the next call. Not present when there are no more Fibre Channel target port name objects to return.
> num-records | [0..100] | integer | The number of records returned in this call.

> Errno | Description
> EINTERNALERROR |  |

fcp-service-get-iter | [top]

> Iterate over the list of FCP Services.

> Input Name | Range | Type | Description
> desired-attributes |  | fcp-service-info optional | Specify the attributes that should be returned. If not present, all attributes for which information is available will be returned. If present, only the desired attributes for which information is available will be returned.
> max-records | [1..100] | integer optional | The maximum number of records to return in this call. Default: 20
> query |  | fcp-service-info optional | A query that specifies which objects to return. A query could be specified on any number of attributes in the FCP Service object. All FCP Service objects matching this query up to 'max-records' will be returned.
> tag |  | string optional | Specify the tag from the last call. It is usually not specified for the first call. For subsequent calls, copy values from the 'next-tag' obtained from the previous call.
> Output Name | Range | Type | Description
> attributes-list |  | fcp-service-info[] optional | The list of attributes of FCP Service objects.
> next-tag |  | string optional | Tag for the next call. Not present when there are no more FCP Service objects to return.
> num-records | [0..100] | integer | The number of records returned in this call.

> Errno | Description
> EINTERNALERROR |  |

fcp-wwpnalias-get-iter | [top]

> Iterate over the list of assigned World Wide Port Name (WWPN) aliases.

> Input Name | Range | Type | Description
> desired-attributes |  | aliases-info optional | Specify the attributes that should be returned. If not present, all attributes for which information is available will be returned. If present, only the desired attributes for which information is available will be returned.
> max-records | [1..100] | integer optional | The maximum number of records to return in this call. Default: 20
> query |  | aliases-info optional | A query that specifies which objects to return. A query could be specified on any number of attributes in the WWPN aliases object. All WWPN aliases objects matching this query up to 'max-records' will be returned.
> tag |  | string optional | Specify the tag from the last call. It is usually not specified for the first call. For subsequent calls, copy values from the 'next-tag' obtained from the previous call.
> Output Name | Range | Type | Description
> attributes-list |  | aliases-info[] optional | The list of attributes of WWPN aliases objects.
> next-tag |  | string optional | Tag for the next call. Not present when there are no more WWPN aliases objects to return.
> num-records | [0..100] | integer | The number of records returned in this call.

> Errno | Description
> EINTERNALERROR |  |

Element definition: aliases-info | [top]

> A list of WWPNs and their aliases generated according to the input - alias, WWPN or nothing.

> Name | Range | Type | Description
> aliases-alias |  | string | The 32-character alias for a given FCP WWPN
> aliases-wwpn |  | string | The FCP WWPN for which the alias is given
> vserver |  | string optional | Vserver containing the alias

Element definition: fcp-adapter-initiators-info | [top]

> A list of initiators currently connected to the FC adapter or FCP data LIF.

> Name | Range | Type | Description
> adapter |  | string | In Data ONTAP 7-Mode, the name of the physical FC adapter. In Data ONTAP Cluser-Mode, the name of the FCP data LIF.
> fcp-connected-initiators |  | fcp-connected-initiator-info[] | Information about the connected initiators
> vserver |  | string optional | Vserver of the FCP LIF.

Element definition: fcp-adapter-stats-info | [top]

> Statistics for one FC adapter.

> Name | Range | Type | Description
> adapter |  | string | Which FC adapter.
> adapter-resets |  | integer | Number of adapter resets occurred.
> crc-errors |  | integer | Total CRC errors occurred.
> discarded-frames |  | integer | Number of frames discarded by the target HBA. Range [0..2^31-1]
> frame-overruns |  | integer | Number of frame overruns detected by the adapter during write requests.
> frame-underruns |  | integer | Number of frame underruns detected by the adapter during read requests.
> initiators-connected |  | integer | Total number of initiators connected to this target adapter.
> invalid-xmit-words |  | integer | Number of invalid words transmitted. Range [0..2^31-1]
> is-sfp-diagnostics-internally-calibrated |  | boolean | Indicates if the SFP diagnostics are internally calibrated or not. The optional SFP rx/tx fields are invalid (and therefore not provided) if the SFP diagnostics are not internally calibrated.
> is-sfp-optical-transceiver-valid |  | boolean | Validity of the optical transceiver. Until Data ONTAP 8.0.0, this field was incorrectly named "is-spf-optical-transceiver-valid". While that field is also returned for backward compatibility, all new applications must use the current version.
> is-sfp-rx-power-in-range |  | boolean optional | Flag to indicate received optical power is in range.
> is-sfp-tx-power-in-range |  | boolean optional | Flag to indicate transmitted optical power is in range.
> link-breaks |  | integer | Number of times that the link breaks.
> lip-resets |  | integer | Number of times that a selective Reset LIP (Loop Initialization Primitive) occurred. LIP reset is used to preform a verndorspecific reset at the loop port specified by the AL-PA value.
> lr-received |  | integer | Number of LRs (Link Reset) received by the target HBA. Range [0..2^31-1]
> lr-sent |  | integer | Number of LRs (Link Reset) sent from the target HBA. Range [0..2^31-1]
> nos-received |  | integer | Number of NOSs (Not_Operational Primitive Sequence)received by the target HBA. Range [0..2^31-1]
> ols-received |  | integer | Number of OLSs (Offline Primitive Sequence) received by the target HBA. Range [0..2^31-1]
> protocol-errors |  | integer | Number of protocol errors occured. Range [0..2^31-1]
> queue-depth |  | integer | Counts the queue depth on the target HBA.
> scsi-requests-dropped |  | integer | Number of SCSI requests being dropped.
> sfp-connector |  | string | Connector used with the optical transceiver.
> sfp-date-code |  | string | Date code for the optical transceiver.
> sfp-encoding |  | string | Encoding used with the optical transceiver. Possible values ["8B10B", "?????"]
> sfp-fc-speed-capabilties |  | string | FC speed capabilities for the optical transceiver. Possible values [1, 2, 4, 8 in Gbps]
> sfp-formfactor |  | string | Form factor of the optical transceiver. Possible values: "SFP" (for Small FormFactor).
> sfp-part-number |  | string | Part number for the optical transceiver.
> sfp-rev |  | string | Revision for the optical transceiver.
> sfp-rx-power |  | string optional | SFP received optical power, reported to tenth decimal in uWatts.
> sfp-serial-number |  | string | Serial number for the optical transceiver.
> sfp-tx-power |  | string optional | SFP transmitted optical power, reported to tenth decimal in uWatts.
> sfp-vendor-name |  | string | Vendor name for the optical transceiver.
> sfp-vendor-oui |  | string | Vendor OUI (The IEEE Organizationally Unique Identifier) for the optical transceiver.
> sfp-wavelength |  | integer | Wavelength for the optical transceiver. Measured in nanometers. Range [830..860]
> spurious-interrupts |  | integer | Count of spurious interrupts.
> total-logins |  | integer | Counts the times of initiators added. Each time a new initiator is added, the total logins is incremented by 1. Each time an initiator is removed, the total logouts is incremented by 1.
> total-logouts |  | integer | Counts the times of initiators removed. Each time a new initiator is added, the total logins is incremented by 1. Each time an initiator is removed, the total logouts is incremented by 1.

Element definition: fcp-config-adapter-info | [top]

> Configuration information for one physical FC adapter.

> Name | Range | Type | Description
> adapter |  | string | The slot name of the FC adapter.
> cache-line-size |  | integer optional | Cache line size of adapter. verbose only.
> connection-established |  | string optional | Type of connection established, "ptp" or "loop".
> data-link-rate |  | integer optional | Data Link Rate in Gbits. verbose only.
> external-gbic-enabled |  | boolean optional | "true" if enabled, "false" otherwise. verbose only.
> fabric-established |  | boolean optional | "true" if fabric is established to this adapter, "false" otherwise. verbose only.
> firmware-rev |  | string optional | Firmware revision of adapter. verbose only.
> hardware-rev |  | string optional | Hardware revision of adapter. verbose only.
> info-name |  | string optional | Info name given to this adapter. verbose only.
> max-speed | [1..10] | integer | The maximum speed of this adapter in Gbit/sec.
> media-type |  | string optional | Media configured for this adapter, "ptp", "loop", or "auto". If an error occured while retrieving info for this adapter, this will not be returned.
> mpi-firmware-rev |  | string optional | MPI Firmware revision of adapter. verbose only. This is only available for converged network adapters (CNA).
> node |  | string | The name of the node where the adapter is installed.
> node-name |  | string optional | FCP World Wide Node Name (WWNN) of the adapter. If an error occured while retrieving info for this adapter, this will not be returned.
> packet-size |  | integer optional | FC packet size of adapter. verbose only.
> pci-bus-width |  | integer optional | PCI bus width in bits. verbose only.
> pci-clock-speed |  | integer optional | PCI clock speed in MHz. verbose only.
> phy-firmware-rev |  | string optional | PHY Firmware revision of adapter. verbose only. This is only available for converged network adapters (CNA).
> physical-data-link-rate |  | integer optional | Physical Data Link Rate in Gbits. verbose only. This is only available for converged network adapters (CNA).
> physical-link-state |  | string optional | Physical Status of the adapter. verbose only. Possible values are "link up", "link down". This is only available for converged network adapters (CNA).
> physical-protocol |  | string | The physical protocol of the adapter. Possible values: "fibre_channel" - The adapter is a Fibre Channel adapter, "ethernet" - The adapter is a Fibre Channel over Ethernet adapter.
> port-address |  | integer optional | Host port address of adapter. If an error occured while retrieving info for this adapter, this will not be returned.
> port-name |  | string optional | FCP World Wide Port Name (WWPN) of adapter. If an error occured while retrieving info for this adapter, this will not be returned.
> speed |  | string optional | Speed configured for this adapter. Possible values: "auto", "1Gb", "2Gb", "4Gb", "8Gb", "10Gb". If an error occured while retrieving info for this adapter, this will not be returned.
> sram-parity-enabled |  | boolean optional | "true" if enabled, "false" otherwise. verbose only.
> state |  | string optional | Status of the adapter. Possible values are "startup", "uninitialized", "initializing firmware", "link not connected", "waiting for link up", "online", "link disconnected", "resetting", "offline", "offlined by user/system". If an error occured while retrieving info for this adapter, this will not be returned.
> switch-port |  | string optional | Switch and port this adapter is connected to. The string will be of the form X:Y where X is the name of the switch and Y is the port value. verbose only.
> vlan-id |  | integer optional | Assigned FC VLAN ID. verbose only. This is only available for converged network adapters (CNA).

Element definition: fcp-interface-info | [top]

> Information about a single FCP Logical Interface (LIF). When returned as part of the output, all elements of this typedef are reported, unless limited by a set of desired attributes specified by the caller. When used as input to specify desired attributes to return, omitting a given element indicates that it shall not be returned in the output. In contrast, by providing an element (even with no value) the caller ensures that a value for that element will be returned, given that the value can be retrieved. When used as input to specify queries, any element can be omitted in which case the resulting set of objects is not constrained by any specific value of that attribute.

> Name | Range | Type | Description
> current-node |  | string optional | Node currently hosting the LIF. Attributes: non-creatable, non-modifiable
> current-port |  | string optional | FC Adapter currently hosting the LIF. Attributes: non-creatable, non-modifiable
> interface-name |  | string optional | Name of the LIF. Attributes: key, required-for-create, non-modifiable
> node-name |  | string optional | World Wide Node Name (WWNN) of the LIF. All LIFs in a Vserver have the same WWNN as the Vserver's FCP service. Attributes: non-creatable, non-modifiable
> port-address |  | string optional | Host port address of LIF. Attributes: non-creatable, non-modifiable
> port-name |  | string optional | World Wide Port Name (WWPN) of the LIF. Attributes: non-creatable, non-modifiable
> relative-port-id |  | integer optional | The SCSI Relative Target Port Identifier of the LIF. Attributes: non-creatable, non-modifiable
> vserver |  | string optional | Vserver hosting the LIF. Attributes: key, non-creatable, non-modifiable

Element definition: fcp-port-name-info | [top]

> Information for one valid local port name.

> Name | Range | Type | Description
> fcp-adapter |  | string optional | Only if this WWPN is being used by a Fibre Channel interface, the name of the interface is returned. In Data ONTAP 7-Mode, the name of a local adapter. In Data ONTAP Cluster-Mode, the name of an FCP data LIF.
> is-used |  | boolean | This indicates whether this WWPN is being used by a Fibre Channel target interface.
> port-name |  | string | A Fibre Channel WWPN in the form XX:XX:XX:XX:XX:XX:XX:XX where X is a hexadecimal digit.
> vserver |  | string | Vserver containing this port name

Element definition: fcp-service-info | [top]

> FCP target service configuration. When returned as part of the output, all elements of this typedef are reported, unless limited by a set of desired attributes specified by the caller. When used as input to specify desired attributes to return, omitting a given element indicates that it shall not be returned in the output. In contrast, by providing an element (even with no value) the caller ensures that a value for that element will be returned, given that the value can be retrieved. When used as input to specify queries, any element can be omitted in which case the resulting set of objects is not constrained by any specific value of that attribute.

> Name | Range | Type | Description
> is-available |  | boolean optional | true if the FCP Service is running, false otherwise. Attributes: non-creatable, non-modifiable
> node-name |  | string optional | The world-wide node name (WWNN) of the FCP target in the Vserver. Attributes: optional-for-create, modifiable
> vserver |  | string optional | Vserver hosting the FCP service. Attributes: key, non-creatable, non-modifiable

Element definition: fcp-connected-initiator-info | [top]

> Information about an initiator connected to an FC adapter.

> Name | Range | Type | Description
> initiator-group-list |  | initiator-group-list-info[] | List of initiator groups this initiator belongs to.
> node-name |  | string | World Wide Node Name (WWNN) of initiator.
> port-address | [0..2^32-1] | integer | Fibre Channel host address it is connected to.
> port-name |  | string | World Wide Port Name (WWPN) of the initiator.
> portname-alias-list |  | portname-alias-name[] | List of aliases for the WWPN.

Element definition: initiator-group-list-info | [top]

> Initiator group this initiator belogs to.

> Name | Range | Type | Description
> initiator-group-name |  | string | Name of initiator group.

Element definition: portname-alias-name | [top]

> Aliases for this WWPN

> Name | Range | Type | Description
> portname-alias |  | string | Alias for the WWPN