APIs in Category: storage-initiator | API version 1.11

storage-initiator-balance storage-initiator-get-load | These APIs are used to get information on initiator ports as related to their role as a gateway to back end storage.

NetApp Manage ONTAP

storage-initiator-balance | [top]

> Balances primary/secondary array LUN paths across available initiator ports based on I/O load.

> Errno | Description
> EINTERNALERROR |  |

storage-initiator-get-load | [top]

> Gets array LUN I/O rates for a given fibre channel initiator port or for all initiator ports if no port is specified.

> Input Name | Range | Type | Description
> port |  | string optional | Port to show load on, e.g. 0a.
> Output Name | Range | Type | Description
> load-info |  | storage-initiator-load-info[] | A table of per array LUN load related information for the named port.

Element definition: storage-initiator-load-info | [top]

> Contains per port per LUN load information.

> Name | Range | Type | Description
> initiator-port |  | string | Initiator port name, e.g. 0a. If port is not specified, data for all ports is returned.
> io-count |  | integer | Megabytes of data sent to this array LUN over this port. Range: [0..2^32-1]
> lun-number |  | integer | LU number. Range: [0..65535]
> nodename |  | string | IP address of the node serving the port in dotted-decimal format (for example, "192.168.11.12").
> percent-io |  | string | Percentage of all I/O on this port sent to this array LUN. between 0.0 and 100.0%
> serial-number |  | string | Disk/LUN serial number. Maximum length of 129 characters.
> switch-name |  | string | The name of the switch connected to the controllers' initiator port, or N/A when using direct attach
> target-wwpn |  | string | World Wide Port Name of array's target port.