APIs in Category: autosupport | Cluster-Mode API version 1.15

autosupport-budget-get autosupport-budget-get-iter autosupport-budget-get-total-records autosupport-budget-modify autosupport-config-get autosupport-config-get-iter autosupport-config-get-total-records autosupport-config-modify autosupport-destinations-get autosupport-destinations-get-iter autosupport-destinations-get-total-records autosupport-history-get autosupport-history-get-iter autosupport-history-get-total-records autosupport-history-retransmit autosupport-invoke autosupport-manifest-get-iter autosupport-manifest-get-total-records autosupport-trigger-get autosupport-trigger-get-iter autosupport-trigger-get-total-records autosupport-trigger-modify | This set of ZAPIs provides visibility into the AutoSupport infrastructure of the system. The AutoSupport tool collects valuable information on the state of each node in the cluster, which aids in the diagnosis of hardware and software failures.The APIs are divided into the following major features: Configuration: manage AutoSupport general settings Destinations: view the current AutoSupport delivery destinations Triggers: manage what is collected for each AutoSupport trigger Manifest: view detailed collection information for a particular AutoSupport History: view a log of previously generated AutoSupports Budgets: manage AutoSupport collection size and time limits

NetApp Manage ONTAP

autosupport-budget-get | [top]

> Get AutoSupport time and size limits for the given node and subsystem.

> Input Name | Range | Type | Description
> desired-attributes |  | autosupport-budget-info optional | Specify the attributes that should be returned. If not present, all attributes for which information is available will be returned. If present, only the desired attributes for which information is available will be returned.
> node-name |  | string | The name of a filer on which the AutoSupport tool is running.
> subsystem |  | asup-subsystems | The name of a subsystem from which AutoSupport collects data. Possible values: "platform" - Hardware information about the node, "mhost" - User Space application information for a node, "log_files" - Log files for a node, "performance" - This subsystem gathers the .cm_stats_hourly_done file and user space counters, "performance_asup" - Performance specific information for a node, "nht" - This subsystem gathers the /mroot/etc/log/nht_info content, "san" - SAN specific information for a node, "snapvault" - SNAPVAULT specific information for a node, "snapmirror" - Snapmirror specific information for a node, "dedupe" - Dedupe specific information for a node, "nfs" - NFS specific information for a node, "wafl" - WAFL specific information for a node, "mot" - MOT specific information for a node, "ha" - HA specific information for a node, "networking" - Networking specific information for a node, "cifs" - CIFS specific information for a node, "fpolicy" - Fpolicy specific information for a node, "multistore" - Multistore specific information for a node, "raid" - RAID specific information for a node, "storage" - Storage specific information for a node, "asup_ems" - ASUP EMS specific information for a node, "tape" - Tape specific information for a node, "kernel" - kernel specific information for a node, "secd" - SECD specific information for a node, "metrocluster" - Metrocluster specific information for a node, "mandatory" - Mandatory Basic information for a node
> Output Name | Range | Type | Description
> attributes |  | autosupport-budget-info | The attributes of the autosupport-budget.

> Errno | Description
> EOBJECTNOTFOUND |  |
> EINTERNALERROR |  |

autosupport-budget-get-iter | [top]

> Get AutoSupport time and size limits per subsystem for all nodes.

> Input Name | Range | Type | Description
> desired-attributes |  | autosupport-budget-info optional | Specify the attributes that should be returned. If not present, all attributes for which information is available will be returned. If present, only the desired attributes for which information is available will be returned.
> max-records | [1..100] | integer optional | The maximum number of records to return in this call. Default: 20
> query |  | autosupport-budget-info optional | A query that specifies which objects to return. A query could be specified on any number of attributes in the autosupport-budget object. All autosupport-budget objects matching this query up to 'max-records' will be returned.
> tag |  | string optional | Specify the tag from the last call. It is usually not specified for the first call. For subsequent calls, copy values from the 'next-tag' obtained from the previous call.
> Output Name | Range | Type | Description
> attributes-list |  | autosupport-budget-info[] optional | The list of attributes of autosupport-budget objects.
> next-tag |  | string optional | Tag for the next call. Not present when there are no more autosupport-budget objects to return.
> num-records | [0..100] | integer | The number of records returned in this call.

> Errno | Description
> EINTERNALERROR |  |

autosupport-budget-get-total-records | [top]

> Return the total number of records.

> Output Name | Range | Type | Description
> count | [0..2^64-1] | integer | The total number of autosupport-budget objects.

autosupport-budget-modify | [top]

> Modify AutoSupport time and size limits per subsystem.

> Input Name | Range | Type | Description
> node-name |  | string | The name of a filer on which the AutoSupport tool is running.
> size-limit | [0..2^63-1] | integer optional | The maximum allowable collection size (in bytes) for the subsystem.
> subsystem |  | asup-subsystems | The name of a subsystem from which AutoSupport collects data. Possible values: "platform" - Hardware information about the node, "mhost" - User Space application information for a node, "log_files" - Log files for a node, "performance" - This subsystem gathers the .cm_stats_hourly_done file and user space counters, "performance_asup" - Performance specific information for a node, "nht" - This subsystem gathers the /mroot/etc/log/nht_info content, "san" - SAN specific information for a node, "snapvault" - SNAPVAULT specific information for a node, "snapmirror" - Snapmirror specific information for a node, "dedupe" - Dedupe specific information for a node, "nfs" - NFS specific information for a node, "wafl" - WAFL specific information for a node, "mot" - MOT specific information for a node, "ha" - HA specific information for a node, "networking" - Networking specific information for a node, "cifs" - CIFS specific information for a node, "fpolicy" - Fpolicy specific information for a node, "multistore" - Multistore specific information for a node, "raid" - RAID specific information for a node, "storage" - Storage specific information for a node, "asup_ems" - ASUP EMS specific information for a node, "tape" - Tape specific information for a node, "kernel" - kernel specific information for a node, "secd" - SECD specific information for a node, "metrocluster" - Metrocluster specific information for a node, "mandatory" - Mandatory Basic information for a node
> time-limit | [0..2^32-1] | integer optional | The maximum allowable collection time (in seconds ) for the subsystem.

> Errno | Description
> EOBJECTNOTFOUND |  |
> EINTERNALERROR |  |

autosupport-config-get | [top]

> Get AutoSupport configuration settings for the given node.

> Input Name | Range | Type | Description
> desired-attributes |  | autosupport-config-info optional | Specify the attributes that should be returned. If not present, all attributes for which information is available will be returned. If present, only the desired attributes for which information is available will be returned.
> node-name |  | string | The name of the filer that owns the AutoSupport configuration.
> Output Name | Range | Type | Description
> attributes |  | autosupport-config-info | The attributes of the autosupport-config.

> Errno | Description
> EOBJECTNOTFOUND |  |
> EINTERNALERROR |  |

autosupport-config-get-iter | [top]

> Get AutoSupport configuration settings for all nodes.

> Input Name | Range | Type | Description
> desired-attributes |  | autosupport-config-info optional | Specify the attributes that should be returned. If not present, all attributes for which information is available will be returned. If present, only the desired attributes for which information is available will be returned.
> max-records | [1..100] | integer optional | The maximum number of records to return in this call. Default: 20
> query |  | autosupport-config-info optional | A query that specifies which objects to return. A query could be specified on any number of attributes in the autosupport-config object. All autosupport-config objects matching this query up to 'max-records' will be returned.
> tag |  | string optional | Specify the tag from the last call. It is usually not specified for the first call. For subsequent calls, copy values from the 'next-tag' obtained from the previous call.
> Output Name | Range | Type | Description
> attributes-list |  | autosupport-config-info[] optional | The list of attributes of autosupport-config objects.
> next-tag |  | string optional | Tag for the next call. Not present when there are no more autosupport-config objects to return.
> num-records | [0..100] | integer | The number of records returned in this call.

> Errno | Description
> EINTERNALERROR |  |

autosupport-config-get-total-records | [top]

> Return the total number of records.

> Output Name | Range | Type | Description
> count | [0..2^64-1] | integer | The total number of autosupport-config objects.

autosupport-config-modify | [top]

> Modify AutoSupport configuration settings for the given node.

> Input Name | Range | Type | Description
> from |  | mail-address optional | The e-mail address of the local administrator, used as the sender of the AutoSupport message.
> is-enabled |  | boolean optional | Specifies whether the AutoSupport daemon is enabled. When this setting is disabled, delivery of all AutoSupport messages is turned off.
> is-local-collection-enabled |  | boolean optional | Used to enable / disable collection of AutoSupport data when the AutoSupport daemon is disabled. When this setting is true, collection of AutoSupport data will still be done if is-enabled is false.
> is-nht-data-enabled |  | boolean optional | Used to enable / disable collection of NetApp Health Trigger data.
> is-node-in-subject |  | boolean optional | Specifies whether the filer's hostname should be part of an AutoSupport message's subject field.
> is-perf-data-enabled |  | boolean optional | Used to enable / disable collection of Performance AutoSupport data.
> is-private-data-removed |  | boolean optional | Used to enable / disable removal of customer-supplied data.
> is-reminder-enabled |  | boolean optional | Specifies whether to enable / disable AutoSupport reminders.
> is-support-enabled |  | boolean optional | Specifies whether AutoSupport notification to Support is enabled.
> is-throttle-enabled |  | boolean optional | Specifies whether to enable / disable throttling to prevent a potential avalanche of AutoSupport messages.
> mail-hosts |  | string[] optional | The name of the mail server(s) used to deliver AutoSupport messages via SMTP. Both host names and IP addresses may be used as valid input.
> max-http-size | [0..2^63-1] | integer optional | Delivery size limit for the HTTP transport protocol (in bytes).
> max-smtp-size | [0..2^63-1] | integer optional | Delivery size limit for the SMTP transport protocol (in bytes).
> node-name |  | string | The name of the filer that owns the AutoSupport configuration.
> noteto |  | mail-address[] optional | Specifies up to five recipients of short AutoSupport e-mail messages.
> partner-address |  | mail-address[] optional | Specifies up to five partner vendor recipients of full AutoSupport e-mail messages.
> payload-format |  | compression-format optional | The format used to compress the AutoSupport message payload. Possible values: "7z" - 7-Zip Archive, "tgz" - Zipped Tarball
> periodic-tx-window | [0..2^32-1] | integer optional | The transmission window (seconds).
> post-url |  | string optional | The URL used to deliver AutoSupport messages via HTTP POST.
> proxy-url |  | string optional | Optional proxy host for AutoSupport message delivery via HTTP.
> put-url |  | string optional | The URL used to deliver AutoSupport messages via HTTP PUT.
> retry-count | [0..2^32-1] | integer optional | The maximum number of delivery attempts for an AutoSupport message.
> retry-interval | [0..2^32-1] | integer optional | The number of seconds to wait, after a failed delivery attempt, prior to re-transmitting an AutoSupport message.
> support-address |  | mail-address[] optional | The e-mail address of Support.
> to |  | mail-address[] optional | Specifies up to five recipients of full AutoSupport e-mail messages.
> transport |  | asup-transport optional | The name of the transport protocol used to deliver AutoSupport messages. Possible values: "smtp" , "http" , "https"

> Errno | Description
> EOBJECTNOTFOUND |  |
> EINTERNALERROR |  |

autosupport-destinations-get | [top]

> Get the list of AutoSupport destinations for the given node.

> Input Name | Range | Type | Description
> desired-attributes |  | autosupport-destinations-info optional | Specify the attributes that should be returned. If not present, all attributes for which information is available will be returned. If present, only the desired attributes for which information is available will be returned.
> node-name |  | string | The name of the filer that owns this destination configuration.
> Output Name | Range | Type | Description
> attributes |  | autosupport-destinations-info | The attributes of the autosupport-destinations.

> Errno | Description
> EOBJECTNOTFOUND |  |
> EINTERNALERROR |  |

autosupport-destinations-get-iter | [top]

> Get the list of AutoSupport destinations for all nodes.

> Input Name | Range | Type | Description
> desired-attributes |  | autosupport-destinations-info optional | Specify the attributes that should be returned. If not present, all attributes for which information is available will be returned. If present, only the desired attributes for which information is available will be returned.
> max-records | [1..100] | integer optional | The maximum number of records to return in this call. Default: 20
> query |  | autosupport-destinations-info optional | A query that specifies which objects to return. A query could be specified on any number of attributes in the autosupport-destinations object. All autosupport-destinations objects matching this query up to 'max-records' will be returned.
> tag |  | string optional | Specify the tag from the last call. It is usually not specified for the first call. For subsequent calls, copy values from the 'next-tag' obtained from the previous call.
> Output Name | Range | Type | Description
> attributes-list |  | autosupport-destinations-info[] optional | The list of attributes of autosupport-destinations objects.
> next-tag |  | string optional | Tag for the next call. Not present when there are no more autosupport-destinations objects to return.
> num-records | [0..100] | integer | The number of records returned in this call.

> Errno | Description
> EINTERNALERROR |  |

autosupport-destinations-get-total-records | [top]

> Return the total number of records. This sould be equal to the number of nodes in the cluster.

> Output Name | Range | Type | Description
> count | [0..2^64-1] | integer | The total number of autosupport-destinations objects.

autosupport-history-get | [top]

> Get a history record for the given AutoSupport.

> Input Name | Range | Type | Description
> desired-attributes |  | autosupport-history-info optional | Specify the attributes that should be returned. If not present, all attributes for which information is available will be returned. If present, only the desired attributes for which information is available will be returned.
> destination |  | asup-destination | The transport protocol for this AutoSupport message's destination. Possible values: "smtp" , "http" , "noteto" , "retransmit"
> node-name |  | string | The name of the filer where the AutoSupport message was previously generated.
> seq-num | [0..2^64-1] | integer | The AutoSupport message sequence number.
> Output Name | Range | Type | Description
> attributes |  | autosupport-history-info | The attributes of the autosupport-history.

> Errno | Description
> EOBJECTNOTFOUND |  |
> EINTERNALERROR |  |

autosupport-history-get-iter | [top]

> Get the history records for the last 50 AutoSupport messages.

> Input Name | Range | Type | Description
> desired-attributes |  | autosupport-history-info optional | Specify the attributes that should be returned. If not present, all attributes for which information is available will be returned. If present, only the desired attributes for which information is available will be returned.
> max-records | [1..100] | integer optional | The maximum number of records to return in this call. Default: 20
> query |  | autosupport-history-info optional | A query that specifies which objects to return. A query could be specified on any number of attributes in the autosupport-history object. All autosupport-history objects matching this query up to 'max-records' will be returned.
> tag |  | string optional | Specify the tag from the last call. It is usually not specified for the first call. For subsequent calls, copy values from the 'next-tag' obtained from the previous call.
> Output Name | Range | Type | Description
> attributes-list |  | autosupport-history-info[] optional | The list of attributes of autosupport-history objects.
> next-tag |  | string optional | Tag for the next call. Not present when there are no more autosupport-history objects to return.
> num-records | [0..100] | integer | The number of records returned in this call.

> Errno | Description
> EINTERNALERROR |  |

autosupport-history-get-total-records | [top]

> Return the total number of records.

> Output Name | Range | Type | Description
> count | [0..2^64-1] | integer | The total number of autosupport-history objects.

autosupport-history-retransmit | [top]

> Selectively retransmit a previously collected AutoSupport message.

> Input Name | Range | Type | Description
> node-name |  | string | Node
> seq-num | [0..2^64-1] | integer | AutoSupport Sequence Number
> size-limit | [0..2^63-1] | integer optional | Transmit Size Limit for this AutoSupport.
> uri |  | string | Destination to Send this AutoSupport

> Errno | Description
> EOBJECTNOTFOUND |  |
> EINTERNALERROR |  |

autosupport-invoke | [top]

> Generate a new AutoSupport message

> Input Name | Range | Type | Description
> force |  | boolean optional | Force generation, even if AutoSupport is disabled in the system. The default value is false.
> message |  | string optional | Text to include as part of the subject of the AutoSupport message.
> node-name |  | string | The name of the filer on which the AutoSupport message will be generated.
> type |  | asup-invoke-style optional | The type of AutoSupport to generate. Possible values: "test" - Test AutoSupport send and receive only, "performance" - Generate a Performance AutoSupport as requested by NetApp Support, "all" - Send all AutoSupport data without time or size limit, as requested by NetApp Support
> uri |  | string optional | Alternate destination for the AutoSupport. If this field is omitted, the AutoSupport will be delivered to the currently configured destinations.

> Errno | Description
> EOBJECTNOTFOUND |  |
> EINTERNALERROR |  |

autosupport-manifest-get-iter | [top]

> Get a detailed manifest for the contents of an AutoSupport.

> Input Name | Range | Type | Description
> desired-attributes |  | autosupport-manifest-info optional | Specify the attributes that should be returned. If not present, all attributes for which information is available will be returned. If present, only the desired attributes for which information is available will be returned.
> max-records | [1..100] | integer optional | The maximum number of records to return in this call. Default: 20
> query |  | autosupport-manifest-info optional | A query that specifies which objects to return. A query could be specified on any number of attributes in the autosupport-manifest object. All autosupport-manifest objects matching this query up to 'max-records' will be returned.
> tag |  | string optional | Specify the tag from the last call. It is usually not specified for the first call. For subsequent calls, copy values from the 'next-tag' obtained from the previous call.
> Output Name | Range | Type | Description
> attributes-list |  | autosupport-manifest-info[] optional | The list of attributes of autosupport-manifest objects.
> next-tag |  | string optional | Tag for the next call. Not present when there are no more autosupport-manifest objects to return.
> num-records | [0..100] | integer | The number of records returned in this call.

> Errno | Description
> EINTERNALERROR |  |

autosupport-manifest-get-total-records | [top]

> Return the total number of records.

> Output Name | Range | Type | Description
> count | [0..2^64-1] | integer | The total number of autosupport-manifest objects.

autosupport-trigger-get | [top]

> Get the AutoSupport trigger data for the given node and EMS message.

> Input Name | Range | Type | Description
> desired-attributes |  | autosupport-trigger-info optional | Specify the attributes that should be returned. If not present, all attributes for which information is available will be returned. If present, only the desired attributes for which information is available will be returned.
> node-name |  | string | Node
> trigger |  | string | EMS Message
> Output Name | Range | Type | Description
> attributes |  | autosupport-trigger-info | The attributes of the autosupport-trigger.

> Errno | Description
> EOBJECTNOTFOUND |  |
> EINTERNALERROR |  |

autosupport-trigger-get-iter | [top]

> Get a list of the AutoSupport trigger data for all nodes.

> Input Name | Range | Type | Description
> desired-attributes |  | autosupport-trigger-info optional | Specify the attributes that should be returned. If not present, all attributes for which information is available will be returned. If present, only the desired attributes for which information is available will be returned.
> max-records | [1..100] | integer optional | The maximum number of records to return in this call. Default: 20
> query |  | autosupport-trigger-info optional | A query that specifies which objects to return. A query could be specified on any number of attributes in the autosupport-trigger object. All autosupport-trigger objects matching this query up to 'max-records' will be returned.
> tag |  | string optional | Specify the tag from the last call. It is usually not specified for the first call. For subsequent calls, copy values from the 'next-tag' obtained from the previous call.
> Output Name | Range | Type | Description
> attributes-list |  | autosupport-trigger-info[] optional | The list of attributes of autosupport-trigger objects.
> next-tag |  | string optional | Tag for the next call. Not present when there are no more autosupport-trigger objects to return.
> num-records | [0..100] | integer | The number of records returned in this call.

> Errno | Description
> EINTERNALERROR |  |

autosupport-trigger-get-total-records | [top]

> Return the total number of records.

> Output Name | Range | Type | Description
> count | [0..2^64-1] | integer | The total number of autosupport-trigger objects.

autosupport-trigger-modify | [top]

> Modify the AutoSupport trigger data for the given node and EMS message.

> Input Name | Range | Type | Description
> basic-additional |  | asup-subsystems[] optional | Additional Subsystems Reporting Basic Info Possible values: "platform" - Hardware information about the node, "mhost" - User Space application information for a node, "log_files" - Log files for a node, "performance" - This subsystem gathers the .cm_stats_hourly_done file and user space counters, "performance_asup" - Performance specific information for a node, "nht" - This subsystem gathers the /mroot/etc/log/nht_info content, "san" - SAN specific information for a node, "snapvault" - SNAPVAULT specific information for a node, "snapmirror" - Snapmirror specific information for a node, "dedupe" - Dedupe specific information for a node, "nfs" - NFS specific information for a node, "wafl" - WAFL specific information for a node, "mot" - MOT specific information for a node, "ha" - HA specific information for a node, "networking" - Networking specific information for a node, "cifs" - CIFS specific information for a node, "fpolicy" - Fpolicy specific information for a node, "multistore" - Multistore specific information for a node, "raid" - RAID specific information for a node, "storage" - Storage specific information for a node, "asup_ems" - ASUP EMS specific information for a node, "tape" - Tape specific information for a node, "kernel" - kernel specific information for a node, "secd" - SECD specific information for a node, "metrocluster" - Metrocluster specific information for a node, "mandatory" - Mandatory Basic information for a node
> node-name |  | string | Node
> noteto-enabled |  | boolean optional | Deliver to AutoSupport -noteto Addresses
> time-limit | [0..2^32-1] | integer optional | The data collection time budget for this trigger (in seconds). Content not collected will be marked as collection-truncated-time-limit in the manifest.
> to-enabled |  | boolean optional | Deliver to AutoSupport -to Addresses
> trigger |  | string | EMS Message
> troubleshooting-additional |  | asup-subsystems[] optional | Additional Subsystems Reporting Troubleshooting Info Possible values: "platform" - Hardware information about the node, "mhost" - User Space application information for a node, "log_files" - Log files for a node, "performance" - This subsystem gathers the .cm_stats_hourly_done file and user space counters, "performance_asup" - Performance specific information for a node, "nht" - This subsystem gathers the /mroot/etc/log/nht_info content, "san" - SAN specific information for a node, "snapvault" - SNAPVAULT specific information for a node, "snapmirror" - Snapmirror specific information for a node, "dedupe" - Dedupe specific information for a node, "nfs" - NFS specific information for a node, "wafl" - WAFL specific information for a node, "mot" - MOT specific information for a node, "ha" - HA specific information for a node, "networking" - Networking specific information for a node, "cifs" - CIFS specific information for a node, "fpolicy" - Fpolicy specific information for a node, "multistore" - Multistore specific information for a node, "raid" - RAID specific information for a node, "storage" - Storage specific information for a node, "asup_ems" - ASUP EMS specific information for a node, "tape" - Tape specific information for a node, "kernel" - kernel specific information for a node, "secd" - SECD specific information for a node, "metrocluster" - Metrocluster specific information for a node, "mandatory" - Mandatory Basic information for a node

> Errno | Description
> EOBJECTNOTFOUND |  |
> EINTERNALERROR |  |

Element definition: asup-destination | [top]

> smtp|http|noteto|retransmit Possible values: "smtp" , "http" , "noteto" , "retransmit"

> [none]

Element definition: asup-invoke-style | [top]

> test|performance|all Possible values: "test" - Test AutoSupport send and receive only, "performance" - Generate a Performance AutoSupport as requested by NetApp Support, "all" - Send all AutoSupport data without time or size limit, as requested by NetApp Support

> [none]

Element definition: asup-subsystems | [top]

> AutoSupport collection subsystems Possible values: "platform" - Hardware information about the node, "mhost" - User Space application information for a node, "log_files" - Log files for a node, "performance" - This subsystem gathers the .cm_stats_hourly_done file and user space counters, "performance_asup" - Performance specific information for a node, "nht" - This subsystem gathers the /mroot/etc/log/nht_info content, "san" - SAN specific information for a node, "snapvault" - SNAPVAULT specific information for a node, "snapmirror" - Snapmirror specific information for a node, "dedupe" - Dedupe specific information for a node, "nfs" - NFS specific information for a node, "wafl" - WAFL specific information for a node, "mot" - MOT specific information for a node, "ha" - HA specific information for a node, "networking" - Networking specific information for a node, "cifs" - CIFS specific information for a node, "fpolicy" - Fpolicy specific information for a node, "multistore" - Multistore specific information for a node, "raid" - RAID specific information for a node, "storage" - Storage specific information for a node, "asup_ems" - ASUP EMS specific information for a node, "tape" - Tape specific information for a node, "kernel" - kernel specific information for a node, "secd" - SECD specific information for a node, "metrocluster" - Metrocluster specific information for a node, "mandatory" - Mandatory Basic information for a node

> [none]

Element definition: asup-transport | [top]

> smtp|http|https Possible values: "smtp" , "http" , "https"

> [none]

Element definition: autosupport-budget-info | [top]

> AutoSupport budget data When returned as part of the output, all elements of this typedef are reported, unless limited by a set of desired attributes specified by the caller. When used as input to specify desired attributes to return, omitting a given element indicates that it shall not be returned in the output. In contrast, by providing an element (even with no value) the caller ensures that a value for that element will be returned, given that the value can be retrieved. When used as input to specify queries, any element can be omitted in which case the resulting set of objects is not constrained by any specific value of that attribute.

> Name | Range | Type | Description
> node-name |  | string optional | The name of a filer on which the AutoSupport tool is running. Attributes: key, non-creatable, non-modifiable
> size-limit | [0..2^63-1] | integer optional | The maximum allowable collection size (in bytes) for the subsystem. Attributes: non-creatable, modifiable
> subsystem |  | asup-subsystems optional | The name of a subsystem from which AutoSupport collects data. Attributes: key, non-creatable, non-modifiable Possible values: "platform" - Hardware information about the node, "mhost" - User Space application information for a node, "log_files" - Log files for a node, "performance" - This subsystem gathers the .cm_stats_hourly_done file and user space counters, "performance_asup" - Performance specific information for a node, "nht" - This subsystem gathers the /mroot/etc/log/nht_info content, "san" - SAN specific information for a node, "snapvault" - SNAPVAULT specific information for a node, "snapmirror" - Snapmirror specific information for a node, "dedupe" - Dedupe specific information for a node, "nfs" - NFS specific information for a node, "wafl" - WAFL specific information for a node, "mot" - MOT specific information for a node, "ha" - HA specific information for a node, "networking" - Networking specific information for a node, "cifs" - CIFS specific information for a node, "fpolicy" - Fpolicy specific information for a node, "multistore" - Multistore specific information for a node, "raid" - RAID specific information for a node, "storage" - Storage specific information for a node, "asup_ems" - ASUP EMS specific information for a node, "tape" - Tape specific information for a node, "kernel" - kernel specific information for a node, "secd" - SECD specific information for a node, "metrocluster" - Metrocluster specific information for a node, "mandatory" - Mandatory Basic information for a node
> time-limit | [0..2^32-1] | integer optional | The maximum allowable collection time (in seconds ) for the subsystem. Attributes: non-creatable, modifiable

Element definition: autosupport-config-info | [top]

> AutoSupport configuration data When returned as part of the output, all elements of this typedef are reported, unless limited by a set of desired attributes specified by the caller. When used as input to specify desired attributes to return, omitting a given element indicates that it shall not be returned in the output. In contrast, by providing an element (even with no value) the caller ensures that a value for that element will be returned, given that the value can be retrieved. When used as input to specify queries, any element can be omitted in which case the resulting set of objects is not constrained by any specific value of that attribute.

> Name | Range | Type | Description
> from |  | mail-address optional | The e-mail address of the local administrator, used as the sender of the AutoSupport message. Attributes: non-creatable, modifiable
> is-enabled |  | boolean optional | Specifies whether the AutoSupport daemon is enabled. When this setting is disabled, delivery of all AutoSupport messages is turned off. Attributes: non-creatable, modifiable
> is-local-collection-enabled |  | boolean optional | Used to enable / disable collection of AutoSupport data when the AutoSupport daemon is disabled. When this setting is true, collection of AutoSupport data will still be done if is-enabled is false. Attributes: non-creatable, modifiable
> is-nht-data-enabled |  | boolean optional | Used to enable / disable collection of NetApp Health Trigger data. Attributes: non-creatable, modifiable
> is-node-in-subject |  | boolean optional | Specifies whether the filer's hostname should be part of an AutoSupport message's subject field. Attributes: non-creatable, modifiable
> is-perf-data-enabled |  | boolean optional | Used to enable / disable collection of Performance AutoSupport data. Attributes: non-creatable, modifiable
> is-private-data-removed |  | boolean optional | Used to enable / disable removal of customer-supplied data. Attributes: non-creatable, modifiable
> is-reminder-enabled |  | boolean optional | Specifies whether to enable / disable AutoSupport reminders. Attributes: non-creatable, modifiable
> is-support-enabled |  | boolean optional | Specifies whether AutoSupport notification to Support is enabled. Attributes: non-creatable, modifiable
> is-throttle-enabled |  | boolean optional | Specifies whether to enable / disable throttling to prevent a potential avalanche of AutoSupport messages. Attributes: non-creatable, modifiable
> last-subject |  | string optional | The subject field of the last generated AutoSupport message. Attributes: non-creatable, non-modifiable
> last-timestamp | [0..2^31-1] | integer optional | The timestamp of the last generated AutoSupport message. The time value is in seconds since January 1, 1970 UTC. Attributes: non-creatable, non-modifiable
> last-trigger |  | string optional | The EMS trigger of the last generated AutoSupport message. Attributes: non-creatable, non-modifiable
> mail-hosts |  | string[] optional | The name of the mail server(s) used to deliver AutoSupport messages via SMTP. Both host names and IP addresses may be used as valid input. Attributes: non-creatable, modifiable
> max-http-size | [0..2^63-1] | integer optional | Delivery size limit for the HTTP transport protocol (in bytes). Attributes: non-creatable, modifiable
> max-smtp-size | [0..2^63-1] | integer optional | Delivery size limit for the SMTP transport protocol (in bytes). Attributes: non-creatable, modifiable
> node-name |  | string optional | The name of the filer that owns the AutoSupport configuration. Attributes: key, non-creatable, non-modifiable
> noteto |  | mail-address[] optional | Specifies up to five recipients of short AutoSupport e-mail messages. Attributes: non-creatable, modifiable
> partner-address |  | mail-address[] optional | Specifies up to five partner vendor recipients of full AutoSupport e-mail messages. Attributes: non-creatable, modifiable
> payload-format |  | compression-format optional | The format used to compress the AutoSupport message payload. Attributes: non-creatable, modifiable Possible values: "7z" - 7-Zip Archive, "tgz" - Zipped Tarball
> periodic-tx-window | [0..2^32-1] | integer optional | The transmission window (seconds). Attributes: non-creatable, modifiable
> post-url |  | string optional | The URL used to deliver AutoSupport messages via HTTP POST. Attributes: non-creatable, modifiable
> proxy-url |  | string optional | Optional proxy host for AutoSupport message delivery via HTTP. Attributes: non-creatable, modifiable
> put-url |  | string optional | The URL used to deliver AutoSupport messages via HTTP PUT. Attributes: non-creatable, modifiable
> retry-count | [0..2^32-1] | integer optional | The maximum number of delivery attempts for an AutoSupport message. Attributes: non-creatable, modifiable
> retry-interval | [0..2^32-1] | integer optional | The number of seconds to wait, after a failed delivery attempt, prior to re-transmitting an AutoSupport message. Attributes: non-creatable, modifiable
> support-address |  | mail-address[] optional | The e-mail address of Support. Attributes: non-creatable, modifiable
> to |  | mail-address[] optional | Specifies up to five recipients of full AutoSupport e-mail messages. Attributes: non-creatable, modifiable
> transport |  | asup-transport optional | The name of the transport protocol used to deliver AutoSupport messages. Attributes: non-creatable, modifiable Possible values: "smtp" , "http" , "https"

Element definition: autosupport-destinations-info | [top]

> AutoSupport destination summary When returned as part of the output, all elements of this typedef are reported, unless limited by a set of desired attributes specified by the caller. When used as input to specify desired attributes to return, omitting a given element indicates that it shall not be returned in the output. In contrast, by providing an element (even with no value) the caller ensures that a value for that element will be returned, given that the value can be retrieved. When used as input to specify queries, any element can be omitted in which case the resulting set of objects is not constrained by any specific value of that attribute.

> Name | Range | Type | Description
> destinations |  | string[] optional | A comma separated list of destinations used to deliver AutoSupport messages. Attributes: non-creatable, non-modifiable
> node-name |  | string optional | The name of the filer that owns this destination configuration. Attributes: key, non-creatable, non-modifiable

Element definition: autosupport-history-info | [top]

> AutoSupport history data When returned as part of the output, all elements of this typedef are reported, unless limited by a set of desired attributes specified by the caller. When used as input to specify desired attributes to return, omitting a given element indicates that it shall not be returned in the output. In contrast, by providing an element (even with no value) the caller ensures that a value for that element will be returned, given that the value can be retrieved. When used as input to specify queries, any element can be omitted in which case the resulting set of objects is not constrained by any specific value of that attribute.

> Name | Range | Type | Description
> attempt-count | [0..2^32-1] | integer optional | The number of attempted deliveries for this AutoSupport message. Attributes: non-creatable, non-modifiable
> destination |  | asup-destination optional | The transport protocol for this AutoSupport message's destination. Attributes: key, non-creatable, non-modifiable Possible values: "smtp" , "http" , "noteto" , "retransmit"
> last-modification-timestamp | [0..2^31-1] | integer optional | The timestamp of the last update to this history record. The time value is in seconds since January 1, 1970 UTC. Attributes: non-creatable, non-modifiable
> node-name |  | string optional | The name of the filer where the AutoSupport message was previously generated. Attributes: key, non-creatable, non-modifiable
> seq-num | [0..2^64-1] | integer optional | The AutoSupport message sequence number. Attributes: key, non-creatable, non-modifiable
> status |  | asup-status optional | The delivery status for this AutoSupport message. Attributes: non-creatable, non-modifiable Possible values: "initializing" - ASUP request is being processed, "collection_failed" - The AutoSupport Collection failed. See 'Last Error' for more information, "collection_in_progress" - The AutoSupport Collection is in progress, "queued" - ASUP is queued for delivery, "transmitting" - ASUP transmission is in progress, "sent_successful" - ASUP was successfully sent, "ignore" - ASUP was processed successfully but has no destinations configured, "re_queued" - ASUP transmission failed and has been re-queued, "transmission_failed" - ASUP transmission has failed and the retry limit has been exceeded
> subject |  | string optional | The subject field of this AutoSupport message. Attributes: non-creatable, non-modifiable
> trigger |  | string optional | The name of the EMS event that triggered this AutoSupport message. Attributes: non-creatable, non-modifiable
> uri |  | string optional | The URI used to deliver this AutoSupport message. Attributes: non-creatable, non-modifiable

Element definition: autosupport-manifest-info | [top]

> AutoSupport manifest data When returned as part of the output, all elements of this typedef are reported, unless limited by a set of desired attributes specified by the caller. When used as input to specify desired attributes to return, omitting a given element indicates that it shall not be returned in the output. In contrast, by providing an element (even with no value) the caller ensures that a value for that element will be returned, given that the value can be retrieved. When used as input to specify queries, any element can be omitted in which case the resulting set of objects is not constrained by any specific value of that attribute.

> Name | Range | Type | Description
> body-file |  | string optional | The AutoSupport Content Filename for this Data Attributes: non-creatable, non-modifiable
> cmd |  | string optional | Actual Data Being Collected Attributes: non-creatable, non-modifiable
> cmd-tgt |  | autosupport-cmd-tgt optional | Execution Domain for Command Attributes: non-creatable, non-modifiable Possible values: "bsd" - Command executed by BSD, "smf_table" - Command selects SMF table, "file" - Command indicates file to collect, "dblade" - Collect from dbladecli, "dblade_file" - Collect a file from dblade. Could be partner file, "zapi_xml" - Response in XML format, "custom_fx" - Collect custom function output file
> content-type |  | asup-content-type optional | AutoSupport Content Type for this Data Attributes: non-creatable, non-modifiable Possible values: "basic" - ASUP will contain minimal set of data for this subsystem, "troubleshooting" - ASUP will contain detailed collection of data for this subsystem
> error |  | string optional | Textual Description of Error Attributes: non-creatable, non-modifiable
> node-name |  | string optional | Node Attributes: key, non-creatable, non-modifiable
> prio-num | [0..2^32-1] | integer optional | Priority Order of Collection Attributes: key, non-creatable, non-modifiable
> query |  | string optional | Table Query for XML Collection Attributes: non-creatable, non-modifiable
> seq-num | [0..2^64-1] | integer optional | AutoSupport Sequence Number Attributes: key, non-creatable, non-modifiable
> size-collected | [0..2^63-1] | integer optional | Number of Bytes Collected Attributes: non-creatable, non-modifiable
> status |  | asup-manifest-status optional | Status of this Data Item Attributes: non-creatable, non-modifiable Possible values: "requested" - ASUP request has been added to the queue and is waiting processing by the collector, "working" - ASUP Collector is actively gathering the needed data, "file_not_found" - ASUP collection failed, a needed file is missing, "no_such_table" - ASUP collection was unable to find the requested SMF table, "collection_truncated_size_limit" - ASUP collection truncated due to size limits and partial data is available, "collection_skipped_size_limit" - ASUP collection skipped due to size limits and no data is available, "collection_truncated_time_limit" - ASUP collection truncated due to time limits and partial data is available, "collection_skipped_time_limit" - ASUP collection skipped due to time limits and no data is available, "delivery_skipped_size_limit" - ASUP data was skipped at delivery time due to size limits, "general_error" - ASUP collection failed, additional information if any will be in the Error String field, "completed" - ASUP collection is complete, ready for delivery, "content_not_collected_mode" - ASUP content was not collected, incompatible operational mode, "content_not_collected_precheck" - ASUP content was not collected, pre-check function violation, "content_not_collected_privacy" - ASUP content was not collected, the operation is disabled in privacy mode, "content_empty" - ASUP content was collected successfully, but output was empty, "collection_aborted" - ASUP collection aborted
> subsystem |  | asup-subsystems optional | Subsystem Attributes: non-creatable, non-modifiable Possible values: "platform" - Hardware information about the node, "mhost" - User Space application information for a node, "log_files" - Log files for a node, "performance" - This subsystem gathers the .cm_stats_hourly_done file and user space counters, "performance_asup" - Performance specific information for a node, "nht" - This subsystem gathers the /mroot/etc/log/nht_info content, "san" - SAN specific information for a node, "snapvault" - SNAPVAULT specific information for a node, "snapmirror" - Snapmirror specific information for a node, "dedupe" - Dedupe specific information for a node, "nfs" - NFS specific information for a node, "wafl" - WAFL specific information for a node, "mot" - MOT specific information for a node, "ha" - HA specific information for a node, "networking" - Networking specific information for a node, "cifs" - CIFS specific information for a node, "fpolicy" - Fpolicy specific information for a node, "multistore" - Multistore specific information for a node, "raid" - RAID specific information for a node, "storage" - Storage specific information for a node, "asup_ems" - ASUP EMS specific information for a node, "tape" - Tape specific information for a node, "kernel" - kernel specific information for a node, "secd" - SECD specific information for a node, "metrocluster" - Metrocluster specific information for a node, "mandatory" - Mandatory Basic information for a node
> time-collected | [0..2^64-1] | integer optional | Collection Time for this Data Item (ms) Attributes: non-creatable, non-modifiable

Element definition: autosupport-trigger-info | [top]

> AutoSupport trigger data When returned as part of the output, all elements of this typedef are reported, unless limited by a set of desired attributes specified by the caller. When used as input to specify desired attributes to return, omitting a given element indicates that it shall not be returned in the output. In contrast, by providing an element (even with no value) the caller ensures that a value for that element will be returned, given that the value can be retrieved. When used as input to specify queries, any element can be omitted in which case the resulting set of objects is not constrained by any specific value of that attribute.

> Name | Range | Type | Description
> additional-content |  | asup-content-type[] optional | Additional Content Flag Attributes: non-creatable, non-modifiable Possible values: "basic" - ASUP will contain minimal set of data for this subsystem, "troubleshooting" - ASUP will contain detailed collection of data for this subsystem
> basic-additional |  | asup-subsystems[] optional | Additional Subsystems Reporting Basic Info Attributes: non-creatable, modifiable Possible values: "platform" - Hardware information about the node, "mhost" - User Space application information for a node, "log_files" - Log files for a node, "performance" - This subsystem gathers the .cm_stats_hourly_done file and user space counters, "performance_asup" - Performance specific information for a node, "nht" - This subsystem gathers the /mroot/etc/log/nht_info content, "san" - SAN specific information for a node, "snapvault" - SNAPVAULT specific information for a node, "snapmirror" - Snapmirror specific information for a node, "dedupe" - Dedupe specific information for a node, "nfs" - NFS specific information for a node, "wafl" - WAFL specific information for a node, "mot" - MOT specific information for a node, "ha" - HA specific information for a node, "networking" - Networking specific information for a node, "cifs" - CIFS specific information for a node, "fpolicy" - Fpolicy specific information for a node, "multistore" - Multistore specific information for a node, "raid" - RAID specific information for a node, "storage" - Storage specific information for a node, "asup_ems" - ASUP EMS specific information for a node, "tape" - Tape specific information for a node, "kernel" - kernel specific information for a node, "secd" - SECD specific information for a node, "metrocluster" - Metrocluster specific information for a node, "mandatory" - Mandatory Basic information for a node
> basic-default |  | asup-subsystems[] optional | Default Subsystems Reporting Basic Info Attributes: non-creatable, non-modifiable Possible values: "platform" - Hardware information about the node, "mhost" - User Space application information for a node, "log_files" - Log files for a node, "performance" - This subsystem gathers the .cm_stats_hourly_done file and user space counters, "performance_asup" - Performance specific information for a node, "nht" - This subsystem gathers the /mroot/etc/log/nht_info content, "san" - SAN specific information for a node, "snapvault" - SNAPVAULT specific information for a node, "snapmirror" - Snapmirror specific information for a node, "dedupe" - Dedupe specific information for a node, "nfs" - NFS specific information for a node, "wafl" - WAFL specific information for a node, "mot" - MOT specific information for a node, "ha" - HA specific information for a node, "networking" - Networking specific information for a node, "cifs" - CIFS specific information for a node, "fpolicy" - Fpolicy specific information for a node, "multistore" - Multistore specific information for a node, "raid" - RAID specific information for a node, "storage" - Storage specific information for a node, "asup_ems" - ASUP EMS specific information for a node, "tape" - Tape specific information for a node, "kernel" - kernel specific information for a node, "secd" - SECD specific information for a node, "metrocluster" - Metrocluster specific information for a node, "mandatory" - Mandatory Basic information for a node
> node-name |  | string optional | Node Attributes: key, non-creatable, non-modifiable
> noteto-enabled |  | boolean optional | Deliver to AutoSupport -noteto Addresses Attributes: non-creatable, modifiable
> time-limit | [0..2^32-1] | integer optional | The data collection time budget for this trigger (in seconds). Content not collected will be marked as collection-truncated-time-limit in the manifest. Attributes: non-creatable, modifiable
> to-enabled |  | boolean optional | Deliver to AutoSupport -to Addresses Attributes: non-creatable, modifiable
> trigger |  | string optional | EMS Message Attributes: key, non-creatable, non-modifiable
> troubleshooting-additional |  | asup-subsystems[] optional | Additional Subsystems Reporting Troubleshooting Info Attributes: non-creatable, modifiable Possible values: "platform" - Hardware information about the node, "mhost" - User Space application information for a node, "log_files" - Log files for a node, "performance" - This subsystem gathers the .cm_stats_hourly_done file and user space counters, "performance_asup" - Performance specific information for a node, "nht" - This subsystem gathers the /mroot/etc/log/nht_info content, "san" - SAN specific information for a node, "snapvault" - SNAPVAULT specific information for a node, "snapmirror" - Snapmirror specific information for a node, "dedupe" - Dedupe specific information for a node, "nfs" - NFS specific information for a node, "wafl" - WAFL specific information for a node, "mot" - MOT specific information for a node, "ha" - HA specific information for a node, "networking" - Networking specific information for a node, "cifs" - CIFS specific information for a node, "fpolicy" - Fpolicy specific information for a node, "multistore" - Multistore specific information for a node, "raid" - RAID specific information for a node, "storage" - Storage specific information for a node, "asup_ems" - ASUP EMS specific information for a node, "tape" - Tape specific information for a node, "kernel" - kernel specific information for a node, "secd" - SECD specific information for a node, "metrocluster" - Metrocluster specific information for a node, "mandatory" - Mandatory Basic information for a node
> troubleshooting-default |  | asup-subsystems[] optional | Default Subsystems Reporting Troubleshooting Info Attributes: non-creatable, non-modifiable Possible values: "platform" - Hardware information about the node, "mhost" - User Space application information for a node, "log_files" - Log files for a node, "performance" - This subsystem gathers the .cm_stats_hourly_done file and user space counters, "performance_asup" - Performance specific information for a node, "nht" - This subsystem gathers the /mroot/etc/log/nht_info content, "san" - SAN specific information for a node, "snapvault" - SNAPVAULT specific information for a node, "snapmirror" - Snapmirror specific information for a node, "dedupe" - Dedupe specific information for a node, "nfs" - NFS specific information for a node, "wafl" - WAFL specific information for a node, "mot" - MOT specific information for a node, "ha" - HA specific information for a node, "networking" - Networking specific information for a node, "cifs" - CIFS specific information for a node, "fpolicy" - Fpolicy specific information for a node, "multistore" - Multistore specific information for a node, "raid" - RAID specific information for a node, "storage" - Storage specific information for a node, "asup_ems" - ASUP EMS specific information for a node, "tape" - Tape specific information for a node, "kernel" - kernel specific information for a node, "secd" - SECD specific information for a node, "metrocluster" - Metrocluster specific information for a node, "mandatory" - Mandatory Basic information for a node

Element definition: compression-format | [top]

> 7z|tgz Possible values: "7z" - 7-Zip Archive, "tgz" - Zipped Tarball

> [none]

Element definition: mail-address | [top]

> E-mail Address

> [none]

Element definition: asup-content-type | [top]

> Type of AutoSupport content Possible values: "basic" - ASUP will contain minimal set of data for this subsystem, "troubleshooting" - ASUP will contain detailed collection of data for this subsystem

> [none]

Element definition: asup-destination | [top]

> smtp|http|noteto|retransmit Possible values: "smtp" , "http" , "noteto" , "retransmit"

> [none]

Element definition: asup-manifest-status | [top]

> AutoSupport manifest collection status Possible values: "requested" - ASUP request has been added to the queue and is waiting processing by the collector, "working" - ASUP Collector is actively gathering the needed data, "file_not_found" - ASUP collection failed, a needed file is missing, "no_such_table" - ASUP collection was unable to find the requested SMF table, "collection_truncated_size_limit" - ASUP collection truncated due to size limits and partial data is available, "collection_skipped_size_limit" - ASUP collection skipped due to size limits and no data is available, "collection_truncated_time_limit" - ASUP collection truncated due to time limits and partial data is available, "collection_skipped_time_limit" - ASUP collection skipped due to time limits and no data is available, "delivery_skipped_size_limit" - ASUP data was skipped at delivery time due to size limits, "general_error" - ASUP collection failed, additional information if any will be in the Error String field, "completed" - ASUP collection is complete, ready for delivery, "content_not_collected_mode" - ASUP content was not collected, incompatible operational mode, "content_not_collected_precheck" - ASUP content was not collected, pre-check function violation, "content_not_collected_privacy" - ASUP content was not collected, the operation is disabled in privacy mode, "content_empty" - ASUP content was collected successfully, but output was empty, "collection_aborted" - ASUP collection aborted

> [none]

Element definition: asup-status | [top]

> AutoSupport general status Possible values: "initializing" - ASUP request is being processed, "collection_failed" - The AutoSupport Collection failed. See 'Last Error' for more information, "collection_in_progress" - The AutoSupport Collection is in progress, "queued" - ASUP is queued for delivery, "transmitting" - ASUP transmission is in progress, "sent_successful" - ASUP was successfully sent, "ignore" - ASUP was processed successfully but has no destinations configured, "re_queued" - ASUP transmission failed and has been re-queued, "transmission_failed" - ASUP transmission has failed and the retry limit has been exceeded

> [none]

Element definition: asup-subsystems | [top]

> AutoSupport collection subsystems Possible values: "platform" - Hardware information about the node, "mhost" - User Space application information for a node, "log_files" - Log files for a node, "performance" - This subsystem gathers the .cm_stats_hourly_done file and user space counters, "performance_asup" - Performance specific information for a node, "nht" - This subsystem gathers the /mroot/etc/log/nht_info content, "san" - SAN specific information for a node, "snapvault" - SNAPVAULT specific information for a node, "snapmirror" - Snapmirror specific information for a node, "dedupe" - Dedupe specific information for a node, "nfs" - NFS specific information for a node, "wafl" - WAFL specific information for a node, "mot" - MOT specific information for a node, "ha" - HA specific information for a node, "networking" - Networking specific information for a node, "cifs" - CIFS specific information for a node, "fpolicy" - Fpolicy specific information for a node, "multistore" - Multistore specific information for a node, "raid" - RAID specific information for a node, "storage" - Storage specific information for a node, "asup_ems" - ASUP EMS specific information for a node, "tape" - Tape specific information for a node, "kernel" - kernel specific information for a node, "secd" - SECD specific information for a node, "metrocluster" - Metrocluster specific information for a node, "mandatory" - Mandatory Basic information for a node

> [none]

Element definition: asup-transport | [top]

> smtp|http|https Possible values: "smtp" , "http" , "https"

> [none]

Element definition: autosupport-cmd-tgt | [top]

> Execution domain of AutoSupport content Possible values: "bsd" - Command executed by BSD, "smf_table" - Command selects SMF table, "file" - Command indicates file to collect, "dblade" - Collect from dbladecli, "dblade_file" - Collect a file from dblade. Could be partner file, "zapi_xml" - Response in XML format, "custom_fx" - Collect custom function output file

> [none]