APIs in Category: ems | API version 1.3

ems-autosupport-log

NetApp Manage ONTAP

ems-autosupport-log | [top]

> EMS send autosupport message and do system log.

> Input Name | Range | Type | Description
> app-version |  | string | Version of application invoking autosupport log.
> auto-support |  | boolean | If 'true' trigger AutoSupport message. Defaults to 'false'.
> category |  | string | Category of event.
> computer-name |  | string | Host invoking autosupport log.
> event-description |  | string | Description of event (message to log).
> event-id |  | integer | ID of event. Range [0..2^32-1].
> event-source |  | string | Name of the application invoking autosupport log.
> log-level |  | integer | Log level. Accepted values are 0 for 'emergency', 1 for 'alert', 2 for 'critical', 3 for 'error', 4 for 'warning', 5 for 'notice', 6 for 'info', and 7 for 'debug'.

> Errno | Description
> ENOENT |  |