APIs in Category: system | API version 1.4

system-get-info system-get-ontapi-version system-get-version

NetApp Manage ONTAP

system-get-info | [top]

> Obtain appliance information which in includes cpu, and backplane information. The output contains the head information in a sysconfig -a command. I/O information is not included.

> Output Name | Range | Type | Description
> system-info |  | system-info |

system-get-ontapi-version | [top]

> Obtain the current ONTAPI major and minor versions.

> Output Name | Range | Type | Description
> major-version |  | integer | Current ONTAPI major version supported by this appliance.
> minor-version |  | integer | Current ONTAPI minor version supported by this appliance.

system-get-version | [top]

> Obtain the ONTAP version.

> Output Name | Range | Type | Description
> version |  | string | Current ONTAP version running on the appliance.

> Vfiler-enabled
> Yes

Element definition: system-info | [top]

> Information about the system

> Name | Range | Type | Description
> backplane-part-number |  | string optional | Part number of the backplane.
> backplane-revision |  | string optional | Revision of the backplane part number.
> backplane-serial-number |  | string optional | Backplane serial number.
> board-speed |  | integer | Speed of the system board in mega Hertz.
> board-type |  | string | Type of the system board. This is defined by Network Appliance. An example is: NetApp System Board VII D0.
> cpu-ciob-revision-id |  | string optional | Processor's CIOB (Champion I/O Bus) revision ID. Defined by the CPU manufacturer.
> cpu-firmware-release |  | string optional | Firmware release number. Defined by the CPU manufacturer.
> cpu-microcode-version |  | string optional | cpu's microcode version. Defined by the CPU manufacturer.
> cpu-part-number |  | string optional | CPU's part number. Defined by the CPU manufacturer.
> cpu-processor-id |  | string optional | Processor's ID. Defined by the CPU manufacturer.
> cpu-processor-type |  | string optional | Processor's Type. Defined by the CPU manufacturer.
> cpu-revision |  | string optional | CPU's part number revision. Defined by the CPU manufacturer.
> cpu-serial-number |  | string optional | CPU's serial number. Defined by the CPU manufacturer.
> memory-size |  | integer | Memory size in megabytes. (1024*1024).
> number-of-processors |  | integer | Number of processors in the appliance.
> partner-system-id |  | string optional | Partner's system ID. Displayed in a cluster environment. A string of 10 characters.
> partner-system-name |  | string optional | Partner's system name. Displayed in a cluster environment. Defined in the partner's setup.
> partner-system-serial-number |  | string optional | Partner System serial number. This is defined by Network Appliance. Currently a string of numbers.
> system-id |  | string | System ID. This is defined by Network Appliance. Currently, it is a string of numbers
> system-model |  | string | Model name of the system, like F880.
> system-name |  | string | System name. This is the name defined during setup.
> system-revision |  | string optional | System revision. There revision id of the system board. Currently, a character followed by a number, B0.
> system-serial-number |  | string optional | System serial number. This is defined by Network Appliance. Currently a string of numbers.