# IPMI Enable PEF Subcommands

access: Managers

Allows you to enable platform event filtering.

> ipmi enable pef

Return Codes

Following are the return values for this command:

Code | Numeric Code | Description
--- | --- | ---
NWSE_Success | 0 | Command successfully completed.
NWSE_InvalidUsage | 1 | Invalid usage: bad parameter usage, conflicting options specified.
NWSE_NoPermission | 6 | Not authorized to perform this operation.
NWSE_ServiceNotAvailable | 24 | Requested service is not available; could not contact the IPMI server process.

Related Topics

System Management Commands

IPMI Command