# SP Get IP Subcommand

access: All users

Retrieves the ethernet-based network configuration information for the Service Processor, including IP address, network mask, and gateway. In addition, it indicates whether the Service Processor is configured to use DHCP or a static IP address.

> sp get ip [-H | noheader][{-D | --delim <DELIMITER>}]

Argument | Description
--- | ---
{ -H | --noheader } | Suppresses column headings.
{ -D | --delim } | Delimits columns with the specified delimiter. Headings are also delimited unless suppressed. The delimiter can be any character or string.

Return Codes

Following are the return values for this command:

Code | Numeric Code | Description
--- | --- | ---
NWSE_Success | 0 | Command successfully completed.
NWSE_InvalidUsage | 1 | Invalid usage: bad parameter usage, conflicting options specified.
NWSE_NoMemory | 8 | Insufficient memory.
NWSE_Busy | 9 | Device or resource is busy.
NWSE_RPCConnected | 11 | RPC client already connected.
NWSE_RPCConnRefused | 12 | RPC connection refused.
NWSE_NoRouteToHost | 13 | No route to host (network down).
NWSE_HostDown | 14 | Host is down.

Related Topics

System Management Commands

SP Command