# SP Command

The sp command gets or sets Service Processor configuration values, generates or manages events and notices; or adds or modifies subscribers, event routes, and email notification groups for the Service Processor event manager.

The sp subcommands fall into the following categories:

Subcommand Group | Description
--- | ---
Date | Sets or retrieves the date and time on the Service Processor RTC.
DNS | Displays or configures the DNS client configuration on the Service Processor.
Events | Returns detailed information or clears an event.
Hostname | Displays or resets the hostname and/or domain name of the Service Processor.
IP | Sets, modifies, or retrieves the Service Processor network configuration.
JNET Address | Sets or retrieves the jnet address.
Locate Light | Sets the state or reads the value of the locatelight switch.
Logfile | Retrieves or configures the event log file.
MAC | Retrieves the MAC address for the Service Processor.
Miscellaneous | Reads status for a component, retrieves the last port 80 postcode, restores settings to defaults, stores data in tar zipped format, or captures debug data.
Mount | Displays, creates, resets, or deletes a mountpoint.
SMTP | Manages information about SMTP email delivery.
SNMP | Manages SNMP functions.
SSL | Manages SSL capabilities.
Update Flash | Sets the update flag to start the full flash update or copies the Value-Add file to the Value-Add component of the Service Processor flash.

Notes

- Every command returns a return code upon completion.

Related Topics

System Management Commands

Glossary