# IPMI Set Global Enable Subcommand

access: Administrators, Managers

Allows you to set the value of several IPMI global enable variables.

> ipmi set global enable {-n |--name} GLOBAL_NAME {{-e|--enabled) | {-d|--disabled}}

Argument | Description
--- | ---
{-n |--name} | The name of one of the IPMI global enable variables (see table below). You can either use a quoted long string or alias without quotes for the list of global enables.
{-e|--enabled} | Turns the channel on.
{-d|--disabled} | Turns the channel off.

Alias | Name String | Values | Default
--- | --- | --- | ---
oem0 | OEM0 Enable | Enabled/Disabled | Disabled
oem1 | OEM1 Enable | Enabled/Disabled | Disabled
oem2 | OEM 2 Enable | Enabled/Disabled |
logging | Enable System Event Logging | Enabled/Disabled | Enabled
msg_buf | Enable Event Message Buffer | Enabled/Disabled | TBD
msg_buf_interrupt | Enable the Event Message Buffer Full | Enabled/Disabled | TBD
msg_queue_interrupt | Enable Receive Message Queue Interrupt | Enabled/Disabled | Enabled

Return Codes

Following are the return values for this command:

Code | Numeric Code | Description
--- | --- | ---
NWSE_Success | 0 | Command successfully completed.
NWSE_InvalidUsage | 1 | Invalid usage: bad parameter usage, conflicting options specified.
NWSE_InvalidArgument | 4 | Invalid arguments: incorrect or missing. The format of the date string was invalid.
NWSE_NoPermission | 6 | Not authorized to perform this operation.

Related Topics

System Management Commands

IPMI Command