! CHARSETS.TXT - Character set definitions.

! This file is extracted from an udated version of RFC1345, "Character
! Mnemonics & Character Sets", by Keld Simonsen.

! Corrections are marked with ! ***

! &referenceset
! !"  %&'()*+,-./0123456789:;<=>?
! ABCDEFGHIJKLMNOPQRSTUVWXYZ    _
! abcdefghijklmnopqrstuvwxyz

 &charset ISO_646.basic
 &rem source: ECMA registry
 &alias ref
 &alias ISO_646.basic:1983
 &bits 7
 &code 32
 SP ! " ?? ?? % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 ?? A B C D E F G H I J K L M N O P Q R S T U V W X Y Z ?? ?? ?? ?? _
 ?? a b c d e f g h i j k l m n o p q r s t u v w x y z

 &charset ISO_646.irv
 &rem source: ECMA registry
 &alias iso-ir-2
 &alias ISO_646.irv:1983
 &alias irv
 &alias T.50-IRV
 &g0esc x2840 &g1esc x2940 &g2esc x2a40 &g3esc x2b40
 &bits 7
 &IRnum 2
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb Cu % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '- DT

 &charset INVARIANT
 &bits 7
 &alias iso-ir-170
 &g0esc x2840 &g1esc x2940 &g2esc x2a40 &g3esc x2b40
 &IRnum 170
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " ?? ?? % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 ?? A B C D E F G H I J K L M N O P Q R S T U V W X Y Z ?? ?? ?? ?? _
 ?? a b c d e f g h i j k l m n o p q r s t u v w x y z ?? ?? ?? ?? DT

 &charset BS_4730
 &rem source: ECMA registry
 &alias iso-ir-4
 &alias ISO646-GB
 &bits 7
 &g0esc x2841 &g1esc x2941 &g2esc x2a41 &g3esc x2b41
 &alias gb
 &alias uk
 &IRnum 4
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Pd DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '- DT

 &charset US-ASCII
 &rem source: ECMA registry
 &alias iso-ir-6
 &alias ANSI_X3.4-1986
 &alias ISO_646.irv:1991
 &g0esc x2842 &g1esc x2942 &g2esc x2a42 &g3esc x2b42
 &alias ASCII
 &alias ISO646-US
 &alias ANSI_X3.4-1968
 &alias us
 &alias IBM367
 &alias CP367
 &alias T.50
 &alias IA5
 &bits 7
 &IRnum 6
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT

 &charset NATS-SEFI
 &rem source: ECMA registry
 &alias iso-ir-8-1
 &g0esc x2843 &g1esc x2943 &g2esc x2a43 &g3esc x2b43
 &bits 7
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 UA A B C D E F G H I J K L M N O P Q R S T U V W X Y Z A: O: AA fS _
 UB a b c d e f g h i j k l m n o p q r s t u v w x y z a: o: aa -N DT

 &charset NATS-SEFI-ADD
 &rem source: ECMA registry
 &alias iso-ir-8-2
 &g0esc x2844 &g1esc x2944 &g2esc x2a44 &g3esc x2b44
 &bits 7
 &code 0
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? A! ?? ?? D/ E' ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 TH ?? ?? ?? ?? U: ?? ?? ?? ?? ?? AE O/ ?? ?? ??
 ?? a! ?? ?? d/ e' ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 th ?? ?? ?? ?? u: ?? ?? ?? ?? ?? ae o/ ?? ?? ??

 &charset NATS-DANO
 &rem source: ECMA registry
 &alias iso-ir-9-1
 &g0esc x2845 &g1esc x2945 &g2esc x2a45 &g3esc x2b45
 &bits 7
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! << >> DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 UA A B C D E F G H I J K L M N O P Q R S T U V W X Y Z AE O/ AA fS _
 UB a b c d e f g h i j k l m n o p q r s t u v w x y z ae o/ aa -N DT

 &charset NATS-DANO-ADD
 &rem source: ECMA registry
 &alias iso-ir-9-2
 &g0esc x2846 &g1esc x2946 &g2esc x2a46 &g3esc x2b46
 &bits 7
 &code 0
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? A! ?? ?? D/ E' ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 TH ?? ?? ?? ?? U: ?? ?? ?? ?? ?? A: O: ?? ?? ??
 ?? a! ?? ?? d/ e' ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 th ?? ?? ?? ?? u: ?? ?? ?? ?? ?? a: o: ?? ?? ??

 &charset SEN_850200_B
 &rem source: ECMA registry
 &alias iso-ir-10
 &alias FI
 &alias ISO646-FI
 &alias ISO646-SE
 &alias se
 &alias SS636127
 &g0esc x2847 &g1esc x2947 &g2esc x2a47 &g3esc x2b47
 &bits 7
 &IRnum 10
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb Cu % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z A: O: AA '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z a: o: aa '- DT

 &charset SEN_850200_C
 &rem source: ECMA registry
 &alias iso-ir-11
 &alias ISO646-SE2
 &g0esc x2848 &g1esc x2948 &g2esc x2a48 &g3esc x2b48
 &alias se2
 &bits 7
 &IRnum 11
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb Cu % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 E' A B C D E F G H I J K L M N O P Q R S T U V W X Y Z A: O: AA U: _
 e' a b c d e f g h i j k l m n o p q r s t u v w x y z a: o: aa u: DT

 &charset JIS_C6220-1969-jp
 &rem source: ECMA registry
 &alias JIS_C6220-1969
 &alias iso-ir-13
 &alias katakana
 &alias x0201-7
 &g0esc x2849 &g1esc x2949 &g2esc x2a49 &g3esc x2b49
 &bits 7
 &IRnum 13
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ._ <' >' ,_ .6 Wo a6 i6 u6 e6 o6 YA YU YO TU
 -6 A6 I6 U6 E6 O6 Ka Ki Ku Ke Ko Sa Si Su Se So
 Ta Ti Tu Te To Na Ni Nu Ne No Ha Hi Hu He Ho Ma
 Mi Mu Me Mo Ya Yu Yo Ra Ri Ru Re Ro Wa N6 "5 05
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? DT

 &charset JIS_C6220-1969-ro
 &rem source: ECMA registry
 &alias iso-ir-14
 &g0esc x284a &g1esc x294a &g2esc x2a4a &g3esc x2b4a
 &alias jp
 &alias ISO646-JP
 &bits 7
 &IRnum 14
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( Ye )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '- DT

 &charset IT
 &rem source: ECMA registry
 &alias iso-ir-15
 &alias ISO646-IT
 &g0esc x2859 &g1esc x2959 &g2esc x2a59 &g3esc x2b59
 &bits 7
 &IRnum 15
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Pd DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 SE A B C D E F G H I J K L M N O P Q R S T U V W X Y Z DG c, e' '> _
 u! a b c d e f g h i j k l m n o p q r s t u v w x y z a! o! e! i! DT

 &charset PT
 &rem source: ECMA registry
 &alias iso-ir-16
 &alias ISO646-PT
 &g0esc x284c &g1esc x294c &g2esc x2a4c &g3esc x2b4c
 &bits 7
 &IRnum 16
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 SE A B C D E F G H I J K L M N O P Q R S T U V W X Y Z A? C, O? '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z a? c, o? DG DT

 &charset ES
 &rem source: ECMA registry
 &alias iso-ir-17
 &alias ISO646-ES
 &g0esc x285a &g1esc x295a &g2esc x2a5a &g3esc x2b5a
 &bits 7
 &IRnum 17
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Pd DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 SE A B C D E F G H I J K L M N O P Q R S T U V W X Y Z !I N? ?I '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z DG n? c, '? DT

 &charset greek7-old
 &rem source: ECMA registry
 &alias iso-ir-18
 &g0esc x285b &g1esc x295b &g2esc x2a5b &g3esc x2b5b
 &bits 7
 &IRnum 18
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Pd DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 '' a* b* q* d* e* f* g* y* i* c* k* l* m* n* o*
 p* j3 r* s* t* h* w* *s x* u* z* ?, ,, ,' '? _
 '! A* B* Q* D* E* F* G* Y* I* C* K* L* M* N* O*
 P* ?? R* S* T* H* W* .M X* U* Z* ?; ;; ;' ': DT

 &charset latin-greek
 &rem source: ECMA registry
 &alias iso-ir-19
 &g0esc x285c &g1esc x295c &g2esc x2a5c &g3esc x2b5c
 &bits 7
 &IRnum 19
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Pd DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A  B  C  D  E  F  G  H  I  J  K  L  M  N  O
 P  Q  R  S  T  U  V  W  X  Y  Z  <( // )> '> _
 '! A* B* Q* D* E* F* G* Y* I* C* K* L* M* N* O*
 P* ?? R* S* T* H* W* .M X* U* Z* (! !! !) ': DT

 &charset DIN_66003
 &rem source: ECMA registry
 &alias iso-ir-21
 &g0esc x284b &g1esc x294b &g2esc x2a4b &g3esc x2b4b
 &alias de
 &alias ISO646-DE
 &bits 7
 &IRnum 21
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 SE A B C D E F G H I J K L M N O P Q R S T U V W X Y Z A: O: U: '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z a: o: u: ss DT

 &charset NF_Z_62-010_1973
 &rem source: ECMA registry
 &alias iso-ir-25
 &alias ISO646-FR1
 &g0esc x2852 &g1esc x2952 &g2esc x2a52 &g3esc x2b52
 &bits 7
 &IRnum 25
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Pd DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 a! A B C D E F G H I J K L M N O P Q R S T U V W X Y Z DG c, SE '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z e' u! e! ': DT

 &charset Latin-greek-1
 &rem source: ECMA registry
 &alias iso-ir-27
 &g0esc x2855 &g1esc x2955 &g2esc x2a55 &g3esc x2b55
 &bits 7
 &IRnum 27
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP C* " G* Cu % & ' ( ) * + , - . /
 0 1 2 3 4 5 6 7 8 9 Q* ; < = > P*
 D* A B C D E F G H I J K L M N O
 P Q R S T U V W X Y Z W* H* F* L* S*
 '! a b c d e f g h i j k l m n o
 p q r s t u v w x y z (! !! !) '- DT

 &charset ISO_5427
 &rem source: ECMA registry
 &alias iso-ir-37
 &alias KOI-7
 &g0esc x284e &g1esc x294e &g2esc x2a4e &g3esc x2b4e
 &bits 7
 &IRnum 37
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb Cu % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 ju a= b= c= d= e= f= g= h= i= j= k= l= m= n= o=
 p= ja r= s= t= u= z% v= %' y= z= s% je sc c% ='
 JU A= B= C= D= E= F= G= H= I= J= K= L= M= N= O=
 P= JA R= S= T= U= Z% V= %" Y= Z= S% JE Sc C% DT

 &charset JIS_C6226-1978
 &rem source: ECMA registry
 &alias iso-ir-42
 &bits 14
! *** Add missing 28 to g0esc
 &g0esc x242840 &g1esc x242940 &g2esc x242a40 &g3esc x242b40
 &IRnum 42
 &code2 1 1
 SP ,_ ._ , . .6 : ; ! "5 05 '' '! ': '> '- _ *6 +6 *5 +5 +"
 +_ *_ ;_ 0_ -6 -? -N
 &code2 1 31
 FD BD ?1 PP !! .3 .. '6 '9 "6 "9 ( ) (' )' <( )>
 (! !) <1 >1 </ /> <' >' <" >" (" )" + - +- *X -: = != < > =< >= 00
 .: Ml Fm DG 1' 2' oC Ye DO Ct Pd % Nb & * At SE *1 *2 0m 0M 0o LZ
 &code2 2 1
 Db OS fS uT UT dT DT :X =T -> <- -! -v =_
 &code2 3 16
 0 1 2 3 4 5 6 7 8 9
 &code2 3 33
 A B C D E F G H I J K L M N O P Q R S T U V W X Y Z
 &code2 3 65
 a b c d e f g h i j k l m n o p q r s t u v w x y z
 &code2 4 1
    A5 a5 I5 i5 U5 u5 E5 e5 O5 o5 ka ga ki gi ku
 gu ke ge ko go sa za si zi su zu se ze so zo ta
 da ti di tU tu du te de to do na ni nu ne no ha
 ba pa hi bi pi hu bu pu he be pe ho bo po ma mi
 mu me mo yA ya yU yu yO yo ra ri ru re ro wA wa
 wi we wo n5
 &code2 5 1
    a6 A6 i6 I6 u6 U6 e6 E6 o6 O6 Ka Ga Ki Gi Ku
 Gu Ke Ge Ko Go Sa Za Si Zi Su Zu Se Ze So Zo Ta
 Da Ti Di TU Tu Du Te De To Do Na Ni Nu Ne No Ha
 Ba Pa Hi Bi Pi Hu Bu Pu He Be Pe Ho Bo Po Ma Mi
 Mu Me Mo YA Ya YU Yu YO Yo Ra Ri Ru Re Ro WA Wa
 Wi We Wo N6 Vi KA KE
 &code2 6 1
 A* B* G* D* E* Z* Y* H* I* K* L* M* N* C* O*
 P* R* S* T* U* F* X* Q* W*
 &code2 6 33
 a* b* g* d* e* z* y* h* i* k* l* m* n* c* o*
 p* r* s* t* u* f* x* q* w*
 &code2 7 1
 A= B= V= G= D= E= IO Z% Z= I= J= K= L= M= N= O= P=
 R= S= T= U= F= H= C= C% S% Sc =" Y= %" JE JU JA
 &code2 7 49
 a= b= v= g= d= e= io z% z= i= j= k= l= m= n= o= p=
 r= s= t= u= f= h= c= c% s% sc =' y= %' je ju ja
 &codex j 16 46 1 94
 &codex j 47 47 1 51
 &codex j 48 83 1 94

 &charset BS_viewdata
 &rem source: ECMA registry
 &alias iso-ir-47
 &g0esc x2856 &g1esc x2956 &g2esc x2a56 &g3esc x2b56
 &bits 7
 &IRnum 47
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Pd DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <- 12 -> -! OS
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z 14 PP 34 -: DT

 &charset INIS
 &rem source: ECMA registry
 &alias iso-ir-49
 &g0esc x2857 &g1esc x2957 &g2esc x2a57 &g3esc x2b57
 &bits 7
 &IRnum 49
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ?? ?? ?? DO % ?? ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ??
 ?? A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( ?? )> ?? ??
 ?? a b c d e f g h i j k l m n o p q r s t u v w x y z ?? !! ?? ?? DT

 &charset INIS-8
 &rem source: ECMA registry
 &alias iso-ir-50
 &g0esc x285d &g1esc x295d &g2esc x2a5d &g3esc x2b5d
 &bits 7
 &IRnum 50
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? a* b* g* d* C* ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? -> In
 0S 1S 2S 3S 4S 5S 6S 7S 8S 9S +S -S Ru D* L* W*
 0s 1s 2s 3s 4s 5s 6s 7s 8s 9s S* m* n* w* p* DT

 &charset INIS-cyrillic
 &rem source: ECMA registry
 &alias iso-ir-51
 &g0esc x285e &g1esc x295e &g2esc x2a5e &g3esc x2b5e
 &bits 7
 &IRnum 51
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? RT ?? -> In
 a* b* g* d* S* m* n* w* p* C* D* L* W* =" -S +S
 ju a= b= c= d= e= f= g= h= i= j= k= l= m= n= o=
 p= ja r= s= t= u= z% v= %' y= z= s% je sc c% ='
 JU A= B= C= D= E= F= G= H= I= J= K= L= M= N= O=
 P= JA R= S= T= U= Z% V= %" Y= Z= S% JE Sc C% DT

 &charset ISO_5427-ext
 &rem source: ECMA registry
 &alias iso-ir-54
 &alias ISO_5427:1981
 &g0esc x2851 &g1esc x2951 &g2esc x2a51 &g3esc x2b51
 &bits 7
 &IRnum 54
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 g3 d% g% ie io ds ii yi j% lj nj ts kj v% dz ??
 y3 f3 v3 o3 ?? ?? ?? ?? ?? ?? ?? <( ?? )> ?? _
 G3 D% G% IE IO DS II YI J% LJ NJ Ts KJ V% DZ ="
 Y3 F3 V3 O3 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? DT

 &charset ISO_5428
 &rem source: ECMA registry
 &alias iso-ir-55
 &alias ISO_5428:1980
 &g0esc x2853 &g1esc x2953 &g2esc x2a53 &g3esc x2b53
 &bits 7
 &IRnum 55
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP "! "' ": "? "p "d "i ?? ?? ?? ?? ?? ?? ?? ??
 << >> "9 "6 'G ,G ?? ?? ?? ?? ?? .M ?? ?? ?? ;
 ?? A* B* ?? G* D* E* T3 M3 Z* Y* H* I* K* L* M*
 N* C* O* P* K3 R* S* ?? T* U* F* X* Q* W* P3 ??
 ?? a* b* b3 g* d* e* t3 m3 z* y* h* i* k* l* m*
 n* c* o* p* k3 r* s* *s t* u* f* x* q* w* p3 DT

 &charset GB_1988-80
 &rem source: ECMA registry
 &alias iso-ir-57
 &g0esc x2854 &g1esc x2954 &g2esc x2a54 &g3esc x2b54
 &alias cn
 &alias ISO646-CN
 &bits 7
 &IRnum 57
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb Ye % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '- DT

 &charset GB_2312-80
 &rem source: ECMA registry
 &alias iso-ir-58
! *** Add missing 28 to g0esc
 &g0esc x242841 &g1esc x242941 &g2esc x242a41 &g3esc x242b41
 &bits 14
 &alias chinese
 &IRnum 58
 &code2 1 1
 SP ,_ .6 .M 'm '< ': +" *_ -6 ?1
 !2 .3 '6 '9 "6 "9 (' )'
 <1 >1 << >> <+ >+ <7 7> (I )I (" )" +- *X -: :R AN OR +Z *P (U )U (-
 :: RT -T PP -L
 (A 0. In Io =3 =? ?2 CG 0( != !< !> =< >= 00 :. .: Ml Fm DG 1' 2' oC DO
 Cu Ct Pd %0 SE NB *1 *2 0m 0M 0o Dw Db OS fS uT UT :X -> <- -! -v =_
 &code2 2 17
 1. 2. 3. 4. 5. 6. 7. 8. 9. 10. 11. 12. 13. 14. 15. 16. 17. 18. 19. 20.
 (1) (2) (3) (4) (5) (6) (7) (8) (9) (10) (11) (12) (13) (14)
 (15) (16) (17) (18) (19) (20) 1-o 2-o 3-o 4-o 5-o 6-o 7-o 8-o 9-o
 &code2 2 69
 1c 2c 3c 4c 5c 6c 7c 8c 9c 10c
 &code2 2 81
 1R 2R 3R 4R 5R 6R 7R 8R 9R aR bR cR
 &code2 3 1
 ! " Nb Ye % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7
 8 9 : ; < = > ? At A B C D E F G H I J K L M N O
 P Q R S T U V W X Y Z <( // )> '> _ '! a b c d e f g
 h i j k l m n o p q r s t u v w x y z (! !! !) '-
 &code2 4 1
    A5 a5 I5 i5 U5 u5 E5 e5 O5 o5 ka ga ki gi ku
 gu ke ge ko go sa za si zi su zu se ze so zo ta
 da ti di tU tu du te de to do na ni nu ne no ha
 ba pa hi bi pi hu bu pu he be pe ho bo po ma mi
 mu me mo yA ya yU yu yO yo ra ri ru re ro wA wa
 wi we wo n5
 &code2 5 1
    a6 A6 i6 I6 u6 U6 e6 E6 o6 O6 Ka Ga Ki Gi Ku
 Gu Ke Ge Ko Go Sa Za Si Zi Su Zu Se Ze So Zo Ta
 Da Ti Di TU Tu Du Te De To Do Na Ni Nu Ne No Ha
 Ba Pa Hi Bi Pi Hu Bu Pu He Be Pe Ho Bo Po Ma Mi
 Mu Me Mo YA Ya YU Yu YO Yo Ra Ri Ru Re Ro WA Wa
 Wi We Wo N6 Vi KA KE
 &code2 6 1
 A* B* G* D* E* Z* Y* H* I* K* L* M* N* C* O*
 P* R* S* T* U* F* X* Q* W*
 &code2 6 33
 a* b* g* d* e* z* y* h* i* k* l* m* n* c* o*
 p* r* s* t* u* f* x* q* w*
 &code2 7 1
 A= B= V= G= D= E= IO Z% Z= I= J= K= L= M= N= O= P=
 R= S= T= U= F= H= C= C% S% Sc =" Y= %" JE JU JA
 &code2 7 49
 a= b= v= g= d= e= io z% z= i= j= k= l= m= n= o= p=
 r= s= t= u= f= h= c= c% s% sc =' y= %' je ju ja
 &code2 8 1
 a- a' a< a! e- e' e< e! i- i' i< i! o- o' o< o! u- u' u< u! u:- u:<
 u:! u: e>
 &code2 8 37
 b4 p4 m4 f4 d4 t4 n4 l4 g4 k4 h4 j4 q4 x4 zh ch sh r4 z4 c4
 s4 a4 o4 e4 eh4 ai ei au ou an en aN eN er i4 u4 iu
 &code2 9 4
 hh HH vv VV 3- 3_ 3! 3/ 4- 4_ 4! 4/ dr dR Dr DR dl dL Dl LD
 ur uR Ur UR ul uL Ul UL vr vR Udr uDr Vr UdR uDR VR
 vl vL Udl uDl Vl UdL uDL VL
 dh dLr dlR dH Dh DLr DlR DH
 vh vLr vlR vH Udh uDh Vh UdLr
 UdlR uDLr uDlR UdH uDH VLr VlR VH
 &codex c 16 54 1 94
 &codex c 55 55 1 89
 &codex c 56 87 1 94

 &charset NS_4551-1
 &rem source: ECMA registry
 &alias iso-ir-60
 &alias ISO646-NO
 &g0esc x2860 &g1esc x2960 &g2esc x2a60 &g3esc x2b60
 &bits 7
 &alias no
 &IRnum 60
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z AE O/ AA '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z ae o/ aa '- DT

 &charset NS_4551-2
 &rem source: ECMA registry
 &alias ISO646-NO2
 &alias iso-ir-61
 &g0esc x2861 &g1esc x2961 &g2esc x2a61 &g3esc x2b61
 &alias no2
 &bits 7
 &IRnum 61
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " SE DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z AE O/ AA '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z ae o/ aa !! DT

 &charset NF_Z_62-010
 &rem source: ECMA registry
 &alias iso-ir-69
 &alias ISO646-FR
 &g0esc x2866 &g1esc x2966 &g2esc x2a66 &g3esc x2b66
 &alias fr
 &bits 7
 &IRnum 69
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Pd DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 a! A B C D E F G H I J K L M N O P Q R S T U V W X Y Z DG c, SE '> _
 My a b c d e f g h i j k l m n o p q r s t u v w x y z e' u! e! ': DT

 &charset videotex-suppl
 &rem source: ECMA registry
 &alias iso-ir-70
 &g0esc x2862 &g1esc x2962 &g2esc x2a62 &g3esc x2b62
 &bits 8
 &IRnum 70
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " ?? ?? % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '- DT
 PA HO BH NH IN NL SA ES HS HJ VS PD PU RI S2 S3
 DC P1 P2 TS CC MW SG EG SS GC SC CI ST OC PM AC
 ?? !I Ct Pd DO Ye Nb SE Cu '6 "6 << <- -! -> -v
 DG +- 2S 3S *X My PI .M -: '9 "9 >> 14 12 34 ?I
 "1 "! "' "> "? "- "( ". ": ?? "0 ", ?? "" "; "<
 -M 1S Rg Co TM M8 ?? ?? ?? ?? ?? ?? 18 38 58 78
 Om AE D- -a H/ ?? IJ L. L/ O/ OE -o TH T/ NG 'n
 kk ae d/ d- h/ i. ij l. l/ o/ oe ss th t/ ng ??
 &comb2 "' SP '' a a' A A' e e' E E' i i' I I' o o' O O' u u' U U'
		 y y' Y Y' c c' C C' l l' L L' n n' N N' r r' R R'
		 s s' S S' z z' Z Z'
 &comb2 "( SP '( a a( A A( g g( G G(                     u u( U U(
 &comb2 "< SP '< c c< C C< d d< D D< e e< E E< l l< L L< n n< N N<
		 r r< R R< s s< S S< t t< T T< z z< Z Z<
 &comb2 ", SP ', c c, C C, g g, G G, k k, K K, l l, L L, n n, N N,
		 r r, R R, s s, S S, t t, T T,
 &comb2 ">       a a> A A> e e> E E> i i> I I> o o> O O> u u> U U>
		 y y> Y Y> c c> C C> g g> G G> h h> H H> j j> J J>
		 s s> S S> w w> W W>
 &comb2 ": SP ': a a: A A: e e: E E: i i: I I: o o: O O: u u: U U:
		 y y: Y Y:
 &comb2 ". SP '. c c. C C. e e. E E. g g. G G.      I I. z z. Z Z.
 &comb2 "" SP '"                               o o" O O" u u" U U"
 &comb2 "!       a a! A A! e e! E E! i i! I I! o o! O O! u u! U U!
 &comb2 "-       a a- A A- e e- E E- i i- I I- o o- O O- u u- U U-
 &comb2 "; SP '; a a; A A; e e; E E; i i; I I; u u; U U;
 &comb2 "0 SP '0 a aa A AA                               u u0 U U0
 &comb2 "? SP '? a a? A A? n n? N N? i i? I I? o o? O O? u u? U U?

 &charset PT2
 &rem source: ECMA registry
 &alias iso-ir-84
 &alias ISO646-PT2
 &g0esc x2867 &g1esc x2967 &g2esc x2a67 &g3esc x2b67
 &bits 7
 &IRnum 84
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 '' A B C D E F G H I J K L M N O P Q R S T U V W X Y Z A? C, O? '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z a? c, o? '? DT

 &charset ES2
 &rem source: ECMA registry
 &alias iso-ir-85
 &alias ISO646-ES2
 &g0esc x2868 &g1esc x2968 &g2esc x2a68 &g3esc x2b68
 &bits 7
 &IRnum 85
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 sb A B C D E F G H I J K L M N O P Q R S T U V W X Y Z !I N? C, ?I _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z '' n? c, ': DT

 &charset MSZ_7795.3
 &rem source: ECMA registry
 &alias iso-ir-86
 &alias ISO646-HU
 &g0esc x2869 &g1esc x2969 &g2esc x2a69 &g3esc x2b69
 &bits 7
 &alias hu
 &IRnum 86
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb Cu % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 A' A B C D E F G H I J K L M N O P Q R S T U V W X Y Z E' O: U: '> _
 a' a b c d e f g h i j k l m n o p q r s t u v w x y z e' o: u: '" DT

 &charset JIS_C6226-1983
 &rem source: ECMA registry
 &alias iso-ir-87
 &bits 14
! *** Add missing 28 to g0esc
 &g0esc x242842 &g1esc x242942 &g2esc x242a42 &g3esc x242b42
 &alias x0208
 &alias JIS_X0208-1983
 &IRnum 87
 &code2 1 1
 SP ,_ ._ , . .6 : ; ! "5 05 '' '! ': '> '- _ *6 +6 *5 +5 +"
 +_ *_ ;_ 0_ -6 -? -N
 &code2 1 31
 FD BD ?1 PP !! .3 .. '6 '9 "6 "9 ( ) (' )' <( )>
 (! !) <1 >1 </ /> <' >' <" >" (" )" + - +- *X -: = != < > =< >= 00
 .: Ml Fm DG 1' 2' oC Ye DO Ct Pd % Nb & * At SE *1 *2 0m 0M 0o LZ
 &code2 2 1
 Db OS fS uT UT dT DT :X =T -> <- -! -v =_
 &code2 2 26
 (- -) (_ )_ (C )C (U )U
 &code2 2 42
 AN OR NO => <= FA TE
 &code2 2 60
 -V -T (A dP NB =3 HI <* *> RT CG 0( :. In DI
 &code2 2 82
 AA %0 MX Mb M8 /- /= PI
 &code2 2 94
 Ci
 &code2 3 16
 0 1 2 3 4 5 6 7 8 9
 &code2 3 33
 A B C D E F G H I J K L M N O P Q R S T U V W X Y Z
 &code2 3 65
 a b c d e f g h i j k l m n o p q r s t u v w x y z
 &code2 4 1
    A5 a5 I5 i5 U5 u5 E5 e5 O5 o5 ka ga ki gi ku
 gu ke ge ko go sa za si zi su zu se ze so zo ta
 da ti di tU tu du te de to do na ni nu ne no ha
 ba pa hi bi pi hu bu pu he be pe ho bo po ma mi
 mu me mo yA ya yU yu yO yo ra ri ru re ro wA wa
 wi we wo n5
 &code2 5 1
    a6 A6 i6 I6 u6 U6 e6 E6 o6 O6 Ka Ga Ki Gi Ku
 Gu Ke Ge Ko Go Sa Za Si Zi Su Zu Se Ze So Zo Ta
 Da Ti Di TU Tu Du Te De To Do Na Ni Nu Ne No Ha
 Ba Pa Hi Bi Pi Hu Bu Pu He Be Pe Ho Bo Po Ma Mi
 Mu Me Mo YA Ya YU Yu YO Yo Ra Ri Ru Re Ro WA Wa
 Wi We Wo N6 Vi KA KE
 &code2 6 1
 A* B* G* D* E* Z* Y* H* I* K* L* M* N* C* O*
 P* R* S* T* U* F* X* Q* W*
 &code2 6 33
 a* b* g* d* e* z* y* h* i* k* l* m* n* c* o*
 p* r* s* t* u* f* x* q* w*
 &code2 7 1
 A= B= V= G= D= E= IO Z% Z= I= J= K= L= M= N= O= P=
 R= S= T= U= F= H= C= C% S% Sc =" Y= %" JE JU JA
 &code2 7 49
 a= b= v= g= d= e= io z% z= i= j= k= l= m= n= o= p=
 r= s= t= u= f= h= c= c% s% sc =' y= %' je ju ja
 &code2 8 1
 hh vv dr dl ul ur vr dh vl uh vh
 HH VV DR LD UL UR VR DH VL UH VH
 Vr dH Vl uH vH vR Dh vL Uh Vh
 &codex j 16 46 1 94
 &codex j 47 47 1 51
 &codex j 48 83 1 94
 &codex j 84 84 1 4

 &charset greek7
 &rem source: ECMA registry
 &alias iso-ir-88
 &g0esc x286a &g1esc x296a &g2esc x2a6a &g3esc x2b6a
 &bits 7
 &IRnum 88
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb Cu % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A* B* G* D* E* Z* Y* H* I* ?? K* L* M* N* C*
 O* P* R* S* T* U* F* ?? X* Q* W* <( // )> '> _
 '! a* b* g* d* e* z* y* h* i* ?? k* l* m* n* c*
 o* p* r* s* t* u* f* *s x* q* w* (! !! !) '- DT

 &charset ASMO_449
 &rem source: ECMA registry
 &alias ISO_9036
 &alias arabic7
 &alias iso-ir-89
 &g0esc x286b &g1esc x296b &g2esc x2a6b &g3esc x2b6b
 &bits 7
 &IRnum 89
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb Cu % & ' ( ) * + ,+ - . / 0 1 2 3 4 5 6 7 8 9 : ;+ < = > ?+
 At H' aM aH wH ah yH a+ b+ tm t+ tk g+ hk x+ d+
 dk r+ z+ s+ sn c+ dd tj zH e+ i+ <( // )> '> _
 ++ f+ q+ k+ l+ m+ n+ h+ w+ j+ y+ :+ "+ =+ /+ '+
 1+ 3+ 0+ ?? ?? ?? ?? ?? ?? ?? ?? (! !! !) '- DT

 &charset iso-ir-90
 &rem source: ECMA registry
 &alias ISO_6937-2:1983
 &g0esc x286c &g1esc x296c &g2esc x2a6c &g3esc x2b6c
 &bits 8
 &IRnum 90
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb Cu % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '- DT
 PA HO BH NH IN NL SA ES HS HJ VS PD PU RI S2 S3
 DC P1 P2 TS CC MW SG EG SS GC SC CI ST OC PM AC
 ?? !I Ct Pd DO Ye ?? SE ?? '6 "6 << <- -! -> -v
 DG +- 2S 3S *X My PI .M -: '9 "9 >> 14 12 34 ?I
 ?? "! "' "> "? "- "( ". ": ?? "0 ", "_ "" "; "<
 -M 1S Rg Co TM M8 ?? ?? ?? ?? ?? ?? 18 38 58 78
 Om AE D- -a H/ ?? IJ L. L/ O/ OE -o TH T/ NG 'n
 kk ae d/ d- h/ i. ij l. l/ o/ oe ss th t/ ng ??
 &comb2 "' SP '' a a' A A' e e' E E' i i' I I' o o' O O' u u' U U'
		 y y' Y Y' c c' C C' l l' L L' n n' N N' r r' R R'
		 s s' S S' z z' Z Z'
 &comb2 "( SP '( a a( A A( g g( G G(                     u u( U U(
 &comb2 "< SP '< c c< C C< d d< D D< e e< E E< l l< L L< n n< N N<
		 r r< R R< s s< S S< t t< T T< z z< Z Z<
 &comb2 ", SP ', c c, C C, g g, G G, k k, K K, l l, L L, n n, N N,
		 r r, R R, s s, S S, t t, T T,
 &comb2 ">       a a> A A> e e> E E> i i> I I> o o> O O> u u> U U>
		 y y> Y Y> c c> C C> g g> G G> h h> H H> j j> J J>
		 s s> S S> w w> W W>
 &comb2 ": SP ': a a: A A: e e: E E: i i: I I: o o: O O: u u: U U:
		 y y: Y Y:
 &comb2 ". SP '. c c. C C. e e. E E. g g. G G.      I I. z z. Z Z.
 &comb2 "" SP '"                               o o" O O" u u" U U"
 &comb2 "!       a a! A A! e e! E E! i i! I I! o o! O O! u u! U U!
 &comb2 "-       a a- A A- e e- E E- i i- I I- o o- O O- u u- U U-
 &comb2 "; SP '; a a; A A; e e; E E; i i; I I; u u; U U;
 &comb2 "0 SP '0 a aa A AA                               u u0 U U0
 &comb2 "? SP '? a a? A A? n n? N N? i i? I I? o o? O O? u u? U U?

 &charset JIS_C6229-1984-a
 &rem source: ECMA registry
 &alias iso-ir-91
 &g0esc x286d &g1esc x296d &g2esc x2a6d &g3esc x2b6d
 &bits 7
 &alias jp-ocr-a
 &IRnum 91
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ?? " Pd DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; 1h = 3h ?
 ?? A B C D E F G H I J K L M N O P Q R S T U V W X Y Z ?? Ye 2h '> _
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? 4h ?? ?? DT

 &charset JIS_C6229-1984-b
 &rem source: ECMA registry
 &alias iso-ir-92
 &alias ISO646-JP-OCR-B
 &g0esc x286e &g1esc x296e &g2esc x2a6e &g3esc x2b6e
 &alias jp-ocr-b
 &bits 7
 &IRnum 92
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z </ Ye /> '> _
 ?? a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) ?? DT

 &charset JIS_C6229-1984-b-add
 &rem source: ECMA registry
 &alias iso-ir-93
 &g0esc x286f &g1esc x296f &g2esc x2a6f &g3esc x2b6f
 &bits 7
 &alias jp-ocr-b-add
 &IRnum 93
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ?? ?? Pd Cu // ?? SE ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? DT

 &charset JIS_C6229-1984-hand
 &rem source: ECMA registry
 &alias iso-ir-94
 &g0esc x2870 &g1esc x2970 &g2esc x2a70 &g3esc x2b70
 &bits 7
 &alias jp-ocr-hand
 &IRnum 94
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z </ Ye /> '> _
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? !! ?? ?? DT

 &charset JIS_C6229-1984-hand-add
 &rem source: ECMA registry
 &alias iso-ir-95
 &g0esc x2871 &g1esc x2971 &g2esc x2a71 &g3esc x2b71
 &alias jp-ocr-hand-add
 &bits 7
 &IRnum 95
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ?? ?? ?? ?? // ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? DT

 &charset JIS_C6229-1984-kana
 &rem source: ECMA registry
 &alias iso-ir-96
 &g0esc x2872 &g1esc x2972 &g2esc x2a72 &g3esc x2b72
 &bits 7
 &IRnum 96
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ?? <' >' ?? ?? Wo ?? ?? ?? ?? ?? ?? ?? ?? ??
 -6 A6 I6 U6 E6 O6 Ka Ki Ku Ke Ko Sa Si Su Se So
 Ta Ti Tu Te To Na Ni Nu Ne No Ha Hi Hu He Ho Ma
 Mi Mu Me Mo Ya Yu Yo Ra Ri Ru Re Ro Wa N6 "5 05
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? DT

 &charset ISO_2033-1983
 &rem source: ECMA registry
 &alias iso-ir-98
 &alias e13b
 &g0esc x2873 &g1esc x2973 &g2esc x2a73 &g3esc x2b73
 &bits 7
 &IRnum 98
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 0  1  2  3  4  5  6  7  8  9  1j 2j 3j 4j ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? DT

 &charset ANSI_X3.110-1983
 &rem source: ECMA registry
 &alias iso-ir-99
 &alias CSA_T500-1983
 &alias NAPLPS
 &g0esc x2874 &g1esc x2974 &g2esc x2a74 &g3esc x2b74
 &bits 8
 &IRnum 99
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " ?? ?? % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 PA HO BH NH IN NL SA ES HS HJ VS PD PU RI S2 S3
 DC P1 P2 TS CC MW SG EG SS GC SC CI ST OC PM AC
 ?? !I Ct Pd DO Ye Nb SE Cu '6 "6 << <- -! -> -v
 DG +- 2S 3S *X My PI .M -: '9 "9 >> 14 12 34 ?I
 ?? "! "' "> "? "- "( ". ": "/ "0 ", "_ "" "; "<
 -M 1S Rg Co TM M8 hh vv FD BD Fd Bd 18 38 58 78
 Om AE D- -a H/ vh IJ L. L/ O/ OE -o TH T/ NG 'n
 kk ae d/ d- h/ i. ij l. l/ o/ oe ss th t/ ng ??
 &comb2 "' SP '' a a' A A' e e' E E' i i' I I' o o' O O' u u' U U'
		 y y' Y Y' c c' C C' l l' L L' n n' N N' r r' R R'
		 s s' S S' z z' Z Z'
 &comb2 "( SP '( a a( A A( g g( G G(                     u u( U U(
 &comb2 "< SP '< c c< C C< d d< D D< e e< E E< l l< L L< n n< N N<
		 r r< R R< s s< S S< t t< T T< z z< Z Z<
 &comb2 ", SP ', c c, C C, g g, G G, k k, K K, l l, L L, n n, N N,
		 r r, R R, s s, S S, t t, T T,
 &comb2 ">       a a> A A> e e> E E> i i> I I> o o> O O> u u> U U>
		 y y> Y Y> c c> C C> g g> G G> h h> H H> j j> J J>
		 s s> S S> w w> W W>
 &comb2 ": SP ': a a: A A: e e: E E: i i: I I: o o: O O: u u: U U:
		 y y: Y Y:
 &comb2 ". SP '. c c. C C. e e. E E. g g. G G.      I I. z z. Z Z.
 &comb2 "" SP '"                               o o" O O" u u" U U"
 &comb2 "!       a a! A A! e e! E E! i i! I I! o o! O O! u u! U U!
 &comb2 "- SP 'm a a- A A- e e- E E- i i- I I- o o- O O- u u- U U-
 &comb2 "; SP '; a a; A A; e e; E E; i i; I I; u u; U U;
 &comb2 "0 SP '0 a aa A AA                               u u0 U U0
 &comb2 "?       a a? A A? n n? N N? i i? I I? o o? O O? u u? U U?

 &charset ISO-8859-1
 &rem source: ECMA registry
 &alias iso-ir-100
 &g1esc x2d41 &g2esc x2e41 &g3esc x2f41
 &bits 8
 &alias ISO_8859-1:1987
 &alias ISO_8859-1
 &alias latin1
 &alias latin-1
 &alias l1
 &alias IBM819
 &alias CP819
 &IRnum 100
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 PA HO BH NH IN NL SA ES HS HJ VS PD PU RI S2 S3
 DC P1 P2 TS CC MW SG EG SS GC SC CI ST OC PM AC
 NS !I Ct Pd Cu Ye BB SE ': Co -a << NO -- Rg 'm
 DG +- 2S 3S '' My PI .M ', 1S -o >> 14 12 34 ?I
 A! A' A> A? A: AA AE C, E! E' E> E: I! I' I> I:
 D- N? O! O' O> O? O: *X O/ U! U' U> U: Y' TH ss
 a! a' a> a? a: aa ae c, e! e' e> e: i! i' i> i:
 d- n? o! o' o> o? o: -: o/ u! u' u> u: y' th y:

 &charset ISO-8859-2
 &rem source: ECMA registry
 &alias iso-ir-101
 &g1esc x2d42 &g2esc x2e42 &g3esc x2f42
 &bits 8
 &alias ISO_8859-2:1987
 &alias ISO_8859-2
 &alias latin2
 &alias latin-2
 &alias l2
 &IRnum 101
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 PA HO BH NH IN NL SA ES HS HJ VS PD PU RI S2 S3
 DC P1 P2 TS CC MW SG EG SS GC SC CI ST OC PM AC
 NS A; '( L/ Cu L< S' SE ': S< S, T< Z' -- Z< Z.
 DG a; '; l/ '' l< s' '< ', s< s, t< z' '" z< z.
 R' A' A> A( A: L' C' C, C< E' E; E: E< I' I> D<
 D/ N' N< O' O> O" O: *X R< U0 U' U" U: Y' T, ss
 r' a' a> a( a: l' c' c, c< e' e; e: e< i' i> d<
 d/ n' n< o' o> o" o: -: r< u0 u' u" u: y' t, '.

 &charset T-61-7bit
 &alias T.61-7bit
 &rem source: ECMA registry
 &alias iso-ir-102
 &g0esc x2875 &g1esc x2975 &g2esc x2a75 &g3esc x2b75
 &bits 7
 &IRnum 102
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb Cu % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( ?? )> ?? _
 ?? a b c d e f g h i j k l m n o p q r s t u v w x y z ?? !! ?? ?? DT

 &charset T-61
 &alias T.61
 &alias T.61-8bit
 &alias T-61-8bit
 &alias T61
 &rem source: ECMA registry
 &alias iso-ir-103
 &g0esc x2876 &g1esc x2976 &g2esc x2a76 &g3esc x2b76
 &bits 8
 &IRnum 103
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " ?? ?? % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( ?? )> ?? _
 ?? a b c d e f g h i j k l m n o p q r s t u v w x y z ?? !! ?? ?? DT
 PA HO BH NH IN NL SA ES HS HJ VS PD PU RI S2 S3
 DC P1 P2 TS CC MW SG EG SS GC SC CI ST OC PM AC
 ?? !I Ct Pd DO Ye Nb SE Cu ?? ?? << ?? ?? ?? ??
 DG +- 2S 3S *X My PI .M -: ?? ?? >> 14 12 34 ?I
 ?? "! "' "> "? "- "( ". ": ?? "0 ", "_ "" "; "<
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 Om AE D- -a H/ ?? IJ L. L/ O/ OE -o TH T/ NG 'n
 kk ae d/ d- h/ i. ij l. l/ o/ oe ss th t/ ng ??
 &comb2 "' SP '' a a' A A' e e' E E' i i' I I' o o' O O' u u' U U'
		 y y' Y Y' c c' C C' l l' L L' n n' N N' r r' R R'
		 s s' S S' z z' Z Z'
 &comb2 "( SP '( a a( A A( g g( G G(                     u u( U U(
 &comb2 "< SP '< c c< C C< d d< D D< e e< E E< l l< L L< n n< N N<
		 r r< R R< s s< S S< t t< T T< z z< Z Z<
 &comb2 ", SP ', c c, C C, g g, G G, k k, K K, l l, L L, n n, N N,
		 r r, R R, s s, S S, t t, T T,
 &comb2 ">       a a> A A> e e> E E> i i> I I> o o> O O> u u> U U>
		 y y> Y Y> c c> C C> g g> G G> h h> H H> j j> J J>
		 s s> S S> w w> W W>
 &comb2 ": SP ': a a: A A: e e: E E: i i: I I: o o: O O: u u: U U:
		 y y: Y Y:
 &comb2 ". SP '. c c. C C. e e. E E. g g. G G.      I I. z z. Z Z.
 &comb2 "" SP '"                               o o" O O" u u" U U"
 &comb2 "!       a a! A A! e e! E E! i i! I I! o o! O O! u u! U U!
 &comb2 "- SP 'm a a- A A- e e- E E- i i- I I- o o- O O- u u- U U-
 &comb2 "; SP '; a a; A A; e e; E E; i i; I I; u u; U U;
 &comb2 "0 SP '0 a aa A AA                               u u0 U U0
 &comb2 "?       a a? A A? n n? N N? i i? I I? o o? O O? u u? U U?

 &charset ISO-8859-3
 &rem source: ECMA registry
 &alias iso-ir-109
 &g1esc x2d43 &g2esc x2e43 &g3esc x2f43
 &bits 8
 &alias ISO_8859-3:1988
 &alias ISO_8859-3
 &alias latin3
 &alias latin-3
 &alias l3
 &IRnum 109
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 PA HO BH NH IN NL SA ES HS HJ VS PD PU RI S2 S3
 DC P1 P2 TS CC MW SG EG SS GC SC CI ST OC PM AC
 NS H/ '( Pd Cu ?? H> SE ': I. S, G( J> -- ?? Z.
 DG h/ 2S 3S '' My h> .M ', i. s, g( j> 12 ?? z.
 A! A' A> ?? A: C. C> C, E! E' E> E: I! I' I> I:
 ?? N? O! O' O> G. O: *X G> U! U' U> U: U( S> ss
 a! a' a> ?? a: c. c> c, e! e' e> e: i! i' i> i:
 ?? n? o! o' o> g. o: -: g> u! u' u> u: u( s> '.

 &charset ISO-8859-4
 &rem source: ECMA registry
 &alias iso-ir-110
 &g1esc x2d44 &g2esc x2e44 &g3esc x2f44
 &bits 8
 &alias ISO_8859-4:1988
 &alias ISO_8859-4
 &alias latin4
 &alias latin-4
 &alias l4
 &IRnum 110
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 PA HO BH NH IN NL SA ES HS HJ VS PD PU RI S2 S3
 DC P1 P2 TS CC MW SG EG SS GC SC CI ST OC PM AC
 NS A; kk R, Cu I? L, SE ': S< E- G, T/ -- Z< 'm
 DG a; '; r, '' i? l, '< ', s< e- g, t/ NG z< ng
 A- A' A> A? A: AA AE I; C< E' E; E: E. I' I> I-
 D/ N, O- K, O> O? O: *X O/ U; U' U> U: U? U- ss
 a- a' a> a? a: aa ae i; c< e' e; e: e. i' i> i-
 d/ n, o- k, o> o? o: -: o/ u; u' u> u: u? u- '.

 &charset ECMA-cyrillic
 &rem source: ECMA registry
 &alias iso-ir-111
 &g1esc x2d40 &g2esc x2e40 &g3esc x2f40
 &bits 8
 &IRnum 111
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 PA HO BH NH IN NL SA ES HS HJ VS PD PU RI S2 S3
 DC P1 P2 TS CC MW SG EG SS GC SC CI ST OC PM AC
 NS d% g% io ie ds ii yi j% lj nj ts kj -- v% dz
 N0 D% G% IO IE DS II YI J% LJ NJ Ts KJ Cu V% DZ
 ju a= b= c= d= e= f= g= h= i= j= k= l= m= n= o=
 p= ja r= s= t= u= z% v= %' y= z= s% je sc c% ='
 JU A= B= C= D= E= F= G= H= I= J= K= L= M= N= O=
 P= JA R= S= T= U= Z% V= %" Y= Z= S% JE Sc C% ="

 &charset CSA_Z243.4-1985-1
 &rem source: ECMA registry
 &alias iso-ir-121
 &g0esc x2877 &g1esc x2977 &g2esc x2a77 &g3esc x2b77
 &bits 7
 &alias ISO646-CA
 &alias csa7-1
 &alias ca
 &IRnum 121
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 a! A B C D E F G H I J K L M N O P Q R S T U V W X Y Z a> c, e> i> _
 o> a b c d e f g h i j k l m n o p q r s t u v w x y z e' u! e! u> DT

 &charset CSA_Z243.4-1985-2
 &rem source: ECMA registry
 &alias iso-ir-122
 &alias ISO646-CA2
 &g0esc x2878 &g1esc x2978 &g2esc x2a78 &g3esc x2b78
 &bits 7
 &alias csa7-2
 &IRnum 122
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 a! A B C D E F G H I J K L M N O P Q R S T U V W X Y Z a> c, e> E' _
 o> a b c d e f g h i j k l m n o p q r s t u v w x y z e' u! e! u> DT

 &charset CSA_Z243.4-1985-gr
 &rem source: ECMA registry
 &alias iso-ir-123
 &g1esc x2d45 &g2esc x2e45 &g3esc x2f45
 &bits 8
 &IRnum 123
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 PA HO BH NH IN NL SA ES HS HJ VS PD PU RI S2 S3
 DC P1 P2 TS CC MW SG EG SS GC SC CI ST OC PM AC
 NS !I ': Pd Ct Ye +- '' (S )S 12 +S ', -- .M -S
 0S 1S 2S 3S 4S 5S 6S 7S 8S 9S 14 34 <= != >= ?I
 A! A' A> C, E! E' E> E: I' I> I: N? O' O> U! U'
 U> U: Rg SE PI My -a -o '6 '9 "6 "9 << >> DG BB
 a! a' a> c, e! e' e> e: i' i> i: n? o' o> u! u'
 u> u: Co hh vv ur ul dl dr vr uh vl dh vh NO FB

 &charset ISO-8859-7
 &rem source: ECMA registry
 &alias iso-ir-126
 &g1esc x2d46 &g2esc x2e46 &g3esc x2f46
 &bits 8
 &alias ISO_8859-7:1987
 &alias ISO_8859-7
 &alias ELOT_928
 &alias ECMA-118
 &alias greek
 &alias greek8
 &IRnum 126
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 PA HO BH NH IN NL SA ES HS HJ VS PD PU RI S2 S3
 DC P1 P2 TS CC MW SG EG SS GC SC CI ST OC PM AC
 NS 9' '9 Pd ?? ?? BB SE ': Co ?? << NO -- ?? -M
 DG +- 2S 3S '' '% A% .M E% Y% I% >> O% 12 U% W%
 i3 A* B* G* D* E* Z* Y* H* I* K* L* M* N* C* O*
 P* R* ?? S* T* U* F* X* Q* W* J* V* a% e% y% i%
 u3 a* b* g* d* e* z* y* h* i* k* l* m* n* c* o*
 p* r* *s s* t* u* f* x* q* w* j* v* o% u% w% ??

 &charset ISO-8859-6
 &rem source: ECMA registry
 &alias iso-ir-127
 &g1esc x2d47 &g2esc x2e47 &g3esc x2f47
 &bits 8
 &alias ISO_8859-6:1987
 &alias ISO_8859-6
 &alias ECMA-114
 &alias ASMO-708
 &alias arabic
 &IRnum 127
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 PA HO BH NH IN NL SA ES HS HJ VS PD PU RI S2 S3
 DC P1 P2 TS CC MW SG EG SS GC SC CI ST OC PM AC
 NS ?? ?? ?? Cu ?? ?? ?? ?? ?? ?? ?? ,+ -- ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ;+ ?? ?? ?? ?+
 ?? H' aM aH wH ah yH a+ b+ tm t+ tk g+ hk x+ d+
 dk r+ z+ s+ sn c+ dd tj zH e+ i+ ?? ?? ?? ?? ??
 ++ f+ q+ k+ l+ m+ n+ h+ w+ j+ y+ :+ "+ =+ /+ '+
 1+ 3+ 0+ ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??

 &charset T.101-G2
 &rem source: ECMA registry
 &alias iso-ir-128
 &g0esc x287c &g1esc x297c &g2esc x2a7c &g3esc x2b7c
 &bits 8
 &IRnum 128
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " ?? ?? % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 PA HO BH NH IN NL SA ES HS HJ VS PD PU RI S2 S3
 DC P1 P2 TS CC MW SG EG SS GC SC CI ST OC PM AC
 ?? !I Ct Pd DO Ye Nb SE Cu '6 "6 << <- -! -> -v
 DG +- 2S 3S *X My PI .M -: '9 "9 >> 14 12 34 ?I
 ?? "! "' "> "? "- "( ". ": "/ "0 ", "_ "" "; "<
 -M 1S Rg Co TM M8 hh vv FD BD Fd Bd 18 38 58 78
 Om AE D- -a H/ vh IJ L. L/ O/ OE -o TH T/ NG 'n
 kk ae d/ d- h/ i. ij l. l/ o/ oe ss th t/ ng ??
 &comb2 "' SP '' a a' A A' e e' E E' i i' I I' o o' O O' u u' U U'
		 y y' Y Y' c c' C C' l l' L L' n n' N N' r r' R R'
		 s s' S S' z z' Z Z'
 &comb2 "( SP '( a a( A A( g g( G G(                     u u( U U(
 &comb2 "< SP '< c c< C C< d d< D D< e e< E E< l l< L L< n n< N N<
		 r r< R R< s s< S S< t t< T T< z z< Z Z<
 &comb2 ", SP ', c c, C C, g g, G G, k k, K K, l l, L L, n n, N N,
		 r r, R R, s s, S S, t t, T T,
 &comb2 ">       a a> A A> e e> E E> i i> I I> o o> O O> u u> U U>
		 y y> Y Y> c c> C C> g g> G G> h h> H H> j j> J J>
		 s s> S S> w w> W W>
 &comb2 ": SP ': a a: A A: e e: E E: i i: I I: o o: O O: u u: U U:
		 y y: Y Y:
 &comb2 ". SP '. c c. C C. e e. E E. g g. G G.      I I. z z. Z Z.
 &comb2 "" SP '"                               o o" O O" u u" U U"
 &comb2 "!       a a! A A! e e! E E! i i! I I! o o! O O! u u! U U!
 &comb2 "- SP 'm a a- A A- e e- E E- i i- I I- o o- O O- u u- U U-
 &comb2 "; SP '; a a; A A; e e; E E; i i; I I; u u; U U;
 &comb2 "0 SP '0 a aa A AA                               u u0 U U0
 &comb2 "?       a a? A A? n n? N N? i i? I I? o o? O O? u u? U U?

 &charset ISO-8859-8
 &rem source: ECMA registry
 &alias iso-ir-138
 &g1esc x2d48 &g2esc x2e48 &g3esc x2f48
 &bits 8
 &alias ISO_8859-8:1988
 &alias ISO_8859-8
 &alias hebrew
 &IRnum 138
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 PA HO BH NH IN NL SA ES HS HJ VS PD PU RI S2 S3
 DC P1 P2 TS CC MW SG EG SS GC SC CI ST OC PM AC
 NS ?? Ct Pd Cu Ye BB SE ': Co *X << NO -- Rg '-
 DG +- 2S 3S '' My PI .M ', 1S -: >> 14 12 34 ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? =2
 A+ B+ G+ D+ H+ W+ Z+ X+ Tj J+ K% K+ L+ M% M+ N%
 N+ S+ E+ P% P+ Zj ZJ Q+ R+ Sh T+ ?? ?? ?? ?? ??

 &charset CSN_369103
 &rem source: ECMA registry
 &alias iso-ir-139
 &g1esc x2d49 &g2esc x2e49 &g3esc x2f49
 &bits 8
 &IRnum 139
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb Cu % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 PA HO BH NH IN NL SA ES HS HJ VS PD PU RI S2 S3
 DC P1 P2 TS CC MW SG EG SS GC SC CI ST OC PM AC
 NS A; '( L/ DO L< S' SE ': S< S, T< Z' -- Z< Z.
 DG a; '; l/ '' l< s' '< ', s< s, t< z' '" z< z.
 R' A' A> A( A: L' C' C, C< E' E; E: E< I' I> D<
 D/ N' N< O' O> O" O: *X R< U0 U' U" U: Y' T, ss
 r' a' a> a( a: l' c' c, c< e' e; e: e< i' i> d<
 d/ n' n< o' o> o" o: -: r< u0 u' u" u: y' t, '.

 &charset JUS_I.B1.002
 &rem source: ECMA registry
 &alias iso-ir-141
 &g0esc x287a &g1esc x297a &g2esc x2a7a &g3esc x2b7a
 &bits 7
 &alias ISO646-YU
 &alias js
 &alias yu
 &IRnum 141
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 Z< A B C D E F G H I J K L M N O P Q R S T U V W X Y Z S< D/ C' C< _
 z< a b c d e f g h i j k l m n o p q r s t u v w x y z s< d/ c' c< DT

 &charset ISO_6937-2-add
 &rem source: ECMA registry and ISO 6937-2:1983
 &alias iso-ir-142
 &g1esc x2d4a &g2esc x2e4a &g3esc x2f4a
 &bits 8
 &IRnum 142
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb Cu % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 PA HO BH NH IN NL SA ES HS HJ VS PD PU RI S2 S3
 DC P1 P2 TS CC MW SG EG SS GC SC CI ST OC PM AC
 NS !I Ct Pd DO Ye ?? SE ?? '6 "6 << <- -! -> -v
 DG +- 2S 3S *X My PI .M -: '9 "9 >> 14 12 34 ?I
 ?? "! "' "> "? "- "( ". ": ?? "0 ", "_ "" "; "<
 -M 1S Rg Co TM M8 NO BB ?? ?? ?? ?? 18 38 58 78
 Om AE D- -a H/ ?? IJ L. L/ O/ OE -o TH T/ NG 'n
 kk ae d/ d- h/ i. ij l. l/ o/ oe ss th t/ ng --
 &comb2 "' SP '' a a' A A' e e' E E' i i' I I' o o' O O' u u' U U'
		 y y' Y Y' c c' C C' l l' L L' n n' N N' r r' R R'
		 s s' S S' z z' Z Z'
 &comb2 "( SP '( a a( A A( g g( G G(                     u u( U U(
 &comb2 "< SP '< c c< C C< d d< D D< e e< E E< l l< L L< n n< N N<
		 r r< R R< s s< S S< t t< T T< z z< Z Z<
 &comb2 ", SP ', c c, C C, g g, G G, k k, K K, l l, L L, n n, N N,
		 r r, R R, s s, S S, t t, T T,
 &comb2 ">       a a> A A> e e> E E> i i> I I> o o> O O> u u> U U>
		 y y> Y Y> c c> C C> g g> G G> h h> H H> j j> J J>
		 s s> S S> w w> W W>
 &comb2 ": SP ': a a: A A: e e: E E: i i: I I: o o: O O: u u: U U:
		 y y: Y Y:
 &comb2 ". SP '. c c. C C. e e. E E. g g. G G.      I I. z z. Z Z.
 &comb2 "" SP '"                               o o" O O" u u" U U"
 &comb2 "!       a a! A A! e e! E E! i i! I I! o o! O O! u u! U U!
 &comb2 "- SP 'm a a- A A- e e- E E- i i- I I- o o- O O- u u- U U-
 &comb2 "; SP '; a a; A A; e e; E E; i i; I I; u u; U U;
 &comb2 "0 SP '0 a aa A AA                               u u0 U U0
 &comb2 "?       a a? A A? n n? N N? i i? I I? o o? O O? u u? U U?

 &charset IEC_P27-1
 &rem source: ECMA registry
 &alias iso-ir-143
 &g1esc x2d4b &g2esc x2e4b &g3esc x2f4b
 &bits 8
 &IRnum 143
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 PA HO BH NH IN NL SA ES HS HJ VS PD PU RI S2 S3
 DC P1 P2 TS CC MW SG EG SS GC SC CI ST OC PM AC
 '< =3 AN OR (U )U (C )C <= => .: :. (- -) (_ )_
 In Io 00 NB dP ?1 ?2 ?- ?= =< != >= <> NO FA TE
 A+ OS PP G* D* -T -V -L H* </ /> L* 1' 2' C* -+
 P* 2S S* *X 3S U* F* .M Q* W* /0 >V RT f2 0( +-
 DG a* b* g* d* e* z* y* h* i* k* l* m* n* c* %0
 p* r* s* -: t* u* f* x* q* w* /- <- -! -> -v '-

 &charset ISO-8859-5
 &rem source: ECMA registry
 &alias iso-ir-144
 &g1esc x2d4c &g2esc x2e4c &g3esc x2f4c
 &bits 8
 &alias ISO_8859-5:1988
 &alias ISO_8859-5
 &alias cyrillic
 &IRnum 144
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 PA HO BH NH IN NL SA ES HS HJ VS PD PU RI S2 S3
 DC P1 P2 TS CC MW SG EG SS GC SC CI ST OC PM AC
 NS IO D% G% IE DS II YI J% LJ NJ Ts KJ -- V% DZ
 A= B= V= G= D= E= Z% Z= I= J= K= L= M= N= O= P=
 R= S= T= U= F= H= C= C% S% Sc =" Y= %" JE JU JA
 a= b= v= g= d= e= z% z= i= j= k= l= m= n= o= p=
 r= s= t= u= f= h= c= c% s% sc =' y= %' je ju ja
 N0 io d% g% ie ds ii yi j% lj nj ts kj SE v% dz

 &charset JUS_I.B1.003-serb
 &rem source: ECMA registry
 &alias iso-ir-146
 &g0esc x287b &g1esc x297b &g2esc x2a7b &g3esc x2b7b
 &bits 7
 &alias serbian
 &IRnum 146
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 Z% A= B= C= D= E= F= G= H= I= J% K= L= M= N= O=
 P= LJ R= S= T= U= V= NJ DZ DS Z= S% D% Ts C% _
 z% a= b= c= d= e= f= g= h= i= j% k= l= m= n= o=
 p= lj r= s= t= u= v= nj dz ds z= s% d% ts c% DT

 &charset JUS_I.B1.003-mac
 &rem source: ECMA registry
 &alias macedonian
 &alias iso-ir-147
 &g0esc x287d &g1esc x297d &g2esc x2a7d &g3esc x2b7d
 &bits 7
 &IRnum 147
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 Z% A= B= C= D= E= F= G= H= I= J% K= L= M= N= O=
 P= LJ R= S= T= U= V= NJ DZ DS Z= S% G% KJ C% _
 z% a= b= c= d= e= f= g= h= i= j% k= l= m= n= o=
 p= lj r= s= t= u= v= nj dz ds z= s% g% kj c% DT

 &charset ISO-8859-9
 &rem source: ECMA registry
 &alias iso-ir-148
 &g1esc x2d4d &g2esc x2e4d &g3esc x2f4d
 &bits 8
 &alias ISO_8859-9:1989
 &alias ISO_8859-9
 &alias latin5
 &alias latin-5
 &alias l5
 &IRnum 148
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 PA HO BH NH IN NL SA ES HS HJ VS PD PU RI S2 S3
 DC P1 P2 TS CC MW SG EG SS GC SC CI ST OC PM AC
 NS !I Ct Pd Cu Ye BB SE ': Co -a << NO -- Rg 'm
 DG +- 2S 3S '' My PI .M ', 1S -o >> 14 12 34 ?I
 A! A' A> A? A: AA AE C, E! E' E> E: I! I' I> I:
 G( N? O! O' O> O? O: *X O/ U! U' U> U: I. S, ss
 a! a' a> a? a: aa ae c, e! e' e; e: e. i' i> i-
 g( n? o! o' o> o? o: -: o/ u! u' u> u: i. s, y:

 &charset greek-ccitt
 &rem source: ECMA registry
 &alias iso-ir-150
 &g0esc x282140 &g1esc x292140 &g2esc x2a2140 &g3esc x2b2140
 &bits 7
 &IRnum 150
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb Cu % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A* B* G* D* E* Z* Y* H* I* K* L* M* N* C* O*
 P* R* ?? S* T* U* F* X* Q* W* ?? <( // )> '> _
 ?? a* b* g* d* e* z* y* h* i* k* l* m* n* c* o*
 p* r* *s s* t* u* f* x* q* w* ?? (! !! !) 'm DT

 &charset NC_NC00-10
 &rem source: ECMA registry
 &alias cuba
 &alias NC_NC00-10:81
 &alias iso-ir-151
 &alias ISO646-CU
 &g0esc x282141 &g1esc x292141 &g2esc x2a2141 &g3esc x2b2141
 &bits 7
 &IRnum 151
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb Cu % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z !I N? )> ?I _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z '' n? <( ': DT

 &charset ISO_6937-2-25
 &rem source: ECMA registry
 &alias iso-ir-152
 &g1esc x2d4e &g2esc x2e4e &g3esc x2f4e
 &bits 8
 &IRnum 152
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb Cu % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 PA HO BH NH IN NL SA ES HS HJ VS PD PU RI S2 S3
 DC P1 P2 TS CC MW SG EG SS GC SC CI ST OC PM AC
 NS ?? ?? ?? ?? ?? ?? ?? ?? ?? "6 ?? <- -! -> -v
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? "9 ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? TM M8 ?? ?? ?? ?? ?? ?? 18 38 58 78
 Om ?? ?? ?? ?? ?? IJ L. ?? ?? OE ?? W> Y> Y: 'n
 ?? ?? ?? ?? ?? ?? ij l. ?? ?? oe ?? w> y> ?? ??

 &charset GOST_19768-74
 &rem source: ECMA registry
 &alias ST_SEV_358-88
 &alias iso-ir-153
 &g1esc x2d4f &g2esc x2e4f &g3esc x2f4f
 &bits 8
 &IRnum 153
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 PA HO BH NH IN NL SA ES HS HJ VS PD PU RI S2 S3
 DC P1 P2 TS CC MW SG EG SS GC SC CI ST OC PM AC
 NS IO ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? -- ?? ??
 A= B= V= G= D= E= Z% Z= I= J= K= L= M= N= O= P=
 R= S= T= U= F= H= C= C% S% Sc =" Y= %" JE JU JA
 a= b= v= g= d= e= z% z= i= j= k= l= m= n= o= p=
 r= s= t= u= f= h= c= c% s% sc =' y= %' je ju ja
 ?? io ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??

 &charset ISO_8859-supp
 &rem source: ECMA registry
 &alias iso-ir-154
 &alias latin1-2-5
 &g1esc x2d50 &g2esc x2e50 &g3esc x2f50
 &bits 8
 &IRnum 154
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 PA HO BH NH IN NL SA ES HS HJ VS PD PU RI S2 S3
 DC P1 P2 TS CC MW SG EG SS GC SC CI ST OC PM AC
 ?? ?? A- C> C. ?? E. E- G> '6 "6 TM <- -! -> -v
 ?? ?? a- c> c. d- e. e- g> '9 "9 M8 18 38 58 78
 ?? G( G. G, H> H/ I? I. I- I; IJ J> K, L, L. N,
 -M NG O- OE R, S> T/ TH U? U( U- U; W> Y' Y> Y:
 Om g( g. g, h> h/ i? i. i- i; ij j> k, l, l. n,
 kk ng o- oe r, s> t/ th u? u( u- u; w> y' y> 'n

 &charset ISO_10367-box
 &rem source: ECMA registry
 &alias iso-ir-155
 &g1esc x2d51 &g2esc x2e51 &g3esc x2f51
 &bits 8
 &IRnum 155
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 PA HO BH NH IN NL SA ES HS HJ VS PD PU RI S2 S3
 DC P1 P2 TS CC MW SG EG SS GC SC CI ST OC PM AC
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 VV HH DR LD UR UL VR VL DH UH VH UB LB FB sB ??
 vv hh dr dl ur ul vr vl dh uh vh .S :S ?S ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??

 &charset ISO_6937
 &rem source: ECMA registry and ISO/IEC 6937:1992
 &alias iso-ir-156
 &alias ISO_6937:1992
 &alias ISO6937
 &g1esc x2d52 &g2esc x2e52 &g3esc x2f52
 &bits 8
 &IRnum 156
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 PA HO BH NH IN NL SA ES HS HJ VS PD PU RI S2 S3
 DC P1 P2 TS CC MW SG EG SS GC SC CI ST OC PM AC
 NS !I Ct Pd ?? Ye ?? SE Cu '6 "6 << <- -! -> -v
 DG +- 2S 3S *X My PI .M -: '9 "9 >> 14 12 34 ?I
 ?? "! "' "> "? "- "( ". ": "_ "0 ", ?? "" "; "<
 -M 1S Rg Co TM M8 NO BB ?? ?? ?? ?? 18 38 58 78
 Om AE D- -a H/ ?? IJ L. L/ O/ OE -o TH T/ NG 'n
 kk ae d/ d- h/ i. ij l. l/ o/ oe ss th t/ ng --
 &comb2 "' SP '' a a' A A' e e' E E' i i' I I' o o' O O' u u' U U'
		 y y' Y Y' c c' C C' l l' L L' n n' N N' r r' R R'
		 s s' S S' z z' Z Z'
 &comb2 "( SP '( a a( A A( g g( G G(                     u u( U U(
 &comb2 "< SP '< c c< C C< d d< D D< e e< E E< l l< L L< n n< N N<
		 r r< R R< s s< S S< t t< T T< z z< Z Z<
 &comb2 ", SP ', c c, C C, g g, G G, k k, K K, l l, L L, n n, N N,
		 r r, R R, s s, S S, t t, T T,
 &comb2 ">       a a> A A> e e> E E> i i> I I> o o> O O> u u> U U>
		 y y> Y Y> c c> C C> g g> G G> h h> H H> j j> J J>
		 s s> S S> w w> W W>
 &comb2 ": SP ': a a: A A: e e: E E: i i: I I: o o: O O: u u: U U:
		 y y: Y Y:
 &comb2 ". SP '. c c. C C. e e. E E. g g. G G.      I I. z z. Z Z.
 &comb2 "" SP '"                               o o" O O" u u" U U"
 &comb2 "!       a a! A A! e e! E E! i i! I I! o o! O O! u u! U U!
 &comb2 "- SP 'm a a- A A- e e- E E- i i- I I- o o- O O- u u- U U-
 &comb2 "; SP '; a a; A A; e e; E E; i i; I I; u u; U U;
 &comb2 "0 SP '0 a aa A AA                               u u0 U U0
 &comb2 "?       a a? A A? n n? N N? i i? I I? o o? O O? u u? U U?

 &charset ISO-8859-10
 &rem source: ECMA registry
 &g1esc x2d56 &g2esc x2e56 &g3esc x2f56
 &alias iso-ir-157
 &alias ISO_8859-10:1993
 &alias ISO_8859-10
 &alias L6
 &alias latin6
 &alias latin-6
 &alias csISOLatin6
 &bits 8
 &IRnum 157
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 PA HO BH NH IN NL SA ES HS HJ VS PD PU RI S2 S3
 DC P1 P2 TS CC MW SG EG SS GC SC CI ST OC PM AC
 NS A; E- G, I- I? K, SE L, D/ S< T/ Z< -- U- NG
 DG a; e- g, i- i? k, .M l, d/ s< t/ z< -M u- ng
 A- A' A> A? A: AA AE I; C< E' E; E: E. I' I> I:
 D- N, O- O' O> O? O: U? O/ U; U' U> U: Y' TH ss
 a- a' a> a? a: aa ae i; c< e' e; e: e. i' i> i:
 d- n, o- o' o> o? o: u? o/ u; u' u> u: y' th kk

 &charset ISO-8859-14
 &rem source: ISO-8859-14
 &g1esc x2d5f &g2esc x2e5f &g3esc x2f5f
 &bits 8
 &alias ISO_8859-14
 &alias iso-ir-199
 &alias latin8
 &alias latin-8
 &alias l8
 &alias csISOLatin8
 &IRnum 199
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 PA HO BH NH IN NL SA ES HS HJ VS PD PU RI S2 S3
 DC P1 P2 TS CC MW SG EG SS GC SC CI ST OC PM AC
 NS B. b. Pd C. c. D. SE W! Co W' d. Y! -- Rg Y:
 F. f. G. g. M. m. PI P. w! p. w' S. y! W: w: s.
 A! A' A> A? A: AA AE C, E! E' E> E: I! I' I> I:
 W> N? O! O' O> O? O: T. O/ U! U' U> U: Y' Y> ss
 a! a' a> a? a: aa ae c, e! e' e> e: i! i' i> i:
 w> n? o! o' o> o? o: t. o/ u! u' u> u: y' y> y:

 &charset ISO-8859-15
 &rem source: ISO-8859-15
 &g1esc x2d62 &g2esc x2e62 &g3esc x2f62
 &bits 8
 &alias ISO_8859-15
 &alias iso-ir-203
 &alias latin9
 &alias latin-9
 &alias l9
 &alias csISOLatin9
 &alias latin0
 &alias latin-0
 &alias l0
 &alias csISOLatin0
 &IRnum 203
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 PA HO BH NH IN NL SA ES HS HJ VS PD PU RI S2 S3
 DC P1 P2 TS CC MW SG EG SS GC SC CI ST OC PM AC
 NS !I Ct Pd EU Ye S< SE s< Co -a << NO -- Rg 'm
 DG +- 2S 3S Z< My PI .M z< 1S -o >> OE oe Y: ?I
 A! A' A> A? A: AA AE C, E! E' E> E: I! I' I> I:
 D- N? O! O' O> O? O: *X O/ U! U' U> U: Y' TH ss
 a! a' a> a? a: aa ae c, e! e' e> e: i! i' i> i:
 d- n? o! o' o> o? o: -: o/ u! u' u> u: y' th y:

 &charset iso-ir-204
 &rem source: ECMA registry
 &g1esc x2d63 &g2esc x2e63 &g3esc x2f63
 &bits 8
 &IRnum 204
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 PA HO BH NH IN NL SA ES HS HJ VS PD PU RI S2 S3
 DC P1 P2 TS CC MW SG EG SS GC SC CI ST OC PM AC
 NS !I Ct Pd EU Ye BB SE ': Co -a << NO -- Rg 'm
 DG +- 2S 3S '' My PI .M ', 1S -o >> 14 12 34 ?I
 A! A' A> A? A: AA AE C, E! E' E> E: I! I' I> I:
 D- N? O! O' O> O? O: *X O/ U! U' U> U: Y' TH ss
 a! a' a> a? a: aa ae c, e! e' e> e: i! i' i> i:
 d- n? o! o' o> o? o: -: o/ u! u' u> u: y' th y:

 &charset iso-ir-205
 &rem source: ECMA registry
 &g1esc x2d64 &g2esc x2e64 &g3esc x2f64
 &bits 8
 &IRnum 205
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 PA HO BH NH IN NL SA ES HS HJ VS PD PU RI S2 S3
 DC P1 P2 TS CC MW SG EG SS GC SC CI ST OC PM AC
 NS A; kk R, EU I? L, SE ': S< E- G, T/ -- Z< 'm
 DG a; '; r, '' i? l, '< ', s< e- g, t/ NG z< ng
 A- A' A> A? A: AA AE I; C< E' E; E: E. I' I> I-
 D/ N, O- K, O> O? O: *X O/ U; U' U> U: U? U- ss
 a- a' a> a? a: aa ae i; c< e' e; e: e. i' i> i-
 d/ n, o- k, o> o? o: -: o/ u; u' u> u: u? u- '.

 &charset sami
 &rem source: ECMA registry
 &g2esc x2d58 &g2esc x2e58 &g3esc x2f58
 &alias latin-lap
 &alias lap
 &alias iso-ir-158
 &IRnum 158
 &bits 8
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 PA HO BH NH IN NL SA ES HS HJ VS PD PU RI S2 S3
 DC P1 P2 TS CC MW SG EG SS GC SC CI ST OC PM AC
 '' ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ;S ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 A( A! A1 A7 A3 E( E! G/ G< K< O( O! O; O1 ED EZ
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 a( a! a1 a7 a3 e( e! g/ g< k< o( o! o; o1 ed ez
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??

 &charset JIS_X0212-1990
 &rem source: ECMA registry
 &alias x0212
 &alias iso-ir-159
 &bits 14
 &g0esc x242844 &g1esc x242944 &g2esc x242a44 &g3esc x242b44
 &IRnum 159
 &code2 2 15
 '( '< ', '. '" '- '; '0 '?
 '' '%
 &code2 2 34
 !I BB ?I
 &code2 2 75
 -o -a Co Rg TM Cu N0
 &code2 6 65
 A% E% Y% I% J* ?? O% ?? U% V* ?? W%
 &code2 6 81
 a% e% y% i% j* i3 o% *s u% v* u3 w%
 &code2 7 34
 D% G% IE DS II YI J% LJ NJ Ts KJ V% DZ
 &code2 7 82
 d% g% ie ds ii yi j% lj nj ts kj v% dz
 &code2 9 1
 AE D/ ?? H/ ?? IJ ?? L/ L. ?? NG O/ OE ?? T/ TH
 &code2 9 33
 ae d/ d- h/ i. ij kk l/ l. 'n ng o/ oe ss t/ th
 &code2 10 1
 A' A! A: A> A( A< A- A; AA A? C' C> C< C, C. D< E' E! E: E> E( E. E-
 E; ?? G> G( G, G. H> I' I! I: I> I< I. I- I; I? J> K, L' L< L, N' N< N,
 N? O' O! O: O> O< O" O- O? R' R< R, S' S> S< S, T< T, U' U! U: U> U( U<
 U" U- U; U0 U? U:' U:! U:< U:- W. Y' Y: Y> Z' Z< Z.
 &code2 11 1
 a' a! a: a> a( a< a- a; aa a? c' c> c< c, c. d< e' e! e: e> e( e. e-
 e; g' g> g( ?? g. h> i' i! i: i> i< ?? i- i; i? j> k, l' l< l, n' n< n,
 n? o' o! o: o> o< o" o- o? r' r< r, s' s> s< s, t< t, u' u! u: u> u( u<
 u" u- u; u0 u? u:' u:! u:< u:- w. y' y: y> z' z< z.
 &codex J 16 76 1 94
 &codex J 77 77 1 67

 &charset baltic
 &rem source: ECMA registry
 &rem &g1esc x2d56 &g2esc x2e56 &g3esc x2f56
 &alias iso-ir-179
 &bits 8
 &IRnum 179
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 PA HO BH NH IN NL SA ES HS HJ VS PD PU RI S2 S3
 DC P1 P2 TS CC MW SG EG SS GC SC CI ST OC PM AC
 NS "9 Ct Pd Cu Ye BB SE O/ Co :9 << NO -- Rg AE
 DG +- 2S 3S '' My PI .M o/ 1S "6 >> 14 12 34 ae
 I; E. A- C' A: AA A; C< G, E' Z< E; E- K, I- L,
 L/ N, N' O' O- O? O: *X U; S< S' U- U: Z. Z' ss
 i; e. a- c' a: aa a; c< g, e' z< e; e- k, i- l,
 l/ n, n' o' o- o? o: -: u; s< s' u- u: z. z' kk

 &charset DS_2089
 &rem source: Danish Standard, DS 2089, February 1974
 &alias DS2089
 &alias ISO646-DK
 &alias dk
 &bits 7
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z AE O/ AA '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z ae o/ aa '? DT

 &charset us-dk
 &rem for compatibility with ASCII
 &bits 7
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 &duplicate 91 AE
 &duplicate 92 O/
 &duplicate 93 AA
 &duplicate 123 ae
 &duplicate 124 o/
 &duplicate 125 aa
 &duplicate 91 A:
 &duplicate 92 O:
 &duplicate 123 a:
 &duplicate 124 o:

 &charset dk-us
 &bits 7
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z AE O/ AA '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z ae o/ aa '? DT
 &duplicate 91 <(
 &duplicate 92 //
 &duplicate 93 )>
 &duplicate 123 (!
 &duplicate 124 !!
 &duplicate 125 !)
 &duplicate 91 A:
 &duplicate 92 O:
 &duplicate 123 a:
 &duplicate 124 o:

 &charset JIS_X0201
 &alias X0201
 &bits 8
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( Ye )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '- DT
 PA HO BH NH IN NL SA ES HS HJ VS PD PU RI S2 S3
 DC P1 P2 TS CC MW SG EG SS GC SC CI ST OC PM AC
 ?? ._ <' >' ,_ .6 Wo a6 i6 u6 e6 o6 YA YU YO TU
 -6 A6 I6 U6 E6 O6 Ka Ki Ku Ke Ko Sa Si Su Se So
 Ta Ti Tu Te To Na Ni Nu Ne No Ha Hi Hu He Ho Ma
 Mi Mu Me Mo Ya Yu Yo Ra Ri Ru Re Ro Wa N6 "5 05
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??

 &charset KSC5636
 &alias ISO646-KR
 &bits 7
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( W= )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT

 &charset DEC-MCS
 &rem VAX/VMS User's Manual, Order Number: AI-Y517A-TE, April 1986.
 &alias dec
 &bits 8
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 PA HO BH NH IN NL SA ES HS HJ VS PD PU RI S2 S3
 DC P1 P2 TS CC MW SG EG SS GC SC CI ST OC PM AC
 ?? !I Ct Pd EU Ye ?? SE Cu Co -a << ?? ?? ?? ??
 DG +- 2S 3S ?? My PI .M ?? 1S -o >> 14 12 ?? ?I
 A! A' A> A? A: AA AE C, E! E' E> E: I! I' I> I:
 ?? N? O! O' O> O? O: OE O/ U! U' U> U: Y: ?? ss
 a! a' a> a? a: aa ae c, e! e' e> e: i! i' i> i:
 ?? n? o! o' o> o? o: oe o/ u! u' u> u: y: ?? ??

 &charset hp-roman8
 &rem source: LaserJet IIP Printer User's Manual,
 &rem HP part no 33471-90901, Hewlet-Packard, June 1989.
 &bits 8
 &alias roman8
 &alias r8
 &alias x-roman8
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 PA HO BH NH IN NL SA ES HS HJ VS PD PU RI S2 S3
 DC P1 P2 TS CC MW SG EG SS GC SC CI ST OC PM AC
! *** Replace 1!, 1? etc. with proper accent symbols
 NS A! A> E! E> E: I> I: '' '! '> ': '? U! U> Li
 'm Y' y' DG C, c, N? n? !I ?I Cu Pd Ye SE f2 Ct
 a> e> o> u> a' e' o' u' a! e! o! u! a: e: o: u:
 AA i> O/ AE aa i' o/ ae A: i! O: U: E' i: ss O>
 A' A? a? D- d- I' I! O' O! O? o? S< s< U' Y: y:
 TH th .M My PI 34 -M 14 12 -a -o << fS >> +- ??

 &charset NeXTSTEP
 &rem source: Peter Svanberg.
 &alias next
 &bits 8
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 NS A! A' A> A? A: AA C, E! E' E> E: I! I' I> I:
 D- N? O! O' O> O? O: U! U' U> U: Y' TH My *X -:
 Co !I Ct Pd /f Ye f2 SE Cu ?? "6 << ?? ?? fi fl
 Rg -N /- /= .M BB PI sb ?? ?? "9 >> .3 %0 NO ?I
! *** Replace 1!, 1? etc. with proper accent symbols
 1S '! '' '> '? 'm '( '. ': 2S '0 ', 3S '" '; '<
 -M +- 14 12 34 a! a' a> a? a: aa c, e! e' e> e:
 i! AE i' -a i> i: d- n? L/ O/ OE -o o! o' o> o?
 o: ae u! u' u> i. u: y' l/ o/ oe ss th y: ?? ??

 &charset macintosh
 &rem source: The Unicode Standard ver 1.0, ISBN 0-201-56788-1, Oct 1991
 &alias mac
 &bits 8
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 A: AA C, E' N? O: U: a' a! a> a: a? aa c, e' e!
 e> e: i' i! i> i: n? o' o! o> o: o? u' u! u> u:
 /- DG Ct Pd SE sb PI ss Rg Co TM '' ': != AE O/
 00 +- =< >= Ye My dP +Z *P p* In -a -o W* ae o/
 ?I !I NO RT f2 ?2 D* << >> .3 NS A! A? Om OE oe
 -N -M "6 "9 '6 '9 -: LZ y: Y: /f Cu <1 >1 fi fl
 /= .M .9 :9 %0 A> E> A' E: E! I' I> I: I! O' O>
 Mc O! U' U> U! i. ?? ?? 'm '( '. '0 ', '" '; '<

 &charset mac-is
 &bits 8
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 A: AA C, E' N? O: U: a' a! a> a: a? aa c, e' e!
 e> e: i' i! i> i: n? o' o! o> o: o? u' u! u> u:
 /- DG Ct Pd SE sb PI ss Rg Co TM '' ': != AE O/
 00 +- =< >= Ye My dP +Z *P p* In -a -o W* ae o/
 ?I !I NO RT f2 ?2 D* << >> .3 NS A! A? O? OE oe
 -M -N "6 "9 '6 '9 -: Db y: Y: /f Cu D/ d/ TH th
 /= .M .9 :9 %0 A> E> A' E: E! I' I> I: I! O' O>
 Mc O! U' U> U! i. ?? ?? 'm '( '. '0 ', '" '; '<

 &charset macintoshps
 &rem source: PostScript encoding vector (macvec) used by Mac System 7 laserprep
 &alias macps
 &bits 8
 &code 0
!macintosh with Rg -> R, '' -> ', NO -> -, ?2 -> ~, NS -> SP,
!               -M -> -, -N -> -, "6 -> ", "9 -> ", '6 -> ', '9 -> ', /f -> /,
!               <1 -> <, >1 -> >, .9 -> ', :9 -> ", 'O -> DG
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 A: AA C, E' N? O: U: a' a! a> a: a? aa c, e' e!
 e> e: i' i! i> i: n? o' o! o> o: o? u' u! u> u:
 /- DG Ct Pd SE Sb PI ss R  Co TM  '  ': != AE O/
 00 +- =< >= Ye My dP +Z *P p* In -a -o W* ae o/
 ?I !I -  RT Fl '? D* << >> .3 SP A! A? O? OE oe
 -  -  "  "  '  '  -: Db y: Y: /  Cu <  >  fi fl
 /= .M '  "  %0 A> E> A' E: E! I' I> I: I! O' O>
 ?? O! U' U> U! i. ?? ?? '- '( '. DG ', '" '; '<

 &charset windowsps
 &rem source: PostScript encoding vector (ANSIvec) used by PC Windows
 &alias winsps
 &bits 8
 &code 0
! *** GRAVE ACCENT incorrectly written as `, should be '!
! *** TILDE incorrectly written as ~, should be '?
 '!  '  '> '?  'm '( '. ': DG ', ': '; '< i. SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP !  "  Nb DO %  &  '  (  )  *  +  ,  -  .  / 
 0  1  2  3  4  5  6  7  8  9  :  ;  <  =  >  ? 
 At A  B  C  D  E  F  G  H  I  J  K  L  M  N  O 
 P  Q  R  S  T  U  V  W  X  Y  Z  <( // )> '> _ 
 '! a  b  c  d  e  f  g  h  i  j  k  l  m  n  o 
 p  q  r  s  t  u  v  w  x  y  z  (! !! !) '? DT
 ?? ?? ?? Fl "  .3 /- /= %0 ?? s< <  OE ?? ?? ??
! *** GRAVE ACCENT written as ` also appeared in following line; duplicate OK?
 i. '!  '  "  "  .M -  -  '? TM '< >  oe ': ', Y:
 SP !I Ct Pd Cu Ye BB SE ': Co -a << NO -  Rg 'm
 DG +- 2S 3S '  My PI .M ', 1S -o >> 14 12 34 ?I
 A! A' A> A? A: AA AE C, E! E' E> E: I! I' I> I:
 D- N? O! O' O> O? O: *X O/ U! U' U> U: Y' TH ss
 a! a' a> a? a: aa ae c, e! e' e> e: i! i' i> i:
 d- n? o! o' o> o? o: -: o/ u! u' u> u: y' th y:

 &charset decwriteps
 &rem source: PostScript encoding vector used by DECwrite
 &bits 8
 &code 0
 ?? ?? -  -  ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? "  "  ?? ?? ?? ?? ?? ?? ?? ??
 SP !  "  Nb DO %  &  '  (  )  *  +  ,  -  .  /
 0  1  2  3  4  5  6  7  8  9  :  ;  <  =  >  ?
 At A  B  C  D  E  F  G  H  I  J  K  L  M  N  O
 P  Q  R  S  T  U  V  W  X  Y  Z  <( // )> '> _
 '! a  b  c  d  e  f  g  h  i  j  k  l  m  n  o
 p  q  r  s  t  u  v  w  x  y  z  (! !! !) '? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 i. '! '' '> '? '- '( '. ': ?? '0 ', ?? '" '; '<
 SP !I Ct Pd Cu Ye BB SE ': Co -a << NO -  Rg '-
 DG +- 2S 3S '' My PI .M ', 1S -o >> 14 12 34 ?I
 A! A' A> A? A: AA AE C, E! E' E> E: I! I' I> I:
 D- N? O! O' O> O? O: *X O/ U! U' U> U: Y' TH ss
 a! a' a> a? a: aa ae c, e! e' e> e: i! i' i> i:
 d- n? o! o' o> o? o: -: o/ u! u' u> u: y' th y:

 &charset IBM037
 &rem source: IBM NLS RM Vol2 SE09-8002-01, March 1990
 &bits 8
 &alias CP037
 &alias ebcdic-cp-us
 &alias ebcdic-cp-ca
 &alias ebcdic-cp-wt
 &alias ebcdic-cp-nl
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP NS a> a: a! a' a? aa c, n? Ct .  <  (  +  !!
 &  e' e> e: e! i' i> i: i! ss !  DO *  )  ;  NO
 -  /  A> A: A! A' A? AA C, N? BB ,  %  _  >  ?
 o/ E' E> E: E! I' I> I: I! '! :  Nb At '  =  "
 O/ a  b  c  d  e  f  g  h  i  << >> d- y' th +-
 DG j  k  l  m  n  o  p  q  r  -a -o ae ', AE Cu
 My '? s  t  u  v  w  x  y  z  !I ?I D- Y' TH Rg
 '> Pd Ye .M Co SE PI 14 12 34 <( )> 'm ': '' *X
 (! A  B  C  D  E  F  G  H  I  -- o> o: o! o' o?
 !) J  K  L  M  N  O  P  Q  R  1S u> u: u! u' y:
 // -: S  T  U  V  W  X  Y  Z  2S O> O: O! O' O?
 0  1  2  3  4  5  6  7  8  9  3S U> U: U! U' AC

 &charset IBM038
 &rem source: IBM 3174 Character Set Ref, GA27-3831-02, March 1990
 &alias EBCDIC-INT
 &bits 8
 &alias CP038
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP ?? ?? ?? ?? ?? ?? ?? ?? ?? <( .  <  (  +  !
 &  ?? ?? ?? ?? ?? ?? ?? ?? ?? )> DO *  )  ;  '>
 -  /  ?? ?? ?? ?? ?? ?? ?? ?? BB ,  %  _  >  ?
 ?? ?? ?? ?? ?? ?? ?? ?? ?? '! :  Nb At '  =  "
 ?? a  b  c  d  e  f  g  h  i  ?? ?? ?? ?? ?? ??
 ?? j  k  l  m  n  o  p  q  r  ?? ?? ?? ?? ?? ??
 ?? '? s  t  u  v  w  x  y  z  ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 (! A  B  C  D  E  F  G  H  I  ?? ?? ?? ?? ?? ??
 !) J  K  L  M  N  O  P  Q  R  ?? ?? ?? ?? ?? ??
 // ?? S  T  U  V  W  X  Y  Z  ?? ?? ?? ?? ?? ??
 0  1  2  3  4  5  6  7  8  9  ?? ?? ?? ?? ?? AC

 &charset IBM256
 &rem source: IBM Registry C-H 3-3220-050
 &alias EBCDIC-INT1
 &bits 8
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP NS a> a: a! a' a? aa c, n? <( .  <  (  +  !
 &  e' e> e: e! i' i> i: i! ss )> DO *  )  ;  '>
 -  /  A> A: A! A' A? AA C, N? BB ,  %  _  >  ?
 o/ E' E> E: E! I' I> I: I! '! :  Nb At '  =  "
 O/ a  b  c  d  e  f  g  h  i  << >> d- y' th +-
 DG j  k  l  m  n  o  p  q  r  -a -o ae ', AE Cu
 My '? s  t  u  v  w  x  y  z  !I ?I D- Y' TH Rg
 Ct Pd Ye Pt f2 SE PI 14 12 34 NO !! '- ': '' =2
 (! A  B  C  D  E  F  G  H  I  -- o> o: o! o' o?
 !) J  K  L  M  N  O  P  Q  R  1S u> u: u! u' y:
 // 1M S  T  U  V  W  X  Y  Z  2S O> O: O! O' O?
 0  1  2  3  4  5  6  7  8  9  3S U> U: U! U' AC

 &charset IBM273
 &rem source: IBM NLS RM Vol2 SE09-8002-01, March 1990
 &alias CP273
 &bits 8
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP NS a> (! a! a' a? aa c, n? A: .  <  (  +  !
 &  e' e> e: e! i' i> i: i! '? U: DO *  )  ;  '>
 -  /  A> <( A! A' A? AA C, N? o: ,  %  _  >  ?
 o/ E' E> E: E! I' I> I: I! '! :  Nb SE '  =  "
 O/ a  b  c  d  e  f  g  h  i  << >> d- y' th +-
 DG j  k  l  m  n  o  p  q  r  -a -o ae ', AE Cu
 My ss s  t  u  v  w  x  y  z  !I ?I D- Y' TH Rg
 Ct Pd Ye .M Co At PI 14 12 34 NO !! '- ': '' *X
 a: A  B  C  D  E  F  G  H  I  -- o> BB o! o' o?
 u: J  K  L  M  N  O  P  Q  R  1S u> !) u! u' y:
 O: -: S  T  U  V  W  X  Y  Z  2S O> // O! O' O?
 0  1  2  3  4  5  6  7  8  9  3S U> )> U! U' AC

 &charset IBM274
 &rem source: IBM 3174 Character Set Ref, GA27-3831-02, March 1990
 &alias EBCDIC-BE
 &alias CP274
 &bits 8
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP ?? ?? ?? ?? ?? ?? ?? ?? ?? <( .  <  (  +  !
 &  ?? ?? ?? ?? ?? ?? ?? ?? ?? )> DO *  )  ;  '>
 -  /  ?? ?? ?? ?? ?? ?? ?? ?? u! ,  %  _  >  ?
 ?? ?? ?? ?? ?? ?? ?? ?? ?? '! :  Nb a! '  =  "
 ?? a  b  c  d  e  f  g  h  i  ?? ?? ?? ?? ?? ??
 ?? j  k  l  m  n  o  p  q  r  ?? ?? ?? ?? ?? ??
 ?? ': s  t  u  v  w  x  y  z  ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 e' A  B  C  D  E  F  G  H  I  ?? ?? ?? ?? ?? ??
 e! J  K  L  M  N  O  P  Q  R  ?? ?? ?? ?? ?? ??
 c, ?? S  T  U  V  W  X  Y  Z  ?? ?? ?? ?? ?? ??
 0  1  2  3  4  5  6  7  8  9  ?? ?? ?? ?? ?? AC

 &charset IBM275
 &rem source: IBM NLS RM Vol2 SE09-8002-01, March 1990
 &alias EBCDIC-BR
 &alias CP275
 &bits 8
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP ?? ?? ?? ?? ?? ?? ?? ?? ?? E' .  <  (  +  !
 &  ?? ?? ?? ?? ?? ?? ?? ?? ?? DO C, *  )  ;  '>
 -  /  ?? ?? ?? ?? ?? ?? ?? ?? c, ,  %  _  >  ?
 ?? ?? ?? ?? ?? ?? ?? ?? ?? a? :  O? A? '  =  "
 ?? a  b  c  d  e  f  g  h  i  ?? ?? ?? ?? ?? ??
 ?? j  k  l  m  n  o  p  q  r  ?? ?? ?? ?? ?? ??
 ?? '? s  t  u  v  w  x  y  z  ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 o? A  B  C  D  E  F  G  H  I  ?? ?? ?? ?? ?? ??
 e' J  K  L  M  N  O  P  Q  R  ?? ?? ?? ?? ?? ??
 // ?? S  T  U  V  W  X  Y  Z  ?? ?? ?? ?? ?? ??
 0  1  2  3  4  5  6  7  8  9  ?? ?? ?? ?? ?? AC

 &charset IBM277
 &rem source: IBM NLS RM Vol2 SE09-8002-01, March 1990
 &alias EBCDIC-CP-DK
 &alias EBCDIC-CP-NO
 &bits 8
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP NS a> a: a! a' a? !) c, n? Nb .  <  (  +  !
 &  e' e> e: e! i' i> i: i! ss Cu AA *  )  ;  '>
 -  /  A> A: A! A' A? DO C, N? o/ ,  %  _  >  ?
 BB E' E> E: E! I' I> I: I! '! :  AE O/ '  =  "
 At a  b  c  d  e  f  g  h  i  << >> d- y' th +-
 DG j  k  l  m  n  o  p  q  r  -a -o (! ', <( )>
 My u: s  t  u  v  w  x  y  z  !I ?I D- Y' TH Rg
 Ct Pd Ye .M Co SE PI 14 12 34 NO !! '- ': '' *X
 ae A  B  C  D  E  F  G  H  I  -- o> o: o! o' o?
 aa J  K  L  M  N  O  P  Q  R  1S u> '? u! u' y:
 // -: S  T  U  V  W  X  Y  Z  2S O> O: O! O' O?
 0  1  2  3  4  5  6  7  8  9  3S U> U: U! U' AC

 &charset IBM278
 &rem source: IBM NLS RM Vol2 SE09-8002-01, March 1990
 &alias CP278
 &bits 8
 &alias ebcdic-cp-fi
 &alias ebcdic-cp-se
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP NS a> (! a! a' a? !) c, n? SE .  <  (  +  !
 &  '! e> e: e! i' i> i: i! ss Cu AA *  )  ;  '>
 -  /  A> Nb A! A' A? DO C, N? o: ,  %  _  >  ?
 o/ E' E> E: E! I' I> I: I! e' :  A: O: '  =  "
 O/ a  b  c  d  e  f  g  h  i  << >> d- y' th +-
 DG j  k  l  m  n  o  p  q  r  -a -o ae ', AE )>
 My u: s  t  u  v  w  x  y  z  !I ?I D- Y' TH Rg
 Ct Pd Ye .M Co <( PI 14 12 34 NO !! '- ': '' *X
 a: A  B  C  D  E  F  G  H  I  -- o> BB o! o' o?
 aa J  K  L  M  N  O  P  Q  R  1S u> '? u! u' y:
 // -: S  T  U  V  W  X  Y  Z  2S O> At O! O' O?
 0  1  2  3  4  5  6  7  8  9  3S U> U: U! U' AC

 &charset IBM280
 &rem source: IBM NLS RM Vol2 SE09-8002-01, March 1990
 &alias CP280
 &alias ebcdic-cp-it
 &bits 8
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP NS a> a: (! a' a? aa // n? DG .  <  (  +  !
 &  )> e> e: !) i' i> i: '? ss e' DO *  )  ;  '>
 -  /  A> A: A! A' A? AA C, N? o! ,  %  _  >  ?
 o/ E' E> E: E! I' I> I: I! u! :  Pd SE '  =  "
 O/ a  b  c  d  e  f  g  h  i  << >> d- y' th +-
 <( j  k  l  m  n  o  p  q  r  -a -o ae ', AE Cu
 My i! s  t  u  v  w  x  y  z  !I ?I D- Y' TH Rg
 Ct Nb Ye .M Co At PI 14 12 34 NO !! '- ': '' *X
 a! A  B  C  D  E  F  G  H  I  -- o> o: BB o' o?
 e! J  K  L  M  N  O  P  Q  R  1S u> u: '! u' y:
 c, -: S  T  U  V  W  X  Y  Z  2S O> O: O! O' O?
 0  1  2  3  4  5  6  7  8  9  3S U> U: U! U' AC

 &charset IBM281
 &rem source: IBM 3174 Character Set Ref, GA27-3831-02, March 1990
 &alias EBCDIC-JP-E
 &bits 8
 &alias CP281
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP ?? ?? ?? ?? ?? ?? ?? ?? ?? Pd .  <  (  +  !!
 &  ?? ?? ?? ?? ?? ?? ?? ?? ?? !  Ye *  )  ;  NO
 -  /  ?? ?? ?? ?? ?? ?? ?? ?? BB ,  %  _  >  ?
 ?? ?? ?? ?? ?? ?? ?? ?? ?? '! :  Nb At '  =  "
 ?? a  b  c  d  e  f  g  h  i  ?? ?? ?? ?? ?? ??
 ?? j  k  l  m  n  o  p  q  r  ?? ?? ?? ?? ?? ??
 ?? '- s  t  u  v  w  x  y  z  ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 (! A  B  C  D  E  F  G  H  I  ?? ?? ?? ?? ?? ??
 !) J  K  L  M  N  O  P  Q  R  ?? ?? ?? ?? ?? ??
 DO ?? S  T  U  V  W  X  Y  Z  ?? ?? ?? ?? ?? ??
 0  1  2  3  4  5  6  7  8  9  ?? ?? ?? ?? ?? AC

 &charset IBM284
 &rem source: IBM NLS RM Vol2 SE09-8002-01, March 1990
 &alias CP284
 &bits 8
 &alias ebcdic-cp-es
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP NS a> a: a! a' a? aa c, BB <( .  <  (  +  !!
 &  e' e> e: e! i' i> i: i! ss )> DO *  )  ;  NO
 -  /  A> A: A! A' A? AA C, Nb n? ,  %  _  >  ?
 o/ E' E> E: E! I' I> I: I! '! :  N? At '  =  "
 O/ a  b  c  d  e  f  g  h  i  << >> d- y' th +-
 DG j  k  l  m  n  o  p  q  r  -a -o ae ', AE Cu
 My ': s  t  u  v  w  x  y  z  !I ?I D- Y' TH Rg
 Ct Pd Ye .M Co SE PI 14 12 34 '> !  '- '? '' *X
 (! A  B  C  D  E  F  G  H  I  -- o> o: o! o' o?
 !) J  K  L  M  N  O  P  Q  R  1S u> u: u! u' y:
 // -: S  T  U  V  W  X  Y  Z  2S O> O: O! O' O?
 0  1  2  3  4  5  6  7  8  9  3S U> U: U! U' AC

 &charset IBM285
 &rem source: IBM NLS RM Vol2 SE09-8002-01, March 1990
 &alias CP285
 &alias ebcdic-cp-gb
 &bits 8
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP NS a> a: a! a' a? aa c, n? DO .  <  (  +  !!
 &  e' e> e: e! i' i> i: i! ss !  Pd *  )  ;  NO
 -  /  A> A: A! A' A? AA C, N? BB ,  %  _  >  ?
 o/ E' E> E: E! I' I> I: I! '! :  Nb At '  =  "
 O/ a  b  c  d  e  f  g  h  i  << >> d- y' th +-
 DG j  k  l  m  n  o  p  q  r  -a -o ae ', AE Cu
 My '- s  t  u  v  w  x  y  z  !I ?I D- Y' TH Rg
 Ct <( Ye .M Co SE PI 14 12 34 '> )> '? ': '' *X
 (! A  B  C  D  E  F  G  H  I  -- o> o: o! o' o?
 !) J  K  L  M  N  O  P  Q  R  1S u> u: u! u' y:
 // -: S  T  U  V  W  X  Y  Z  2S O> O: O! O' O?
 0  1  2  3  4  5  6  7  8  9  3S U> U: U! U' AC

 &charset IBM290
 &rem source: IBM 3174 Character Set Ref, GA27-3831-02, March 1990
 &alias CP290
 &bits 8
 &alias EBCDIC-JP-kana
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP ._ <' >' ,_ .6 Wo a6 i6 u6 Pd .  <  (  +  !!
 &  e6 o6 YA YU YO TU ?? -6 ?? !  Ye *  )  ;  NO
 -  /  ?? ?? ?? ?? ?? ?? ?? ?? BB ,  %  _  >  ?
 ?? ?? ?? ?? ?? ?? ?? ?? ?? '! :  Nb At '  =  "
 ?? A6 I6 U6 E6 O6 Ka Ki Ku Ke Ko ?? Sa Si Su Se
 So Ta Ti Tu Te To Na Ni Nu Ne No ?? ?? Ha Hi Hu
 ?? '- He Ho Ma Mi Mu Me Mo Ya Yu ?? Yo Ra Ri Ru
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? Re Ro Wa N6 "5 05
 ?? A  B  C  D  E  F  G  H  I  ?? ?? ?? ?? ?? ??
 ?? J  K  L  M  N  O  P  Q  R  ?? ?? ?? ?? ?? ??
 DO ?? S  T  U  V  W  X  Y  Z  ?? ?? ?? ?? ?? ??
 0  1  2  3  4  5  6  7  8  9  ?? ?? ?? ?? ?? AC

 &charset IBM297
 &rem source: IBM NLS RM Vol2 SE09-8002-01, March 1990
 &alias CP297
 &bits 8
 &alias ebcdic-cp-fr
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP NS a> a: At a' a? aa // n? DG .  <  (  +  !
 &  (! e> e: !) i' i> i: i! ss SE DO *  )  ;  '>
 -  /  A> A: A! A' A? AA C, N? u! ,  %  _  >  ?
 o/ E' E> E: E! I' I> I: I! My :  Pd a! '  =  "
 O/ a  b  c  d  e  f  g  h  i  << >> d- y' th +-
 <( j  k  l  m  n  o  p  q  r  -a -o ae ', AE Cu
 '! ': s  t  u  v  w  x  y  z  !I ?I D- Y' TH Rg
 Ct Nb Ye .M Co )> PI 14 12 34 NO !! '- '? '' *X
 e' A  B  C  D  E  F  G  H  I  -- o> o: o! o' o?
 e! J  K  L  M  N  O  P  Q  R  1S u> u: BB u' y:
 c, -: S  T  U  V  W  X  Y  Z  2S O> O: O! O' O?
 0  1  2  3  4  5  6  7  8  9  3S U> U: U! U' AC

 &charset IBM420
 &rem source: IBM NLS RM Vol2 SE09-8002-01, March 1990
 &rem IBM NLS RM p 11-11
 &alias CP420
 &bits 8
 &alias ebcdic-cp-ar1
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP  NS  3+  3+; ++  ??  H'  aM  aM. aH  Ct  .   <   (   +   !!
 &   aH. wH  ??  ??  yH  a+  a+. b+  b+, !   DO  *   )   ;   NO
 -   /   tm  t+  t+, tk  tk, g+  g+, hk  BB  ,   %   _   >   ?
 hk, x+  x+, d+  dk  r+  z+  s+  s+, ,+  :   Nb  At  '   =   "
 sn  a   b   c   d   e   f   g   h   i   sn, c+  c+, dd  dd, tj
 zH  j   k   l   m   n   o   p   q   r   e+  e+. e+, e+; i+  i+.
 i+, -:  s   t   u   v   w   x   y   z   i+; f+  f+, q+  q+, k+
 k+, l+  lM- lM. lH- lH. ??  ??  la- la. l+, m+  m+, n+  n+, h+
 ;+  A   B   C   D   E   F   G   H   I   --  h+, ??  h+; ??  w+
 ?+  J   K   L   M   N   O   P   Q   R   j+  j+. y+  y+. y+, 0a
 *X  ??  S   T   U   V   W   X   Y   Z   1a  2a  ??  3a  4a  5a
 0   1   2   3   4   5   6   7   8   9   ??  6a  7a  8a  9a  AC

 &charset IBM423
 &rem source: IBM NLS RM Vol2 SE09-8002-01, March 1990
 &alias CP423
 &bits 8
 &alias ebcdic-cp-gr
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP A* B* G* D* E* Z* Y* H* I* <( .  <  (  +  !
 &  K* L* M* N* C* O* P* R* S* )> DO *  )  ;  '>
 -  /  T* U* F* X* Q* W* ?? ?? ?? ,  %  _  >  ?
 ?? A% E% Y% ?? I% O% U% W% '! :  Pd SE '  =  "
 A: a  b  c  d  e  f  g  h  i  a* b* g* d* e* z*
 O: j  k  l  m  n  o  p  q  r  y* h* i* k* l* m*
 U: ': s  t  u  v  w  x  y  z  n* c* o* p* r* *s
 ?? a% e% y% j* i% o% u% v* w% s* t* u* f* x* q*
 ', A  B  C  D  E  F  G  H  I  ?? w* A> a! a: e>
 '' J  K  L  M  N  O  P  Q  R  +- e' e! e: i> i:
 DG ?? S  T  U  V  W  X  Y  Z  12 o: o> u> u! u:
 0  1  2  3  4  5  6  7  8  9  y: c, C, ?? ?? AC

 &charset IBM424
 &rem source: IBM NLS RM Vol2 SE09-8002-01, March 1990
 &alias CP424
 &bits 8
 &alias ebcdic-cp-he
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP A+ B+ G+ D+ H+ W+ Z+ X+ Tj Ct .  <  (  +  !!
 &  J+ K% K+ L+ M% M+ N% N+ S+ !  DO *  )  ;  NO
 -  /  E+ P% P+ Zj ZJ Q+ R+ Sh BB ,  %  _  >  ?
 ?? T+ ?? ?? NS ?? ?? ?? == '! :  Nb At '  =  "
 ?? a  b  c  d  e  f  g  h  i  << >> ?? ?? ?? ??
 DG j  k  l  m  n  o  p  q  r  ?? ?? ?? ', ?? Cu
 My '? s  t  u  v  w  x  y  z  ?? ?? ?? ?? ?? Rg
 '> Pd Ye .M Co SE PI 14 12 34 <( )> '- ': '' *X
 (! A  B  C  D  E  F  G  H  I  -- ?? ?? ?? ?? ??
 !) J  K  L  M  N  O  P  Q  R  1S ?? ?? ?? ?? ??
 // -: S  T  U  V  W  X  Y  Z  2S ?? ?? ?? ?? ??
 0  1  2  3  4  5  6  7  8  9  3S ?? ?? ?? ?? AC

 &charset IBM437
 &rem source: IBM NLS RM Vol2 SE09-8002-01, March 1990
 &alias CP437
 &bits 8
 &alias 437
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 C, u: e' a> a: a! aa c, e> e: e! i: i> i! A: AA
 E' ae AE o> o: o! u> u! y: O: U: Ct Pd Ye Pt f2
 a' i' o' u' n? N? -a -o ?I NI NO 12 14 !I << >>
 .S :S ?S vv vl vL Vl Dl dL VL VV LD UL Ul uL dl
 ur uh dh vr hh vh vR Vr UR DR UH DH VR HH VH uH
 Uh dH Dh Ur uR dR Dr Vh vH ul dr FB LB lB RB TB
 a* ss G* p* S* s* My t* F* H* W* d* 00 f* e* (U
 =3 +- >= =< Iu Il -: ?2 DG .M sb RT nS 2S fS NS

 &charset IBM500
 &rem source: IBM NLS RM Vol2 SE09-8002-01, March 1990
 &alias CP500
 &alias 500
 &alias 500V1
 &alias ebcdic-cp-be
 &alias ebcdic-cp-ch
 &bits 8
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP NS a> a: a! a' a? aa c, n? <( .  <  (  +  !
 &  e' e> e: e! i' i> i: i! ss )> DO *  )  ;  '>
 -  /  A> A: A! A' A? AA C, N? BB ,  %  _  >  ?
 o/ E' E> E: E! I' I> I: I! '! :  Nb At '  =  "
 O/ a  b  c  d  e  f  g  h  i  << >> d- y' th +-
 DG j  k  l  m  n  o  p  q  r  -a -o ae ', AE Cu
 My '? s  t  u  v  w  x  y  z  !I ?I D- Y' TH Rg
 Ct Pd Ye .M Co SE PI 14 12 34 NO !! 'm ': '' *X
 (! A  B  C  D  E  F  G  H  I  -- o> o: o! o' o?
 !) J  K  L  M  N  O  P  Q  R  1S u> u: u! u' y:
 // -: S  T  U  V  W  X  Y  Z  2S O> O: O! O' O?
 0  1  2  3  4  5  6  7  8  9  3S U> U: U! U' AC

 &charset IBM850
 &rem source: IBM NLS RM Vol2 SE09-8002-01, March 1990
 &rem source: UNICODE 1.0
 &alias CP850
 &alias 850
 &bits 8
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 C, u: e' a> a: a! aa c, e> e: e! i: i> i! A: AA
 E' ae AE o> o: o! u> u! y: O: U: o/ Pd O/ *X f2
 a' i' o' u' n? N? -a -o ?I Rg NO 12 14 !I << >>
 .S :S ?S vv vl A' A> A! Co VL VV LD UL Ct Ye dl
 ur uh dh vr hh vh a? A? UR DR UH DH VR HH VH Cu
 d- D- E> E: E! i. I' I> I: ul dr FB LB BB I! TB
 O' ss O> O! o? O? My th TH U' U> U! y' Y' 'm ''
 -- +- =2 34 PI SE -: ', DG ': .M 1S 3S 2S fS NS

 &charset IBM851
 &rem source: IBM NLS RM Vol2 SE09-8002-01, March 1990
 &alias CP851
 &alias 851
 &bits 8
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 C, u: e' a> a: a! A% c, e> e: e! i: i> E% A: Y%
 I% ?? O% o> o: U% u> u! W% O: U: a% Pd e% y% i%
 j* i3 o% u% A* B* G* D* E* Z* Y* 12 H* I* << >>
 .S :S ?S vv vl K* L* N* M* VL VV LD UL C* O* dl
 ur uh dh vr hh vh P* R* UR DR UH DH VR HH VH S*
 T* U* F* X* Q* W* a* b* g* ul dr FB LB d* e* TB
 z* y* h* i* k* l* m* n* c* o* p* r* s* *s t* ''
 -- +- u* f* x* SE q* '; DG ': w* v* u3 w% fS NS

 &charset IBM852
 &rem source: IBM NLS RM Vol2 SE09-8002-01, March 1990
 &alias CP852
 &alias 852
 &bits 8
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 C, u: e' a> a: u0 c' c, l/ e: O" o" i> Z' A: C'
 E' L' l' o> o: L< l< S' s' O: U: T< t< L/ *X c<
 a' i' o' u' A; a; Z< z< E; e; NO z' C< s, << >>
 .S :S ?S vv vl A' A> E< S, VL VV LD UL Z. z. dl
 ur uh dh vr hh vh A( a( UR DR UH DH VR HH VH Cu
 d/ D/ D< E: d< N< I' I> e< ul dr FB LB T, U0 TB
 O' ss O> N' n' n< S< s< R' U' r' U" y' Y' t, ''
 -- '" '; '< '( SE -: ', DG ': '. u" R< r< fS NS

 &charset IBM855
 &rem source: IBM NLS RM Vol2 SE09-8002-01, March 1990
 &alias CP855
 &alias 855
 &bits 8
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 d% D% g% G% io IO ie IE ds DS ii II yi YI j% J%
 lj LJ nj NJ ts TS kj KJ v% V% dz DZ ju JU =' ="
 a= A= b= B= c= C= d= D= e= E= f= F= g= G= << >>
 .S :S ?S vv vl h= H= i= I= VL VV LD UL j= J= dl
 ur uh dh vr hh vh k= K= UR DR UH DH VR HH VH Cu
 l= L= m= M= n= N= o= O= p= ul dr FB LB P= ja TB
 JA r= R= s= S= t= T= u= U= z% Z% v= V= %' %" ''
 -- y= Y= z= Z= s% S% je JE sc Sc c% C% ?? fS NS

 &charset IBM857
 &rem source: IBM NLS RM Vol2 SE09-8002-01, March 1990
 &alias CP857
 &alias 857
 &bits 8
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 C, u: e' a> a: a! aa c, e> e: e! i: i> i. A: AA
 E' ae AE o> o: o! u> u! I. O: U: o/ Pd O/ S, s,
 a' i' o' u' n? N? G( g( ?I Rg NO 12 14 !I << >>
 .S :S ?S vv vl A' A> A! Co VL VV LD UL Ct Ye dl
 ur uh dh vr hh vh a? A? UR DR UH DH VR HH VH Cu
 -o -a E> E: E! ?? I' I> I: ul dr FB LB BB I! TB
 O' ss O> O! o? O? My ?? *X U' U> U! i! y: -M ''
 -- +- ?? 34 PI SE -: '; DG ': '. 1S 3S 2S fS NS

 &charset IBM860
 &rem source: IBM NLS RM Vol2 SE09-8002-01, March 1990
 &alias CP860
 &alias 860
 &bits 8
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 C, u: e' a> a? a! A' c, e> E> e! I> O> i! A? A>
 E' A! E! o> o? o! U' u! I! O? U: Ct Pd U! Pt O!
 a' i' o' u' n? N? -a -o ?I O' NO 12 14 !I << >>
 .S :S ?S vv vl vL Vl Dl dL VL VV LD UL Ul uL dl
 ur uh dh vr hh vh vR Vr UR DR UH DH VR HH VH uH
 Uh dH Dh Ur uR dR Dr Vh vH ul dr FB LB lB RB TB
 a* ss G* p* S* s* My t* F* H* W* d* 00 f* e* (U
 =3 +- >= =< Iu Il -: ?2 DG .M sb RT nS 2S fS NS

 &charset IBM861
 &rem source: IBM NLS RM Vol2 SE09-8002-01, March 1990
 &alias CP861
 &alias 861
 &alias cp-is
 &bits 8
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 C, u: e' a> a: a! aa c, e> e: e! D- d- TH A: AA
 E' ae AE o> o: th u> Y' y' O: U: o/ Pd O/ Pt O!
 a' i' o' u' A' I' O' U' ?I ?? NO 12 14 !I << >>
 .S :S ?S vv vl vL Vl Dl dL VL VV LD UL Ul uL dl
 ur uh dh vr hh vh vR Vr UR DR UH DH VR HH VH uH
 Uh dH Dh Ur uR dR Dr Vh vH ul dr FB LB lB RB TB
 a* ss G* p* S* s* My t* F* H* W* d* 00 f* e* (U
 =3 +- >= =< Iu Il -: ?2 DG .M sb RT nS 2S fS NS

 &charset IBM862
 &rem source: IBM NLS RM Vol2 SE09-8002-01, March 1990
 &alias CP862
 &alias 862
 &bits 8
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 A+ B+ G+ D+ H+ W+ Z+ X+ Tj J+ K% K+ L+ M% M+ N%
 N+ S+ E+ P% P+ Zj ZJ Q+ R+ Sh T+ Ct Pd U! Pt O!
 a' i' o' u' n? N? -a -o ?I ?? NO 12 14 !I << >>
 .S :S ?S vv vl vL Vl Dl dL VL VV LD UL Ul uL dl
 ur uh dh vr hh vh vR Vr UR DR UH DH VR HH VH uH
 Uh dH Dh Ur uR dR Dr Vh vH ul dr FB LB lB RB TB
 a* ss G* p* S* s* My t* F* H* W* d* 00 f* e* (U
 =3 +- >= =< Iu Il -: ?2 DG .M sb RT nS 2S fS NS

 &charset IBM863
 &rem source: IBM Keyboard layouts and code pages, PN 07G4586 June 1991
 &alias CP863
 &alias 863
 &bits 8
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 C, u: e' a> A> a! PI c, e> e: e! i: i> i! A! SE
 E' E! E> o> E: I: u> u! Cu O> U: Ct Pd U! U> f2
 BB '' o' u' ': ', 3S 'm I> NI NO 12 14 34 << >>
 .S :S ?S vv vl vL Vl Dl dL VL VV LD UL Ul uL dl
 ur uh dh vr hh vh vR Vr UR DR UH DH VR HH VH uH
 Uh dH Dh Ur uR dR Dr Vh vH ul dr FB LB lB RB TB
 a* ss G* p* S* s* My t* F* H* W* d* 00 /0 e* (U
 =3 +- >= =< Iu Il -: ?2 Ob .M sb RT nS 2S fS NS

 &charset IBM864
 &rem source: IBM Keyboard layouts and code pages, PN 07G4586 June 1991
 &alias CP864
 &bits 8
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 DG  .M  Ob  RT  :S  hh  vv  vh  vl  dh  vr  uh  dl  dr  ur  ul
 ss  00  o/  +-  12  14  ?2  <<  >>  lH- lH. ??  ??  la- la. a+:
 ??  --  aM. Pd  Cu  aH. ??  ??  a+. b+  t+  tk  ,+  g+  hk  x+
 0a  1a  2a  3a  4a  5a  6a  7a  8a  9a  v+  ;+  s+  sn  c+  ?+
 Ct  H'  aM  aH  wH  e+. yH  a+  b+, tm  t+, tk, g+, hk, x+, d+
 dk  r+  z+  s+, sn, c+, dd, tj  zH  e+, i+, BB  NO  -:  *X  e+
 ++  f+. q+. k+, l+. m+, n+. h+, w+  j+  y+, dd  m+. i+. i+  m+
 3+; 3+  n+  h+  h+; j+. y+. f+  q+  lM- lM. l+  k+  y+  fS  NS

 &charset IBM865
 &rem source: IBM DOS 3.3 Ref (Abridged), 94X9575 (Feb 1987)
 &alias CP865
 &alias 865
 &bits 8
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 C, u: e' a> a: a! aa c, e> e: e! i: i> i! A: AA
 E' ae AE o> o: o! u> u! y: O: U: o/ Pd O/ Pt f2
 a' i' o' u' n? N? -a -o ?I NI NO 12 14 !I << >>
 .S :S ?S vv vl vL Vl Dl dL VL VV LD UL Ul uL dl
 ur uh dh vr hh vh vR Vr UR DR UH DH VR HH VH uH
 Uh dH Dh Ur uR dR Dr Vh vH ul dr FB LB lB RB TB
 a* ss G* p* S* s* My t* F* H* W* d* 00 /0 e* (U
 =3 +- >= =< Iu Il -: ?2 Ob .M sb RT nS 2S fS NS

 &charset IBM868
 &rem source: IBM NLS RM Vol2 SE09-8002-01, March 1990
 &alias CP868
 &alias cp-ar
 &bits 8
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 0a  1a  2a  3a  4a  5a  6a  7a  8a  9a  ,+  ;+  ?+  aM  a+  a+.
 a+: b+  b+, p+  ??  tm  t+  t+, ??  ??  tk  tk, g+  g+, ??  ??
 hk  hk, x+  x+, d+  ??  dk  r+  ??  z+  ??  s+  s+, sn  <<  >>
 sn, c+  .S  :S  ?S  vv  vl  c+, dd  dd, tj  VL  VV  LD  UL  zH
 e+  dl  ur  uh  dh  vr  hh  vh  e+. e+, UR  DR  UH  DH  VR  HH
 VH  e+; i+  i+. i+, i+; f+  f+, q+  q+, k+. ul  dr  FB  TB  k+,
 ??  LB  ??  l+  l+. l+; m+  m+, ??  n+  n+, ??  w+  ??  ??  ??
 ??  H'  --  ??  ??  ??  ??  ??  ??  ??  ??  3+  3+; ??  fS  NS

 &charset IBM869
 &rem source: IBM Keyboard layouts and code pages, PN 07G4586 June 1991
 &alias CP869
 &alias 869
 &alias cp-gr
 &bits 8
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 ?? ?? ?? ?? ?? ?? A% ?? .M NO BB 9' '9 E% -M Y%
 I% J* O% ?? ?? U% V* Co W% 2S 3S a% Pd e% y% i%
 j* i3 o% u% A* B* G* D* E* Z* Y* 12 H* I* << >>
 .S :S ?S vv vl K* L* M* N* VL VV LD UL C* O* dl
 ur uh dh vr hh vh P* R* UR DR UH DH VR HH VH S*
 T* U* F* X* Q* W* a* b* g* ul dr FB LB d* e* TB
 z* y* h* i* k* l* m* n* c* o* p* r* s* *s t* ''
 -- +- u* f* x* SE q* '% DG ': w* v* u3 w% fS NS

 &charset IBM870
 &rem source: IBM NLS RM Vol2 SE09-8002-01, March 1990
 &alias CP870
 &alias ebcdic-cp-roece
 &alias ebcdic-cp-yu
 &bits 8
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP NS ?? a: ?? a' a( c< c, c' <( .  <  (  +  !
 &  e' ?? e: u0 i' ?? l< l' ss )> DO *  )  ;  '>
 -  /  ?? A: '" A' ?? C< C, C' !! ,  %  _  >  ?
 '< E' ?? E: U0 I' ?? L< L' '! :  Nb At '  =  "
 '( a  b  c  d  e  f  g  h  i  s' n< d/ y' r< ??
 DG j  k  l  m  n  o  p  q  r  l/ n' s< ', '; Cu
 a; '? s  t  u  v  w  x  y  z  S' N< D/ Y' R< ??
 .M A; z. ?? Z. SE PI z< z' Z< Z' N' S< ': '' *X
 (! A  B  C  D  E  F  G  H  I  -- o> o: r' o' o"
 !) J  K  L  M  N  O  P  Q  R  E< u" u: t< u' e<
 // -: S  T  U  V  W  X  Y  Z  d< O> O: R' O' O"
 0  1  2  3  4  5  6  7  8  9  D< U" U: T< U' AC

 &charset IBM871
 &rem source: IBM NLS RM Vol2 SE09-8002-01, March 1990
 &alias CP871
 &alias ebcdic-cp-is
 &bits 8
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP NS a> a: a! a' a? aa c, n? th .  <  (  +  !
 &  e' e> e: e! i' i> i: i! ss AE DO *  )  ;  O:
 -  /  A> A: A! A' A? AA C, N? BB ,  %  _  >  ?
 o/ E' E> E: E! I' I> I: I! d- :  Nb D- '  =  "
 O/ a  b  c  d  e  f  g  h  i  << >> '! y' (! +-
 DG j  k  l  m  n  o  p  q  r  -a -o !) ', )> Cu
 My o: s  t  u  v  w  x  y  z  !I ?I At Y' <( Rg
 Ct Pd Ye .M Co SE PI 14 12 34 NO !! 'm ': // *X
 TH A  B  C  D  E  F  G  H  I  -- o> '? o! o' o?
 ae J  K  L  M  N  O  P  Q  R  1S u> u: u! u' y:
 '' -: S  T  U  V  W  X  Y  Z  2S O> '> O! O' O?
 0  1  2  3  4  5  6  7  8  9  3S U> U: U! U' AC

 &charset IBM875
 &rem source: UNICODE 1.0
 &alias CP875
 &alias EBCDIC-Greek
 &bits 8
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP A* B* G* D* E* Z* Y* H* I* <( .  <  (  +  !
 &  K* L* M* N* C* O* P* R* S* )> DO *  )  ;  '>
 -  /  T* U* F* X* Q* W* J* V* ?? ,  %  _  >  ?
 ': A% E% Y% NB I% O% U% W% '! :  Nb At '  =  "
 '% a  b  c  d  e  f  g  h  i  a* b* g* d* e* z*
 DG j  k  l  m  n  o  p  q  r  y* h* i* k* l* m*
 '' '? s  t  u  v  w  x  y  z  n* c* o* p* r* s*
 Pd a% e% y% i3 i% o% u% u3 w% *s t* u* f* x* q*
 (! A  B  C  D  E  F  G  H  I  -- w* j* v* '6 -3
 !) J  K  L  M  N  O  P  Q  R  +- 12 ?? .M '9 BB
 // ?? S  T  U  V  W  X  Y  Z  2S SE ?? ?? << NO
 0  1  2  3  4  5  6  7  8  9  3S Co ?? ?? >> AC

 &charset IBM880
 &rem source: IBM NLS RM Vol2 SE09-8002-01, March 1990
 &alias CP880
 &alias EBCDIC-Cyrillic
 &bits 8
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP ?? d% g% io ?? ds ii yi j% <( .  <  (  +  !
 &  lj nj ts kj ?? dz =" N0 D% )> DO *  )  ;  '>
 -  /  G% IO ?? DS II YI J% LJ BB ,  %  _  >  ?
 NJ Ts KJ ?? ?? DZ ju a= b= ?? :  Nb At '  =  "
 c= a  b  c  d  e  f  g  h  i  d= e= f= g= h= i=
 j= j  k  l  m  n  o  p  q  r  k= l= m= n= o= p=
 ja ?? s  t  u  v  w  x  y  z  r= s= t= u= z% v=
 %' y= z= s% je sc c% =' JU A= B= C= D= E= F= G=
 ?? A  B  C  D  E  F  G  H  I  H= I= J= K= L= M=
 ?? J  K  L  M  N  O  P  Q  R  N= O= P= JA R= S=
 // Cu S  T  U  V  W  X  Y  Z  T= U= Z% V= %" Y=
 0  1  2  3  4  5  6  7  8  9  Z= S% JE Sc C% AC

 &charset IBM891
 &rem source: IBM NLS RM Vol2 SE09-8002-01, March 1990
 &alias CP891
 &bits 8
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??

 &charset IBM903
 &rem source: IBM NLS RM Vol2 SE09-8002-01, March 1990
 &alias CP903
 &bits 8
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??

 &charset IBM904
 &rem source: IBM NLS RM Vol2 SE09-8002-01, March 1990
 &alias CP904
 &alias 904
 &bits 8
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 Ct ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? NO BB ??

 &charset IBM905
 &rem source: IBM 3174 Character Set Ref, GA27-3831-02, March 1990
 &alias CP905
 &alias ebcdic-cp-tr
 &bits 8
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP ?? a> a: a! a' ?? c. (! n? C, .  <  (  +  !
 &  e' e> e: e! i' i> i: i! ss G( I. *  )  ;  '>
 -  /  A> A: A! A' ?? C. <( N? s, ,  %  _  >  ?
 ?? E' E> E: E! I' I> I: I! i. :  O: S, '  =  U:
 '( a  b  c  d  e  f  g  h  i  h/ c> s> u( ?? !!
 DG j  k  l  m  n  o  p  q  r  h> g> j> '; ?? Cu
 My o: s  t  u  v  w  x  y  z  H/ C> S> U( ?? At
 .M Pd z. !) Z. SE )> ?? 12 DO H> G> J> ': '' *X
 c, A  B  C  D  E  F  G  H  I  -- o> '? o! o' g.
 g( J  K  L  M  N  O  P  Q  R  '! u> // u! u' ??
 u: -: S  T  U  V  W  X  Y  Z  2S O> Nb O! O' G.
 0  1  2  3  4  5  6  7  8  9  3S U> "  U! U' AC

 &charset IBM918
 &rem source: IBM NLS RM Vol2 SE09-8002-01, March 1990
 &alias CP918
 &alias ebcdic-cp-ar2
 &bits 8
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP  NS  ,+  ;+  ?+  aH  a+  a+. ??  b+  <(  .   <   (   +   !
 &   b+, p+  ??  tm  t+  t+, ??  ??  tk  )>  DO  *   )   ;   '>
 -   /   tk, g+  g+, ??  ??  hk  hk, x+  '!  ,   %   _   >   ?
 0a  1a  2a  3a  4a  5a  6a  7a  8a  9a  :   Nb  At  '   =   "
 x+, a   b   c   d   e   f   g   h   i   d+  ??  dk  r+  ??  z+
 ??  j   k   l   m   n   o   p   q   r   s+  s+, sn  sn, c+  c+,
 dd  '?  s   t   u   v   w   x   y   z   dd, tj  zH  e+  e+. e+,
 e+; i+  i+. i+, i+; f+  f+, q+  q+, k+  k+, !!  ??  ??  l+  l+.
 (!  A   B   C   D   E   F   G   H   I   --  ??  m+  m+, ??  n+
 !)  J   K   L   M   N   O   P   Q   R   n+, ??  w+  ??  ??  ??
 //  ??  S   T   U   V   W   X   Y   Z   H'  ??  ??  ??  ??  ??
 0   1   2   3   4   5   6   7   8   9   ??  ??  ??  3+  3+; AC

 &charset IBM1004
 &rem source: CEN/TC304 N283, 1994-02-04
 &bits 8
 &alias CP1004
 &alias os2latin1
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
! *** 1> -> '>
 ?? ?? .9 ?? :9 .3 /- /= '> %0 S< <1 OE ?? ?? ??
! *** 1? -> '?
 ?? '6 '9 "6 "9 sb -N -M '? TM s< >1 oe ?? ?? Y:
 NS !I Ct Pd Cu Ye BB SE ': Co -a << NO -- Rg 'm
 DG +- 2S 3S '' My PI .M ', 1S -o >> 14 12 34 ?I
 A! A' A> A? A: AA AE C, E! E' E> E: I! I' I> I:
 D- N? O! O' O> O? O: *X O/ U! U' U> U: Y' TH ss
 a! a' a> a? a: aa ae c, e! e' e> e: i! i' i> i:
 d- n? o! o' o> o? o: -: o/ u! u' u> u: y' th y:

 &charset IBM1026
 &rem source: IBM NLS RM Vol2 SE09-8002-01, March 1990
 &alias CP1026
 &alias 1026
 &bits 8
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP NS a> a: a! a' a? aa (! n? C, .  <  (  +  !
 &  e' e> e: e! i' i> i: i! ss G( I. *  )  ;  '>
 -  /  A> A: A! A' A? AA <( N? s, ,  %  _  >  ?
 o/ E' E> E: E! I' I> I: I! i. :  O: S, '  =  U:
 O/ a  b  c  d  e  f  g  h  i  << >> !) '! BB +-
 DG j  k  l  m  n  o  p  q  r  -a -o ae '; AE Cu
 My o: s  t  u  v  w  x  y  z  !I ?I )> DO At Rg
 Ct Pd Ye .M Co SE PI 14 12 34 NO !! -M ': '' *X
 c, A  B  C  D  E  F  G  H  I  -- o> '? o! o' o?
 g( J  K  L  M  N  O  P  Q  R  1S u> // u! u' y:
 u: -: S  T  U  V  W  X  Y  Z  2S O> Nb O! O' O?
 0  1  2  3  4  5  6  7  8  9  3S U> "  U! U' AC

 &charset IBM1047
 &rem source: IBM Character Data Representation Architecture
 &rem Registry SC09-1391-00 p 150.
 &alias CP1047
 &alias 1047
 &bits 8
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP NS a> a: a! a' a? aa c, n? Ct .  <  (  +  !!
 &  e' e> e: e! i' i> i: i! ss !  DO *  )  ;  '>
 -  /  A> A: A! A' A? AA C, N? BB ,  %  _  >  ?
 o/ E' E> E: E! I' I> I: I! '! :  Nb At '  =  "
 O/ a  b  c  d  e  f  g  h  i  << >> d- y' th +-
 DG j  k  l  m  n  o  p  q  r  -a -o ae ', AE Cu
 My '? s  t  u  v  w  x  y  z  !I ?I D- <( TH Rg
 NO Pd Ye .M Co SE PI 14 12 34 Y' ': 'm )> '' *X
 (! A  B  C  D  E  F  G  H  I  -- o> o: o! o' o?
 !) J  K  L  M  N  O  P  Q  R  1S u> u: u! u' y:
 // -: S  T  U  V  W  X  Y  Z  2S O> O: O! O' O?
 0  1  2  3  4  5  6  7  8  9  3S U> U: U! U' AC

 &charset Windows-1250
 &alias CP1250
! *** Updated to 2.0
 &rem source: UNICODE 2.0
 &bits 8
 &alias ms-ee
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
! *** ?? -> EU
! *** .3 -> ...
 EU ?? .9 ?? :9 ... /- /= ?? %0 S< <1 S' T< Z< Z'
 ?? '6 '9 "6 "9 sb -N -M ?? TM s< >1 s' t< z< z'
 NS '< '( L/ Cu A; BB SE ': Co S, << NO -- Rg Z.
 DG +- '; l/ '' My PI .M ', a; s, >> L< '" l< z.
 R' A' A> A( A: L' C' C, C< E' E; E: E< I' I> D<
 D/ N' N< O' O> O" O: *X R< U0 U' U" U: Y' T, ss
 r' a' a> a( a: l' c' c, c< e' e; e: e< i' i> d<
 d/ n' n< o' o> o" o: -: r< u0 u' u" u: y' t, '.

 &charset Windows-1251
 &alias CP1251
! *** Updated to 2.0
 &rem source: UNICODE 2.0
 &bits 8
 &alias ms-cyrl
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
! *** ?? -> EU
! *** .3 -> ...
 D% G% .9 g% :9 ... /- /= EU %0 LJ <1 NJ KJ Ts DZ
 d% '6 '9 "6 "9 sb -N -M ?? TM lj >1 nj kj ts dz
 NS V% v% J% Cu G3 BB SE IO Co IE << NO -- Rg YI
 DG +- II ii g3 My PI .M io N0 ie >> j% DS ds yi
 A= B= V= G= D= E= Z% Z= I= J= K= L= M= N= O= P=
 R= S= T= U= F= H= C= C% S% Sc =" Y= %" JE JU JA
 a= b= v= g= d= e= z% z= i= j= k= l= m= n= o= p=
 r= s= t= u= f= h= c= c% s% sc =' y= %' je ju ja

 &charset Windows-1252
 &alias CP1252
! *** Updated to 2.0
 &rem source: UNICODE 2.0
 &bits 8
 &alias ms-ansi
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
! *** 1> -> ;>
! *** ?? -> EU
! *** .3 -> ...
! *** ?? -> Z<
 EU ?? .9 f2 :9 ... /- /= ;> %0 S< <1 OE ?? Z< ??
! *** ?? -> z<
 ?? '6 '9 "6 "9 sb -N -M 1? TM s< >1 oe ?? z< Y:
 NS !I Ct Pd Cu Ye BB SE ': Co -a << NO -- Rg 'm
 DG +- 2S 3S '' My PI .M ', 1S -o >> 14 12 34 ?I
 A! A' A> A? A: AA AE C, E! E' E> E: I! I' I> I:
 D- N? O! O' O> O? O: *X O/ U! U' U> U: Y' TH ss
 a! a' a> a? a: aa ae c, e! e' e> e: i! i' i> i:
 d- n? o! o' o> o? o: -: o/ u! u' u> u: y' th y:

 &charset Windows-1253
 &alias CP1253
! *** Updated to 2.0
 &rem source: UNICODE 2.0
 &bits 8
 &alias ms-greek
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
! *** ?? -> EU
! *** .3 -> ...
 EU ?? .9 f2 :9 ... /- /= ?? %0 ?? <1 ?? ?? ?? ??
 ?? '6 '9 "6 "9 sb -N -M ?? TM ?? >1 ?? ?? ?? ??
 NS %% A% Pd Cu Ye BB SE ': Co ?? << NO -- Rg -3
 DG +- 2S 3S '* My PI .M E% Y% I% >> O% 12 U% W%
 i3 A* B* G* D* E* Z* Y* H* I* K* L* M* N* C* O*
 P* R* ?? S* T* U* F* X* Q* W* J* V* a% e% y% i%
 u3 a* b* g* d* e* z* y* h* i* k* l* m* n* c* o*
 p* r* *s s* t* u* f* x* q* w* j* v* o% u% w% ??

 &charset Windows-1254
 &alias CP1254
! *** Updated to 2.0
 &rem source: UNICODE 2.0
 &bits 8
 &alias ms-turk
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
! *** 1> -> ;>
! *** ?? -> EU
 EU ?? .9 f2 :9 .3 /- /= ;> %0 S< <1 OE ?? ?? ??
 ?? '6 '9 "6 "9 sb -N -M 1? TM s< >1 oe ?? ?? Y:
 NS !I Ct Pd Cu Ye BB SE ': Co -a << NO -- Rg 'm
 DG +- 2S 3S '' My PI .M ', 1S -o >> 14 12 34 ?I
 A! A' A> A? A: AA AE C, E! E' E> E: I! I' I> I:
 G( N? O! O' O> O? O: *X O/ U! U' U> U: I. S, ss
! *** e; -> e>
! *** e. -> i!
 a! a' a> a? a: aa ae c, e! e' e> e: i! i' i> i:
 g( n? o! o' o> o? o: -: o/ u! u' u> u: i. s, y:

 &charset Windows-1255
 &alias CP1255
! *** Updated to 2.0
 &rem source: UNICODE 2.0
 &bits 8
 &alias ms-hebr
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
! *** ?? -> EU
! *** .3 -> ...
! *** ?/ -> ;>
 EU ?? .9 f2 :9 ... /- /= ;> %0 ?? <1 ?? ?? ?? ??
 ?? '6 '9 "6 "9 sb -N -M 1? TM ?? >1 ?? ?? ?? ??
! *** ?? -> !I
! *** Cu -> Sq
! *** '- -> 'm
 NS !I Ct Pd Sq Ye BB SE ': Co *X << NO -- Rg 'm
! *** ?? -> ?I
 DG +- 2S 3S '' My PI .M ', 1S -: >> 14 12 34 ?I
! *** Entire row added
 SE+ HS+ HP+ HQ+ HI+ TS+ SG+ PA+ QA+ HO+ ?? QU+ DA+ ME+ MA+ RA+
! *** First nine entries added; last entry =2 deleted
 PS+ SH+ SI+ SO+ WW+ WJ+ JJ+ GE+ GY+ ?? ?? ?? ?? ?? ?? ??
 A+ B+ G+ D+ H+ W+ Z+ X+ Tj J+ K% K+ L+ M% M+ N%
 N+ S+ E+ P% P+ Zj ZJ Q+ R+ Sh T+ ?? ?? LR RL ??

 &charset Windows-1256
 &alias CP1256
! *** Almost completely redone for 2.0
 &rem source: UNICODE 2.0
 &bits 8
 &alias ms-arab
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . /
 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O
 P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o
 p q r s t u v w x y z (! !! !) '? DT
 EU p+ .9 f2 :9 ... /- /= ;> %0 tt+ <1 OE tc zj dd+
 gf '6 '9 "6 "9 sb -N -M kh+ TM rr+ >1 oe 0NJ 0J ng+
 NS ,+ Ct Pd Cu Ye BB SE ': Co hd+ << NO -- Rg 'm
 DG +- 2S 3S '' My PI .M ', 1S ;+ >> 14 12 34 ?+
 hg+ H' aM aH wH ah yH a+ b+ tm t+ tk g+ hk x+ d+
 dk r+ z+ s+ sn c+ dd *X tj zH e+ i+ ++ f+ q+ k+
 a! l+ a> m+ n+ h+ w+ c, e! e' e> e: j+ y+ i> i:
 :+ "+ =+ /+ o> '+ 1+ -: 3+ u! 0+ u> u: LR RL yb+

 &charset Windows-1257
 &alias CP1257
! *** New source
 &rem source: Unicode 2.0
 &alias WinBaltRim
 &bits 8
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . /
 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O
 P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o
 p q r s t u v w x y z (! !! !) '? DT
! *** ?? -> EU
! *** .3 -> ...
! *** ?? -> ':
! *** ?? -> '<
! *** ?? -> ',
 EU ?? .9 ?? :9 ... /- /= ?? %0 ?? <1 ?? ': '< ',
! *** ?? -> 'm
! *** ?? -> ';
 ?? '6 '9 "6 "9 sb -N -M ?? TM ?? >1 ?? 'm '; ??
 NS ?? Ct Pd Cu ?? BB SE O/ Co R, << NO -- Rg AE
! *** ?? -> ''
 DG +- 2S 3S '' My PI .M o/ 1S r, >> 14 12 34 ae
 A; I; A- C' A: AA E; E- C< E' Z' E. G, K, I- L,
 S< N' N, O' O- O? O: *X U; L/ S' U- U: Z. Z< ss
 a; i; a- c' a: aa e; e- c< e' z' e. g, k, i- l,
! *** ?? -> '.
 s< n' n, o' o- o? o: -: u; l/ s' u- u: z. z< '.

 &charset Windows-1258
 &alias CP1258
 &rem source: Unicode 2.0
 &alias WinViet
 &bits 8
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . /
 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O
 P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o
 p q r s t u v w x y z (! !! !) '? DT
 EU ?? .9 f2 :9 ... /- /= ;> %0 ?? <1 OE ?? ?? ??
 ?? '6 '9 "6 "9 sb -N -M 1? TM ?? >1 oe ?? ?? Y:
 NS !I Ct Pd Cu Ye BB SE ': Co -a << NO -- Rg 'm
 DG +- 2S 3S '' My PI .M ', 1S -o >> 14 12 34 ?I
 A! A' A> A( A: AA AE C, E! E' E> E: "!" I' I> I:
 D/ N? "2" O' O> O9 O: *X O/ U! U' U> U: U9 "?" ss
 a! a' a> a( a: aa ae c, e! e' e> e: "'" i' i> i:
 d/ n? "-." o' o> o9 o: -: o/ u! u' u> u: u9 Dg y:

 &charset EBCDIC-AT-DE
 &rem source: IBM 3270 Char Set Ref Ch 10, GA27-2837-9, April 1987
 &bits 8
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP ?? ?? ?? ?? ?? ?? ?? ?? ?? A: .  <  (  +  !
 &  ?? ?? ?? ?? ?? ?? ?? ?? ?? U: DO *  )  ;  '>
 -  /  ?? ?? ?? ?? ?? ?? ?? ?? o: ,  %  _  >  ?
 ?? ?? ?? ?? ?? ?? ?? ?? ?? '! :  Nb SE '  =  "
 ?? a  b  c  d  e  f  g  h  i  ?? ?? ?? ?? ?? ??
 ?? j  k  l  m  n  o  p  q  r  ?? ?? ?? ?? ?? ??
 ?? ss s  t  u  v  w  x  y  z  ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 a: A  B  C  D  E  F  G  H  I  ?? ?? ?? ?? ?? ??
 u: J  K  L  M  N  O  P  Q  R  ?? ?? ?? ?? ?? ??
 O: ?? S  T  U  V  W  X  Y  Z  ?? ?? ?? ?? ?? ??
 0  1  2  3  4  5  6  7  8  9  ?? ?? ?? ?? ?? AC

 &charset EBCDIC-AT-DE-A
 &rem source: IBM 3270 Char Set Ref Ch 10, GA27-2837-9, April 1987
 &bits 8
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP ?? ?? ?? ?? ?? ?? ?? ?? ?? o: .  <  (  +  !!
 &  ?? ?? ?? ?? ?? ?? ?? ?? ?? u: U: *  )  ;  NO
 -  /  ?? ?? ?? ?? ?? ?? ?? ?? ss ,  %  _  >  ?
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? :  A: O: '  =  a:
 ?? a  b  c  d  e  f  g  h  i  ?? ?? ?? ?? ?? ??
 ?? j  k  l  m  n  o  p  q  r  ?? ?? ?? ?? ?? ??
 ?? ?? s  t  u  v  w  x  y  z  ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? A  B  C  D  E  F  G  H  I  ?? ?? ?? ?? ?? ??
 ?? J  K  L  M  N  O  P  Q  R  ?? ?? ?? ?? ?? ??
 ?? ?? S  T  U  V  W  X  Y  Z  ?? ?? ?? ?? ?? ??
 0  1  2  3  4  5  6  7  8  9  ?? ?? ?? ?? ?? AC

 &charset EBCDIC-CA-FR
 &rem source: IBM 3270 Char Set Ref Ch 10, GA27-2837-9, April 1987
 &bits 8
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP ?? a> ?? ?? ?? ?? ?? c, ?? a! .  <  (  +  !
 &  ?? e> e: ?? ?? i> i: ?? ?? '' DO *  )  ;  '>
 -  /  A> ?? A! ?? ?? ?? C, ?? u! ,  %  _  >  ?
 ?? E' E> E: ?? I> I: ?? ?? '! :  Nb At '  =  "
 ?? a  b  c  d  e  f  g  h  i  ?? ?? ?? ?? ?? ??
 ?? j  k  l  m  n  o  p  q  r  ?? ?? ?? ?? ?? ??
 ?? ': s  t  u  v  w  x  y  z  ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 e' A  B  C  D  E  F  G  H  I  ?? o> ?? ?? ?? ??
 e! J  K  L  M  N  O  P  Q  R  ?? u> u: ?? ?? ??
 ', ?? S  T  U  V  W  X  Y  Z  ?? O> ?? ?? ?? ??
 0  1  2  3  4  5  6  7  8  9  ?? U> U: U! ?? AC

 &charset EBCDIC-DK-NO
 &rem source: IBM 3270 Char Set Ref Ch 10, GA27-2837-9, April 1987
 &bits 8
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP ?? ?? ?? ?? ?? ?? ?? ?? ?? Nb .  <  (  +  !
 &  ?? ?? ?? ?? ?? ?? ?? ?? ?? Cu AA *  )  ;  '>
 -  /  ?? ?? ?? ?? ?? ?? ?? ?? o/ ,  %  _  >  ?
 ?? ?? ?? ?? ?? ?? ?? ?? ?? '! :  AE O/ '  =  "
 ?? a  b  c  d  e  f  g  h  i  ?? ?? ?? ?? ?? ??
 ?? j  k  l  m  n  o  p  q  r  ?? ?? ?? ?? ?? ??
 ?? u: s  t  u  v  w  x  y  z  ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ae A  B  C  D  E  F  G  H  I  ?? ?? ?? ?? ?? ??
 aa J  K  L  M  N  O  P  Q  R  ?? ?? ?? ?? ?? ??
 // ?? S  T  U  V  W  X  Y  Z  ?? ?? ?? ?? ?? ??
 0  1  2  3  4  5  6  7  8  9  ?? ?? ?? ?? ?? AC

 &charset EBCDIC-DK-NO-A
 &rem source: IBM 3270 Char Set Ref Ch 10, GA27-2837-9, April 1987
 &bits 8
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP ?? ?? ?? ?? ?? ?? ?? ?? ?? o/ .  <  (  +  !!
 &  ?? ?? ?? ?? ?? ?? ?? ?? ?? aa AA *  )  ;  NO
 -  /  ?? ?? ?? ?? ?? ?? ?? ?? BB ,  %  _  >  ?
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? :  AE O/ '  =  ae
 ?? a  b  c  d  e  f  g  h  i  ?? ?? ?? ?? ?? ??
 ?? j  k  l  m  n  o  p  q  r  ?? ?? ?? ?? ?? ??
 ?? ?? s  t  u  v  w  x  y  z  ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? A  B  C  D  E  F  G  H  I  ?? ?? ?? ?? ?? ??
 ?? J  K  L  M  N  O  P  Q  R  ?? ?? ?? ?? ?? ??
 ?? ?? S  T  U  V  W  X  Y  Z  ?? ?? ?? ?? ?? ??
 0  1  2  3  4  5  6  7  8  9  ?? ?? ?? ?? ?? AC

 &charset EBCDIC-FI-SE
 &rem source: IBM 3270 Char Set Ref Ch 10, GA27-2837-9, April 1987
 &bits 8
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP ?? ?? ?? ?? ?? ?? ?? ?? ?? SE .  <  (  +  !
 &  ?? ?? ?? ?? ?? ?? ?? ?? ?? Cu AA *  )  ;  '>
 -  /  ?? ?? ?? ?? ?? ?? ?? ?? o: ,  %  _  >  ?
 ?? ?? ?? ?? ?? ?? ?? ?? ?? e' :  A: O: '  =  "
 ?? a  b  c  d  e  f  g  h  i  ?? ?? ?? ?? ?? ??
 ?? j  k  l  m  n  o  p  q  r  ?? ?? ?? ?? ?? ??
 ?? u: s  t  u  v  w  x  y  z  ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 a: A  B  C  D  E  F  G  H  I  ?? ?? ?? ?? ?? ??
 aa J  K  L  M  N  O  P  Q  R  ?? ?? ?? ?? ?? ??
 E' ?? S  T  U  V  W  X  Y  Z  ?? ?? ?? ?? ?? ??
 0  1  2  3  4  5  6  7  8  9  ?? ?? ?? ?? ?? AC

 &charset EBCDIC-FI-SE-A
 &rem source: IBM 3270 Char Set Ref Ch 10, GA27-2837-9, April 1987
 &bits 8
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP ?? ?? ?? ?? ?? ?? ?? ?? ?? o: .  <  (  +  !!
 &  ?? ?? ?? ?? ?? ?? ?? ?? ?? aa AA *  )  ;  NO
 -  /  ?? ?? ?? ?? ?? ?? ?? ?? BB ,  %  _  >  ?
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? :  A: O: '  =  a:
 ?? a  b  c  d  e  f  g  h  i  ?? ?? ?? ?? ?? ??
 ?? j  k  l  m  n  o  p  q  r  ?? ?? ?? ?? ?? ??
 ?? ?? s  t  u  v  w  x  y  z  ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? A  B  C  D  E  F  G  H  I  ?? ?? ?? ?? ?? ??
 ?? J  K  L  M  N  O  P  Q  R  ?? ?? ?? ?? ?? ??
 ?? ?? S  T  U  V  W  X  Y  Z  ?? ?? ?? ?? ?? ??
 0  1  2  3  4  5  6  7  8  9  ?? ?? ?? ?? ?? AC

 &charset EBCDIC-FR
 &rem source: IBM 3270 Char Set Ref Ch 10, GA27-2837-9, April 1987
 &bits 8
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP ?? ?? ?? ?? ?? ?? ?? ?? ?? DG .  <  (  +  !
 &  ?? ?? ?? ?? ?? ?? ?? ?? ?? SE DO *  )  ;  '>
 -  /  ?? ?? ?? ?? ?? ?? ?? ?? u! ,  %  _  >  ?
 ?? ?? ?? ?? ?? ?? ?? ?? ?? '! :  Pd a! '  =  "
 ?? a  b  c  d  e  f  g  h  i  ?? ?? ?? ?? ?? ??
 ?? j  k  l  m  n  o  p  q  r  ?? ?? ?? ?? ?? ??
 ?? ': s  t  u  v  w  x  y  z  ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 e' A  B  C  D  E  F  G  H  I  ?? ?? ?? ?? ?? ??
 e! J  K  L  M  N  O  P  Q  R  ?? ?? ?? ?? ?? ??
 c, ?? S  T  U  V  W  X  Y  Z  ?? ?? ?? ?? ?? ??
 0  1  2  3  4  5  6  7  8  9  ?? ?? ?? ?? ?? AC

 &charset EBCDIC-IT
 &rem source: IBM 3270 Char Set Ref Ch 10, GA27-2837-9, April 1987
 &bits 8
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP ?? ?? ?? ?? ?? ?? ?? ?? ?? DG .  <  (  +  !
 &  ?? ?? ?? ?? ?? ?? ?? ?? ?? e' DO *  )  ;  '>
 -  /  ?? ?? ?? ?? ?? ?? ?? ?? o! ,  %  _  >  ?
 ?? ?? ?? ?? ?? ?? ?? ?? ?? u! :  Pd SE '  =  "
 ?? a  b  c  d  e  f  g  h  i  ?? ?? ?? ?? ?? ??
 ?? j  k  l  m  n  o  p  q  r  ?? ?? ?? ?? ?? ??
 ?? i! s  t  u  v  w  x  y  z  ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 a! A  B  C  D  E  F  G  H  I  ?? ?? ?? ?? ?? ??
 e! J  K  L  M  N  O  P  Q  R  ?? ?? ?? ?? ?? ??
 c, ?? S  T  U  V  W  X  Y  Z  ?? ?? ?? ?? ?? ??
 0  1  2  3  4  5  6  7  8  9  ?? ?? ?? ?? ?? AC

 &charset EBCDIC-PT
 &rem source: IBM 3270 Char Set Ref Ch 10, GA27-2837-9, April 1987
 &bits 8
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP ?? ?? ?? ?? ?? ?? ?? ?? ?? <( .  <  (  +  !
 &  ?? ?? ?? ?? ?? ?? ?? ?? ?? )> DO *  )  ;  '>
 -  /  ?? ?? ?? ?? ?? ?? ?? ?? o? ,  %  _  >  ?
 ?? ?? ?? ?? ?? ?? ?? ?? ?? '! :  A? O? '  =  "
 ?? a  b  c  d  e  f  g  h  i  ?? ?? ?? ?? ?? ??
 ?? j  k  l  m  n  o  p  q  r  ?? ?? ?? ?? ?? ??
 ?? c, s  t  u  v  w  x  y  z  ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 a? A  B  C  D  E  F  G  H  I  ?? ?? ?? ?? ?? ??
 '' J  K  L  M  N  O  P  Q  R  ?? ?? ?? ?? ?? ??
 C, ?? S  T  U  V  W  X  Y  Z  ?? ?? ?? ?? ?? ??
 0  1  2  3  4  5  6  7  8  9  ?? ?? ?? ?? ?? AC

 &charset EBCDIC-ES
 &rem source: IBM 3270 Char Set Ref Ch 10, GA27-2837-9, April 1987
 &bits 8
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP ?? ?? ?? ?? ?? ?? ?? ?? ?? Ct .  <  (  +  !!
 &  ?? ?? ?? ?? ?? ?? ?? ?? ?? !  Pt *  )  ;  NO
 -  /  ?? ?? ?? ?? ?? ?? ?? ?? n? ,  %  _  >  ?
 ?? ?? ?? ?? ?? ?? ?? ?? ?? '! :  N? At '  =  "
 ?? a  b  c  d  e  f  g  h  i  ?? ?? ?? ?? ?? ??
 ?? j  k  l  m  n  o  p  q  r  ?? ?? ?? ?? ?? ??
 ?? ': s  t  u  v  w  x  y  z  ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 (! A  B  C  D  E  F  G  H  I  ?? ?? ?? ?? ?? ??
 !) J  K  L  M  N  O  P  Q  R  ?? ?? ?? ?? ?? ??
 // ?? S  T  U  V  W  X  Y  Z  ?? ?? ?? ?? ?? ??
 0  1  2  3  4  5  6  7  8  9  ?? ?? ?? ?? ?? AC

 &charset EBCDIC-ES-A
 &rem source: IBM 3270 Char Set Ref Ch 10, GA27-2837-9, April 1987
 &bits 8
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP ?? ?? ?? ?? ?? ?? ?? ?? ?? Ct .  <  (  +  !!
 &  ?? ?? ?? ?? ?? ?? ?? ?? ?? !  Pt *  )  ;  NO
 -  /  ?? ?? ?? ?? ?? ?? ?? ?? BB ,  %  _  >  ?
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? :  N? At '  =  n?
 ?? a  b  c  d  e  f  g  h  i  ?? ?? ?? ?? ?? ??
 ?? j  k  l  m  n  o  p  q  r  ?? ?? ?? ?? ?? ??
 ?? ?? s  t  u  v  w  x  y  z  ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? A  B  C  D  E  F  G  H  I  ?? ?? ?? ?? ?? ??
 ?? J  K  L  M  N  O  P  Q  R  ?? ?? ?? ?? ?? ??
 ?? ?? S  T  U  V  W  X  Y  Z  ?? ?? ?? ?? ?? ??
 0  1  2  3  4  5  6  7  8  9  ?? ?? ?? ?? ?? AC

 &charset EBCDIC-ES-S
 &rem source: IBM 3270 Char Set Ref Ch 10, GA27-2837-9, April 1987
 &bits 8
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP ?? ?? ?? ?? ?? ?? ?? ?? ?? Ct .  <  (  +  !!
 &  ?? ?? ?? ?? ?? ?? ?? ?? ?? !  DO *  )  ;  NO
 -  /  ?? ?? ?? ?? ?? ?? ?? ?? n? ,  %  _  >  ?
 ?? ?? ?? ?? ?? ?? ?? ?? ?? '! :  N? At '  =  "
 ?? a  b  c  d  e  f  g  h  i  ?? ?? ?? ?? ?? ??
 ?? j  k  l  m  n  o  p  q  r  ?? ?? ?? ?? ?? ??
 ?? ': s  t  u  v  w  x  y  z  ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 (! A  B  C  D  E  F  G  H  I  ?? ?? ?? ?? ?? ??
 !) J  K  L  M  N  O  P  Q  R  ?? ?? ?? ?? ?? ??
 // ?? S  T  U  V  W  X  Y  Z  ?? ?? ?? ?? ?? ??
 0  1  2  3  4  5  6  7  8  9  ?? ?? ?? ?? ?? AC

 &charset EBCDIC-UK
 &rem source: IBM 3270 Char Set Ref Ch 10, GA27-2837-9, April 1987
 &bits 8
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP ?? ?? ?? ?? ?? ?? ?? ?? ?? DO .  <  (  +  !!
 &  ?? ?? ?? ?? ?? ?? ?? ?? ?? !  Pd *  )  ;  NO
 -  /  ?? ?? ?? ?? ?? ?? ?? ?? BB ,  %  _  >  ?
 ?? ?? ?? ?? ?? ?? ?? ?? ?? '! :  Nb At '  =  "
 ?? a  b  c  d  e  f  g  h  i  ?? ?? ?? ?? ?? ??
 ?? j  k  l  m  n  o  p  q  r  ?? ?? ?? ?? ?? ??
 ?? '- s  t  u  v  w  x  y  z  ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 (! A  B  C  D  E  F  G  H  I  ?? ?? ?? ?? ?? ??
 !) J  K  L  M  N  O  P  Q  R  ?? ?? ?? ?? ?? ??
 // ?? S  T  U  V  W  X  Y  Z  ?? ?? ?? ?? ?? ??
 0  1  2  3  4  5  6  7  8  9  ?? ?? ?? ?? ?? AC

 &charset EBCDIC-US
 &rem source: IBM 3270 Char Set Ref Ch 10, GA27-2837-9, April 1987
 &bits 8
 &code 0
 NU SH SX EX ST HT SA DT EG RI S2 VT FF CR SO SI
 DL D1 D2 D3 OC NL BS ES CN EM P2 S3 FS GS RS US
 PA HO BH NH IN LF EB EC HS HJ VS PD PU EQ AK BL
 DC P1 SY TS CC MW SG ET SS GC SC CI D4 NK PM SB
 SP ?? ?? ?? ?? ?? ?? ?? ?? ?? Ct .  <  (  +  !!
 &  ?? ?? ?? ?? ?? ?? ?? ?? ?? !  DO *  )  ;  NO
 -  /  ?? ?? ?? ?? ?? ?? ?? ?? BB ,  %  _  >  ?
 ?? ?? ?? ?? ?? ?? ?? ?? ?? '! :  Nb At '  =  "
 ?? a  b  c  d  e  f  g  h  i  ?? ?? ?? ?? ?? ??
 ?? j  k  l  m  n  o  p  q  r  ?? ?? ?? ?? ?? ??
 ?? '? s  t  u  v  w  x  y  z  ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 (! A  B  C  D  E  F  G  H  I  ?? ?? ?? ?? ?? ??
 !) J  K  L  M  N  O  P  Q  R  ?? ?? ?? ?? ?? ??
 // ?? S  T  U  V  W  X  Y  Z  ?? ?? ?? ?? ?? ??
 0  1  2  3  4  5  6  7  8  9  ?? ?? ?? ?? ?? AC

 &charset EBCDIC-IS-FRISS
 &rem source: Skyrsuvelar Rikisins og Reykjavikurborgar, feb 1982
 &alias friss
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 SP ?? ?? ?? ?? a' ?? ?? ?? ?? <  .  A' (  +  !
 D- e' ?? ?? ?? i' ?? ?? ?? DO %  E' *  )  ;  &
 -  /  ?? ?? ?? ?? ?? ?? ?? Nb '6 ,  TH _  >  ?
 ?? ?? ?? ?? ?? I' ?? ?? !! d- :  AE O: '  =  "
 ?? a  b  c  d  e  f  g  h  i  ?? ?? ?? Y' ?? ??
 ?? j  k  l  m  n  o  p  q  r  ?? ?? ?? ?? ?? ??
 DG o: s  t  u  v  w  x  y  z  ?? ?? <( y' ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? )> ': ?? ??
 th A  B  C  D  E  F  G  H  I  ?? ?? ?? ?? o' ??
 ae J  K  L  M  N  O  P  Q  R  ?? ?? ?? ?? u' ??
 '' ?? S  T  U  V  W  X  Y  Z  ?? ?? ?? ?? O' ??
 0  1  2  3  4  5  6  7  8  9  ?? ?? ?? ?? U' DT

 &charset KOI-8
 &rem source: Andrey A. Chernov <ache@astral.msk.su>
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ju a= b= c= d= e= f= g= h= i= j= k= l= m= n= o=
 p= ja r= s= t= u= z% v= %' y= z= s% je sc c% ='
 JU A= B= C= D= E= F= G= H= I= J= K= L= M= N= O=
 P= JA R= S= T= U= Z% V= %" Y= Z= S% JE Sc C% ??

 &charset KOI8-R
 &rem source: RFC1489 via Gabor Kiss <kissg@sztaki.hu>
 &rem and Andrey A. Chernov <ache@astral.msk.su>
 &bits 8
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 hh vv dr dl ur ul vr vl dh uh vh TB LB FB lB RB
 .S :S ?S Iu fS sb RT ?2 =< >= NS Il DG 2S .M -:
 HH VV dR io Dr DR dL Dl LD uR Ur UR uL Ul UL vR
 Vr VR vL IO Vl VL dH Dh DH uH Uh UH vH Vh VH Co
 ju a= b= c= d= e= f= g= h= i= j= k= l= m= n= o=
 p= ja r= s= t= u= z% v= %' y= z= s% je sc c% ='
 JU A= B= C= D= E= F= G= H= I= J= K= L= M= N= O=
 P= JA R= S= T= U= Z% V= %" Y= Z= S% JE Sc C% ="

 &charset KOI8-U
 &rem source: RFC 2319
 &rem source: http://www.net.ua/KOI8-U/
 &MIBenum 2088
 &bits 8
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 hh vv dr dl ur ul vr vl dh uh vh TB LB FB lB RB
! Sb is math bullet; corrected to sb
 .S :S ?S Iu fS sb RT ?2 =< >= NS Il DG 2S .M -:
 HH VV dR io ie DR ii yi LD uR Ur UR uL g3 UL vR
 Vr VR vL IO IE VL II YI DH uH Uh UH vH G3 VH Co
 ju a= b= c= d= e= f= g= h= i= j= k= l= m= n= o=
 p= ja r= s= t= u= z% v= %' y= z= s% je sc c% ='
 JU A= B= C= D= E= F= G= H= I= J= K= L= M= N= O=
 P= JA R= S= T= U= Z% V= %" Y= Z= S% JE Sc C% ="

 &charset CWI
 &rem source: Computerworld Sza'mita'stechnika vol 3 issue 13 1988-06-29
 &alias CWI-2
 &alias cp-hu
 &bits 8
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 C, u: e' a> a: a! aa c, e> e: e! i: i> I' A: A'
 E' ae AE o" o: O' u" U' U" O: U: Ct Pd Ye Pt Fl
 a' i' o' u' n? N? -a O" ?I NI NO 12 14 !I << >>
 .S :S ?S vv vl vL Vl Dl dL VL VV LD UL Ul uL dl
 ur uh dh vr hh vh vR Vr UR DR UH DH VR HH VH uH
 Uh dH Dh Ur uR dR Dr Vh vH ul dr FB LB lB RB TB
 a* b* G* p* S* s* m* t* F* H* W* d* 00 /0 e* (U
 =3 +- >= =< Iu Il -: ?2 Ob .M sb RT nS 2S fS NS
  
! ***  These special character sets are used to handle Kanji conversions.
! ***  Each of these conversions is provided by a special conversion routine
! ***  or routines. General conversions are not possible here.

 &charset dec-kanji
 &rem This name corresponds to the DEC "high bit set" Kanji.
 &rem This is basically a simplified form of the euc-jp encoding. It is NOT
 &rem equivalent to shift-jis!
 &alias dec_kanji
 &alias kanji-dec
 &alias kanji_dec
 &special 1
 &ascii_equiv
 __

 &charset iso-2022-jp
 &rem This name corresponds to the JIS Kanji; that is, ISO 2022 encoded Kanji
 &alias iso-2022-jis
 &alias iso-2022-japanese
 &alias jis-kanji
 &alias jis_kanji
 &alias kanji-jis
 &alias kanji_jis
 &special 2
 __

 &charset KS_C_5601-1987
 &rem source: ECMA registry
 &rem This name corresponds to the "high bit set" KSC 5601-1987
 &alias iso-ir-149
 &alias KS_C_5601-1989
 &alias KSC_5601
 &alias korean
 &alias euc-kr
 &alias wansung
 &alias dec-hangul
 &alias dec_hangul
 &alias hangul-dec
 &alias hangul_dec
 &IRnum 149
 &bits 14
 &g0esc x242843 &g1esc x242943 &g2esc x242a43 &g3esc x242b43
 &special 3
 &ascii_equiv
 __

 &charset iso-2022-kr
 &rem This name corresponds to ISO 2022 encoded KSC 5601-1987
 &alias iso-2022-korean
 &special 4
 __

 &charset utf-8
 &rem Unicode encoded in UTF-8 format (RFC 2279)
 &alias utf8
 &alias utf-8-2.0
 &special 5
 &ascii_equiv
 __

 &charset utf-16-be
 &rem Unicode encoded in UTF-16-BE format (RFC 2781)
 &alias utf16-be
 &special 11
 __

 &charset utf-7
 &rem Unicode encoded in UTF-7 format
 &alias utf7
 &special 8
 __

 &charset utf-7-imap
 &rem Unicode encoded in the IMAP-specific UTF-7 variant
 &alias utf7-imap
 &special 17
 __

 &charset iso-2022
 &rem Generic ISO-2022 encoded text
 &alias iso-2022-generic
 &special 9
 __

 &charset teletex
 &rem Teletex encoded text (restricted iso-2022 output)
 &alias iso-2022-teletex
 &special 10
 __

 &charset euc-jp
 &rem Extended UNIX code Japanese
 &alias euc_jp
 &special 7

 &charset shift-jis
 &rem Yet another Japanese encoding
 &alias shift_jis
 &special 6

 &charset iso-2022-cn
 &rem This name corresponds to ISO 2022 encoded GB2312/CNS11643
 &special 12
 __

 &charset cn-big5
 &alias cn-big-5
 &alias big5
 &alias big-5
 &special 13
 __

 &charset euc-tw
 &special 18
 __

 &charset cn-gb
 &alias euc-cn
 &alias gb2312
 &special 14
 __

 &charset iso-2022-jp-2
 &special 15
 __

 &charset iso-2022-cn-2
 &special 16
 __

 &charset gsm-7
 &alias gsm-7-default-alphabet
 &code 0
 At Pd DO Ye e! e' u! i! o! c, LF O/ o/ CR AA aa
 D* _ F* G* L* W* P* Q* S* H* C* GESC AE ae ss E'
 SP ! " Nb Cu % & ' ( ) * + , - . /
 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 !I A B C D E F G H I J K L M N O
 P Q R S T U V W X Y Z A: O: N? U: SE
 ?I a b c d e f g h i j k l m n o
 p q r s t u v w x y z a: o: n? u: a!
 &comb2 GESC LF FF L* '> ( (! ) !) < <( > )> = '? e EU

 &charset T61-LDAP
 &alias T.61-LDAP
 &rem source: Innosoft Nb and DO in 7-bit for LDAP
 &g0esc x2876 &g1esc x2976 &g2esc x2a76 &g3esc x2b76
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 PA HO BH NH IN NL SA ES HS HJ VS PD PU RI S2 S3
 DC P1 P2 TS CC MW SG EG SS GC SC CI ST OC PM AC
 NS !I Ct Pd DO Ye Nb SE Cu ?? ?? << ?? ?? ?? ??
 DG +- 2S 3S *X My PI .M -: ?? ?? >> 14 12 34 ?I
 ?? "! "' "> "? "- "( ". ": ?? "0 ", "_ "" "; "<
 ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 Om AE D- -a H/ ?? IJ L. L/ O/ OE -o TH T/ NG 'n
 kk ae d/ d- h/ i. ij l. l/ o/ oe ss th t/ ng ??
 &comb2 "' SP '' a a' A A' e e' E E' i i' I I' o o' O O' u u' U U'
                 y y' Y Y' c c' C C' l l' L L' n n' N N' r r' R R'
                 s s' S S' z z' Z Z'
 &comb2 "( SP '( a a( A A( g g( G G(                     u u( U U(
 &comb2 "< SP '< c c< C C< d d< D D< e e< E E< l l< L L< n n< N N<
                 r r< R R< s s< S S< t t< T T< z z< Z Z<
 &comb2 ", SP ', c c, C C, g g, G G, k k, K K, l l, L L, n n, N N,
                 r r, R R, s s, S S, t t, T T,
 &comb2 ">       a a> A A> e e> E E> i i> I I> o o> O O> u u> U U>
                 y y> Y Y> c c> C C> g g> G G> h h> H H> j j> J J>
                 s s> S S> w w> W W>
 &comb2 ": SP ': a a: A A: e e: E E: i i: I I: o o: O O: u u: U U:
                 y y: Y Y:
 &comb2 ". SP '. c c. C C. e e. E E. g g. G G.      I I. z z. Z Z.
 &comb2 "" SP '"                               o o" O O" u u" U U"
 &comb2 "!       a a! A A! e e! E E! i i! I I! o o! O O! u u! U U!
 &comb2 "- SP '- a a- A A- e e- E E- i i- I I- o o- O O- u u- U U-
 &comb2 "; SP '; a a; A A; e e; E E; i i; I I; u u; U U;
 &comb2 "0 SP '0 a aa A AA                               u u0 U U0
 &comb2 "?       a a? A A? n n? N N? i i? I I? o o? O O? u u? U U?

 &charset tis-620
 &alias tis620
 &bits 8
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 PA HO BH NH IN NL SA ES HS HJ VS PD PU RI S2 S3
 DC P1 P2 TS CC MW SG EG SS GC SC CI ST OC PM AC
 ?? kokai khai khuat khwai khon rakh ngongu
 chan ching chang soso choe ying chada patak
 than nang phut nonen dodek totao thung thahan
 thong nonu baimai popla phung fofa phan fofan
 samph moma yoyak rorua ruT loling luT wowaen
 sosala sorusi sosua hohip chula oang nokhuk yannoi
 aT hanaka saraaa saraam sarai saraii saraue uee
 sarau sarauu phintu ?? ?? ?? ?? baht
 sarae saraae sarao maimua maimal lakkh maiyam maitai
 maiek maitho maitri chataw hakhat hahit makkan fongma
 0t 1t 2t 3t 4t 5t 6t 7t
 8t 9t hankhu khomut ?? ?? ?? ?? 

 &charset cp874
 &bits 8
 &code 0
 NU SH SX EX ET EQ AK BL BS HT LF VT FF CR SO SI
 DL D1 D2 D3 D4 NK SY EB CN EM SB EC FS GS RS US
 SP ! " Nb DO % & ' ( ) * + , - . / 0 1 2 3 4 5 6 7 8 9 : ; < = > ?
 At A B C D E F G H I J K L M N O P Q R S T U V W X Y Z <( // )> '> _
 '! a b c d e f g h i j k l m n o p q r s t u v w x y z (! !! !) '? DT
 EU ?? ?? ?? ?? ... ?? ?? ?? ?? ?? ?? ?? ?? ?? ??
 ?? '6 '9 "6 "9 sb -N -M ?? ?? ?? ?? ?? ?? ?? ??
 NS kokai khai khuat khwai khon rakh ngongu
 chan ching chang soso choe ying chada patak
 than nang phut nonen dodek totao thung thahan
 thong nonu baimai popla phung fofa phan fofan
 samph moma yoyak rorua ruT loling luT wowaen
 sosala sorusi sosua hohip chula oang nokhuk yannoi
 aT hanaka saraaa saraam sarai saraii saraue uee
 sarau sarauu phintu ?? ?? ?? ?? baht
 sarae saraae sarao maimua maimal lakkh maiyam maitai
 maiek maitho maitri chataw hakhat hahit makkan fongma
 0t 1t 2t 3t 4t 5t 6t 7t
 8t 9t hankhu khomut ?? ?? ?? ?? 
