##

### To Configure Fibre Channel Port Settings

This page displays when you click the FC Configuration button from the Configuration page. After you set the FC port configuration settings, the array will attempt to maintain those settings, but may revert to previous settings.

1. Select the port speed from the Set Speed menu.

You can set the speed to 1 gigabits per second, 2 gigabits per seconds, or auto.

2. Select the Fibre Channel topology for the array.

You can set the topology as follows:

- auto - automatically sense the topology type
- loop - loop
- fabric loop - arbitrated loop
- fabric point-to-point - point to point
- no connection

3. Click Save.