##

### Firewall Port Filtering (Sun StorEdge 6300)

This page enables you to open or close ports to enable or disable access to the Storage Service Processor, system, or the Sun StorEdge Configuration Service software. See To Enable or Disable Port Access (Sun StorEdge 6300).

You can open or close the following ports:

Port | Port Number | Description
--- | --- | ---
Array Management HTTP, non-secure | 9080 | Enables access to the Sun StorEdge Configuration Service Login page or command-line interface sscs. A non-secure connection.
Array Management HTTPS | 9443 | Enables secure access to the Sun StorEdge Configuration Service Login page or command-line interface sscs. This port uses the Secure Socket Layer (SSL) protocol. Log in using this port if you are concerned about password security.
Storage Automated Diagnostic Environment software, non-secure HTTP | 7654 | Enables access to the Storage Automated Diagnostic software. The software is installed by default on the Storage Service processor. You can optionally install the software on a Solaris host if you are using Sun StorEdge 6120 arrays.
Storage Automated Diagnostic Environment software, secure HTTPS | 7443 | Enables access to the Storage Automated Diagnostic software. The software is installed by default on the Storage Service processor. You can optionally install the software on a Solaris host if you are using Sun StorEdge 6120 arrays.
SNMP | 161 | Enables the simple network management protocol port for third-party device management application access.
CIM HTTP | 5988 | Enables the Common Information Model port for CIM- compatible web-based management application access.
NTP | 123 | Enables the system to request the current time from a network time protocol server.
PatchPro | 443 | Enables access to the Sun PatchPro web page to provide updates for firmware and software updates.