##

### To Duplicate Tray Settings to Another Tray

Note - These procedures will duplicate array settings and all associated objects, including pools, volumes, volume groups, initiators, initiator groups, and all premissions.

1. Select the Configuration/Array selection tab.
2. Select an array in the Array Selection table and click Configure.
3. Select Trays from the Sub-reports view drop-down menu.

The trays in the array table displays the tray type, role (Master or Alternate Master), State (Enabled or Disabled), Status, Number of Driver, and Array Hot Spares (AHS - firmware Version 3.1 only). For arrays that are not a controller, the Role, State, and Status Columns shows the dash (-) character.

4. Click Duplicate Tray.

The Duplicate Tray wizard is displayed.

5. Select the following in the wizard:

- The source tray that has the settings to duplicate
- The destination trays

Note - If the destination tray has pools with volumes, you will receive a notification of what will be deleted in order to duplicate the configuration of the source tray.

6. Click Confirm.