sun.com | docs.sun.com | How To Buy | My Sun | Worldwide Sites |  |

| Previous Contents Index Next
#### J Java Dynamic Management Kit, () JMX clients, using to provide cluster statistics, () #### L lights-off management, () log files, () information on `nhpmd` daemon actions, () logical addresses, () logical mirroring, () LOM, () #### M manual installation, hardware requirements, () master-eligible node, () supported hardware types, () master-eligible nodes, logical mirroring, () master-ineligible node, () master node, () access to data by other nodes, () collecting cluster statistics, () failover, () floating address triplet, () diagram of, () diagram of after failover, () example, () floating external addresses, () mirroring, () partitioning, (), () switchover, () membership of the cluster, See Cluster Membership Manager metadevice, () mirroring, () data partition, () logical, () monitoring cluster statistics See Node Management Agent daemons See Daemon Monitor hardware watchdogs, () low level monitoring, (), () statistics See Node Management Agent multicast, transmission of heartbeat, () multicast address, () recommendations for, () multicast heartbeat, () #### N nametags, assigned to daemons, () netmask, in IP address, () network cluster, () external accessing the Foundation Services, () accessing user application services, () connecting to the cluster network, () debugging the cluster, () developing applications, () installing software, () retrieving cluster statistics, () network file system, See Reliable NFS network ID, () network part, of IP address, () network paths, See routes NFS, See Reliable NFS `nfs_client` daemon, () `nhcmmd` daemon, () `nhcrfsd` daemon, () `nhinstall` tool hardware requirements, () unsuitable for dataless nodes, () `nhpmd` daemon, () `nhpmdadm` tool, () `nhprobed` daemon, () `nhwdtd` daemon, () NMA See Node Management Agent `noac`, () node, supported hardware types for master-eligible nodes, () node address triplets, (), () node identity, in IP address, () Node Management Agent APIs, () cascading, () monitoring cluster statistics, () monitoring the direct link, () reporting faults, () running on peer nodes, () running on the master node, () summary of, () Node State Manager, () summary of, () nodes accessing data on the master node, () address triplets, (), () assigning roles, (), () backing up the master node, () cluster membership, () dataless, () accessing data on master node, () unsuitability of `nhinstall` tool, () detecting failures, (), () diskfull, () diskless, () accessing data on master node, () allocating IP addresses, (), (), () booting, (), (), () failure of master, () heartbeats, () master, () floating address triplet, () floating external addresses, () mirroring, () partitioning, (), () master-eligible, () logical mirroring, () master-ineligible, () monitoring See Node Management Agent monitoring heartbeats, () monitoring statistics, () nonpeer, () number in a cluster, () peer, () restarting independently, () shutting down independently, () supported software, () switchover, () types of, () vice-master, () mirroring, () partitioning, (), () nonpeer nodes, () connecting to the cluster network, () notifications changes in cluster membership or mastership, () changes in cluster state, () heartbeats, () listening for, () receiving, () NSM, See Node State Manager
Previous Contents Index Next

Copyright 1994-2004 Sun Microsystems