sun.com | docs.sun.com |  | How To Buy | My Sun | Worldwide Sites |

A B C D E F G H I J K L M N O P Q R S T U V W X Y Z

Maintenance Commands | flconfig(1M)

- NAME
- SYNOPSIS
- DESCRIPTION
- OPTIONS
- ATTRIBUTES
- SEE ALSO

## NAME

> flconfig - SMCT command to add user-defined configuration data to a flash archive

## SYNOPSIS

> `flconfig -n swl-name -v swl-version -g node-group-name -f flash-archive [-e export-dir] [-c config-dir] [-l logfile] [-V verbosity-level] [-h]`

## DESCRIPTION

> Do not use the SMCT tool with the current patch level of the Foundation Services product.

> The `flconfig` command adds user-defined configuration data to a specified flash archive. This command uses data from the export directory to create a configuration section that contains all the user application data and application data installation scripts for the node group specified as a parameter. The configuration section is added to the flash archive for the node group.

> Configuration sections are also created for the diskless node groups embedded in the master-eligible node groups.

> You must be superuser to run the `flconfig` command.

## OPTIONS

> The options that you can use with the `flconfig` command are:

> -n swl-name

>   Name of the software load to process. This is an ASCII string.

> -v swl-version

>   Version of the software load to process. This is an ASCII string.

> -g node-group-name

>   Name of the node group associated to the flash archive. This is an ASCII string defined in the file `cluster.conf`.

> -f flash-archive

>   Absolute path and file name of the flash archive. If only the flash archive name is specified, the flash archive is expected to be located in the default directory `SMCT_FLASH_DIR`, which is defined in the `smct.env` file.

> -e export-dir

>   Directory where the software load data has been copied to by the `slexport` command. The default directory is specified by the SMCT variable `SMCT_EXPORT_DIR`, which is defined in the `smct.env` file. For more information on the `smct.env` file, see the `nhsmctsetup`(1M) man page.

> -c config-dir

>   Directory where the configuration files are located. This option overrides the configuration directory specified by the SMCT variable `SMCT_DEFAULT_CONFIG_DIR`, which is defined in the `smct.env` file. For more information on the `smct.env` file, see the `nhsmctsetup`(1M) man page.

> -l log-file

>   Name of the file that stores information and error messages. By default these messages are displayed on the console.

> -V verbose-level

>   Verbosity level. Values are 1, 2, or 3, where 1 is minimal traces and 3 is detailed information.

> -h

>   Displays help information.

## ATTRIBUTES

> See `attributes`(5) for descriptions of the following attributes:

> ATTRIBUTE TYPE | ATTRIBUTE VALUE
> --- | ---
> Architecture | SPARC
> Availability | SUNWnhsmc
> Interface Stability | Evolving

## SEE ALSO

> `flcreate`(1M), `fldeploy`(1M), `flinstall`(1M), `nhsmctsetup`(1M), `slconfig`(1M), `slcreate`(1M), `sldelete`(1M), `sldeploy`(1M), `slexport`(1M)

Netra HAS FS 2.1 | Go To Top | Last Changed September 2004

Company Info | Contact | Copyright 2004 Sun Microsystems, Inc. All rights reserved. Use is subject to license terms.