sun.com | docs.sun.com | How To Buy | My Sun | Worldwide Sites |  |

| Previous Contents Next
Chapter 10 # L logical address A supplementary address on a physical interface or virtual interface of a node. One physical interface or virtual interface can have many logical addresses. See also physical address and virtual address. logical interface A logical interface configured on a physical interface or virtual interface of a node. A logical interface on an `hme0` or `cgtp0` interface might be called `hme0:1` or `cgtp0:1`.
Previous Contents Next

Copyright 1994-2004 Sun Microsystems