sun.com | docs.sun.com | How To Buy | My Sun | Worldwide Sites |  |

| Previous Contents Index Next
### Four-Node Cluster With Netra T1 Servers Following is an example of a hardware configuration for a four-node cluster: Two Netra T1 servers configured as master-eligible nodes Two Netra T1 servers configured as diskless nodes Two Ethernet switches A terminal server to manage the consoles ### Six-Node Cluster With Netra CT 410 Servers Following is an example of a hardware configuration for a six-node cluster: Two Netra CT 410 CompactPCI servers, each fitted with the following: One Netra CP2140 system controller board configured as a master-eligible node Two Netra CP2160 satellite processor boards configured as diskless nodes One alarm card One 18-Gbyte or larger disk per server Two Ethernet switches A terminal server to manage the consoles (Optional) Supplemental PMC Ethernet cards on each CP2140 board to configure the external network of the master-eligible nodes ### Eight-Node Cluster With Netra CT 810 Servers Following is an example of a hardware configuration for an eight-node: Two Netra CT 810 CompactPCI servers, each fitted with the following: One Netra CP2140 system controller board configured as a master-eligible node Three Netra CP2160 satellite processor boards configured as diskless nodes One alarm card Two 18-Gbyte or larger disks per server Two Ethernet switches A terminal server to manage the consoles (Optional) Supplemental PMC Ethernet cards on each CP2140 board to configure the external network of the master-eligible nodes ### Twelve-Node Cluster With Netra 20 and Netra 120 Servers Following is an example of a hardware configuration for a twelve-node cluster: Two Netra 20 servers configured as master-eligible nodes, each fitted with the following: Two Fibre Channel-Arbitrated Loop (FC-AL) disks The FC-AL disks must be managed by the volume management feature that is provided in the Solaris operating system. For more information about using FC-AL disks, see Types of Disks Quad-Fast Ethernet (QFE) or Hundred-Megabit Ethernet (HME) cards to configure the cluster network connection 10 Netra 120 servers configured as dataless nodes Two Ethernet switches A terminal server to manage the consoles (Optional) Supplemental HME cards or QFE cards for the external network connection
Previous Contents Index Next

Copyright 1994-2004 Sun Microsystems