sun.com | docs.sun.com | How To Buy | My Sun | Worldwide Sites |  |

| Previous Contents Index Next
1. ### To Mount the Installation Server Directories Onto the Prototype Machine and the Cluster As file systems may already be shared, this section provides guidelines only. The minimum requirements for sharing files by using the NFS are as follows: Set the permissions to read and write, `-o rw,anon=0`, for the directory where the flash archives are generated. The default directory for the flash archives is `SMCT_FLASH_DIR`. Set the permissions to read only, `-o ro,anon=0`, for the directory containing the Solaris JumpStart environment. The default directory for the Solaris JumpStart environment is `SMCT_JUMPSTART_DIR`. Set the permissions to read only, `-o ro,anon=0`, for the directory containing the Solaris distribution. The default directory for the Solaris distribution is `SMCT_SOL_DIR`. Set the permissions to read only, `-o ro,anon=0`, for the directory containing the exported software load data. The default directory for the exported software load data is `SMCT_EXPORT_DIR`. Set the permissions to read only, `-o ro,anon=0`, for the software repository. The default directory for the exported software load data is `SMCT_EXPORT_DIR`. If you ran the `slexport` command with the `-r` option, the default directory is `SMCT_SOFTREP_DIR`. Set the permissions read-writer permissions, `-o rw,anon=0`, for the SMCT temporary directory. The default temporary directory is `SMCT_TMP_DIR`. ### To Disable the Installation Server as a Router Disable the installation server as a router by creating a `/etc/notrouter` file:
       # touch /etc/notrouter
1. If a system running the Solaris operating system has two network interfaces, it is configured as a router by default. However, a Foundation Services cluster network must not be routed for security reasons. ### To Reboot the Installation Server to Start the Solaris Daemons Reboot the installation server to start or restart the Solaris daemons:
       # init 6
1. The following daemons are started or are restarted: `rarpd` `rpc.bootparamd` `lockd` `statd` `mountd` `nfsd` `inetd` ## Configuring the Prototype Machine This section describes how to erase a previous DHCP boot configuration on the prototype machine. ### To Set the Boot Device on the Prototype Machine Get the `ok` prompt on the prototype machine. For example:
       telnet> send brk
       ok>
2. Configure the OBP parameters:
       ok> setenv boot-device disk net
## SMCT Configuration File Locations The following files are the SMCT configuration files: `cluster.conf` `machine.conf` `network.conf` `master-system.conf` `install-server.conf` Each SMCT configuration file has a template file in the directory `/opt/SUNWcgha/nhsmct/etc/models`. Make sure that you have copied the template files to a directory of your choice as described in the Netra High Availability Suite Foundation Services 2.1 6/03 Release Notes. The default directory for the cluster configuration files is the smct-config-dir`/models` directory. If the `-c` option is not used when running SMCT commands, the cluster configuration files are expected to be located in this directory. If you copy the templates to a user-defined configuration directory, you must use this directory location with the `-c` option when running the SMCT commands. When you run an SMCT command, the SMCT looks for the configuration files first in the directory specified with the `-c` option if used. If the `-c` option is not used, the SMCT looks for the necessary configuration files in the smct-config-dir. If there are no files in the smct-config-dir, the SMCT looks for the configuration files in the `/opt/SUNWcgha/nhsmct/etc/models/` directory. For information about the configurable elements of these files, see Appendix A, Configuration Element Rules.
Previous Contents Index Next

Copyright 1994-2004 Sun Microsystems