sun.com | docs.sun.com | How To Buy | My Sun | Worldwide Sites |  |

| Previous Contents Next
Chapter 14 # P PCI (Peripheral Component Interconnect) peer node A node that is configured to run the Foundation Services. See also cluster_nodes_table, nonpeer node, and node. physical address The IP address of a physical interface. See also physical interface. physical interface A network interface card (NIC). The name of the interface depends on the type of network card that is used. A node could have network interfaces called `hme0` and `hme1`. PMC (PCI Mezzanine Card) predefined node A node that is defined as part of a cluster but that has not been physically connected to the cluster. A predefined node is a peer node with an out-of-cluster role. See also peer node and out node.
Previous Contents Next

Copyright 1994-2004 Sun Microsystems