sun.com | docs.sun.com | How To Buy | My Sun | Worldwide Sites |  |

| Previous Contents Index Next
2. ### To Configure the DHCP Static Boot Policy Log in to the master node as superuser. Update the DHCP configuration table for the NIC0 interface of the diskless node:
       # dhtadm -A -m macro-name -d \
       ':NhCgtpAddr=local-cgtp-addr:Include=Common:\
       BootFile=inetboot.sun4u.os:\
       SrootPTH=/export/root/diskless-node-name:\
       SswapPTH=/export/swap/diskless-node-name:Include=subnet:'
   macro-name is the NIC0 IP address of the node. local-cgtp-addr is the IP address of the `cgtp0` interface of the node. os is the operating system. Specify `Solaris_8` or `Solaris_9` depending on the Solaris version you installed. diskless-node-name is the name of the node. subnet is the NIC0 subnet. For a diskless node, `netraDISKLESS1`, with the NIC0 IP address `10.250.1.30` and Solaris 9, type:
       # dhtadm -A -m 10.250.1.30 -d \
       ':NhCgtpAddr=10.250.3.30:Include=Common:BootFile=inetboot.sun4u.Solaris_9:\
       SrootPTH=/export/root/netraDISKLESS1:\
       SswapPTH=/export/swap/netraDISKLESS1:Include=10.250.1.0:'
3. Update the DHCP container for the NIC0 interface of the diskless node.
       # pntadm -A IP-address \
       -i Ethernet-address \
       -f PERMANENT+MANUAL -m macro-name subnet
   IP-address is the NIC0 IP address of the node. Ethernet-address of the board of the node. The letters of the address must be in upper-case macro-name is the NIC1 IP address of the node. subnet is the NIC0 subnet. For the diskless node with the NIC0 IP address `10.250.1.30` and Ethernet address `01080020F9B360`, type:
       # pntadm -A 10.250.1.30 -i 01080020F9B360 -f PERMANENT+MANUAL \
       -m 10.250.1.30 10.250.1.0
4. Update the DHCP configuration table for the NIC1 interface of the diskless node:
       # dhtadm -A -m macro-name -d \
       ':NhCgtpAddr=local-cgtp-addr:Include=Common:\
       BootFile=inetboot.sun4u.os:\
       SrootPTH=/export/root/diskless-node-name:\
       SswapPTH=/export/swap/diskless-node-name:Include=subnet:'
   macro-name is the NIC1 IP address of the node. local-cgtp-addr is the IP address of the `cgtp0` interface of the node. os is the operating system. Specify `Solaris_8` or `Solaris_9` depending on the Solaris version you installed. diskless-node-name is the name of the node. subnet is the NIC1 subnet. For the diskless node, `netraDISKLESS1`, with the NIC1 IP address `10.250.2.30` and Solaris 9, type:
       # dhtadm -A -m 10.250.2.30 -d \
       ':NhCgtpAddr=10.250.3.30:Include=Common:BootFile=inetboot.sun4u.Solaris_9:\
       SrootPTH=/export/root/netraDISKLESS1:\
       SswapPTH=/export/swap/netraDISKLESS1:Include=10.250.2.0:'
5. Update the DHCP container for the NIC1 interface of the diskless node:
       # pntadm -A IP-address \
       -i Ethernet-address \
       -f PERMANENT+MANUAL -m macro-name subnet
   IP-address is the NIC1 IP address of the node. Ethernet-address of the board of the node. macro-name is the NIC1 IP address of the node. subnet is the NIC1 subnet. For the diskless node with the NIC1 IP address `10.250.2.30` and Ethernet address `01080020F9B361`, type:
       # pntadm -A 10.250.2.30 -i 01080020F9B361 \
       -f PERMANENT+MANUAL -m 10.250.2.30 10.250.2.0
1. 3. ### To Configure the DHCP Client ID Boot Policy This procedure can only be performed on nodes with CompactPCI technology. For information specific to the hardware you are using, see the corresponding hardware documentation. Create or retrieve the client ID for the diskless node. Log in to the diskless node as superuser. Get the `ok` prompt. Check for the client ID of the diskless node:
          ok> printenv dhcp-clientid
      If a client ID is not configured, configure it:
          ok> setenv dhcp-clientid client-id-name
3. where client-id-name is an ASCII string. In this procedure, `test` is used as an example client ID. Convert the ASCII string to hexadecimal. For example, if `test` is your client ID, the hexadecimal equivalent is `74 65 73 74`. Log in to the master node. Declare the diskless node's client ID in the `/export/root/`diskless-node-name`/etc/default/dhcpagent` file. For example, if the hexadecimal equivalent of your client ID is `74 65 73 74` on a Netra CT 810 machine, add the following line to the `dhcpagent` file:
       CLIENT_ID=0x74657374
4. For information about the format of the `CLIENT_ID` on the hardware you are using, see the corresponding hardware documentation. Update the DHCP configuration table for the NIC0 interface of the diskless node:
       # dhtadm -A -m macro-name -d \
       ':NhCgtpAddr=local-cgtp-addr:Include=Common:\
       BootFile=inetboot.sun4u.os:\
       SrootPTH=/export/root/diskless-node-name:\
       SswapPTH=/export/swap/diskless-node-name:Include=subnet:'
   macro-name is the NIC0 IP address of the node. local-cgtp-addr is the IP address of the `cgtp0` interface of the node. os is the operating system. Specify `Solaris_8` or `Solaris_9` depending on the Solaris version you installed. diskless-node-name is the name of the node. subnet is the NIC0 subnet. For a diskless node, `netraDISKLESS1`, with the NIC0 IP address `10.250.1.30` and Solaris 9, type:
       # dhtadm -A -m 10.250.1.30 -d \
       ':NhCgtpAddr=10.250.3.30:Include=Common:BootFile=inetboot.sun4u.Solaris_9:\
       SrootPTH=/export/root/netraDISKLESS1:\
       SswapPTH=/export/swap/netraDISKLESS1:Include=10.250.1.0:'
5. Update the DHCP network table for the NIC0 interface of the diskless node:
       # pntadm -A IP-address -i diskless-node-clientID \
       -f PERMANENT+MANUAL -m macro-name subnet
   IP-address is the NIC0 IP address of the node. diskless-node-clientID is the hexadecimal equivalent of the client ID. macro-name is the NIC0 IP address of the node. subnet is the subnet of the NIC0 interface. For a Netra CT 810 diskless node with the NIC0 IP address `10.250.1.30` and client ID `74657374`, type:
       # pntadm -A 10.250.1.30 -i 74657374 \
       -f PERMANENT+MANUAL -m 10.250.1.30 10.250.1.0
6. For information about the format of the `CLIENT_ID` on the hardware you are using, see the corresponding hardware documentation. Update the DHCP configuration table for the NIC1 interface of the diskless node:
       # dhtadm -A -m macro-name -d \
       ':NhCgtpAddr=local-cgtp-addr:Include=Common:\
       BootFile=inetboot.sun4u.os:\
       SrootPTH=/export/root/diskless-node-name:\
       SswapPTH=/export/swap/diskless-node-name:Include=subnet:'
   macro-name is the NIC1 IP address of the node. local-cgtp-addr is the IP address of the `cgtp0` interface of the node. os is the operating system. Specify `Solaris_8` or `Solaris_9` depending on the Solaris version you installed. diskless-node-name is the name of the node. subnet is the NIC1 subnet. For the diskless node, `netraDISKLESS1`, with the NIC1 IP address `10.250.2.30` and Solaris 9, type:
       # dhtadm -A -m 10.250.2.30 -d \
       ':NhCgtpAddr=10.250.3.30:Include=Common:BootFile=inetboot.sun4u.Solaris_9:\
       SrootPTH=/export/root/netraDISKLESS1:\
       SswapPTH=/export/swap/netraDISKLESS1:Include=10.250.2.0:'
7. Update the DHCP container for the NIC1 interface of the diskless node.
       # pntadm -A IP-address -i diskless-node-clientID \
       -f PERMANENT+MANUAL -m macro-name subnet
   IP-address is the NIC1 IP address of the node. diskless-node-clientID is the hexadecimal equivalent of the client ID. macro-name is the NIC1 IP address of the node. subnet is the NIC1 subnet. For the diskless node with NIC1 IP address `10.250.2.30` and client ID `74657374`, type:
       # pntadm -A 10.250.2.30 -i 74657374 \
       -f PERMANENT+MANUAL -m 10.250.2.30 10.250.2.0
For information about the format of the `CLIENT_ID` on the hardware you are using, see the corresponding hardware documentation.
Previous Contents Index Next

Copyright 1994-2004 Sun Microsystems