# Modem Settings (for servers whose service controller is equipped with a modem)

Changes to modem settings take effect on the next login connection over the RSC modem.

## Parity

This field sets the RSC modem parity.

## Stop Bits

This field sets the RSC modem stop bits.

## Data Bits

This field sets the RSC modem data bits.

## Country

This field sets the modem country code.

# Serial Port Settings (for all servers)

Changes to serial port settings take effect on the next login connection over the RSC serial port.

## Baud Rate

These options set the RSC modem baud rate.

## Parity

These options set the RSC modem parity.

## Stop Bits

These options set the RSC modem stop bits.

## Data Bits

This field sets the RSC modem data bits.

## Enable Hardware Handshaking (for Sun Enterprise 250 servers only)

Check this box to enable hardware handshaking on the serial port. You should check this box if you have a modem connected to the RSC serial port. If this box is not checked, RSC disconnects a session connected to the serial port after 10 minutes of inactivity.

# PPP Settings (for all servers)

Changes to PPP settings take effect on the next PPP connection to RSC.

## Enable PPP

Check this box to make PPP the default protocol for RSC. Leave the following two fields blank if the client connecting to RSC will be responsible for setting them.

### Local IP Address

Use this field to specify the Internet address for RSC to use during a PPP session.

### Remote IP Address

Use this field to specify the Internet address for the remote node during a PPP session.