Patch-ID# 107460-03
Keywords: st Magstar auto eject ioctl uscsigetrqs MLR-3 SLR-5
Synopsis: SunOS 5.7: st driver patch
Date: 21/May/99

Solaris Release: 7

SunOS release: 5.7

Unbundled Product: 

Unbundled Release: 

Topic: SunOS 5.7: st driver patch

BugId's fixed with this patch: 4166568 4166574 4166583 4206636 4208102 4211607 

Changes incorporated in this version: 4206636 4211607

Relevant Architectures: sparc

Patches accumulated and obsoleted by this patch:  

Patches which conflict with this patch: 

Patches required with this patch: 

Obsoleted by: 

Files included with this patch:

/kernel/drv/st
/kernel/drv/sparcv9/st
/kernel/drv/st.conf
/usr/include/sys/mtio.h
/usr/include/sys/scsi/impl/uscsi.h
/usr/include/sys/scsi/targets/stdef.h

Problem Description:

4211607 Tandberg MLR-3 cannot be recognized on Solaris 7
4206636 Tandberg SLR-5(QIC tape device) cannot be used on Solaris 7

(from 107460-02)

4208102 st: implement the "uscsigetrqs" ioctl
4166574 st: new ioctl to acquire the status of clean bit

(from 107460-01)

4166583 PSARC/1998/366: deferred error handling
4166568 PSARC/1998/366: sense tape positioning problems and auto 
        eject the tape

Patch Installation Instructions:
--------------------------------

For Solaris 2.0-2.6 releases, refer to the Install.info file and/or
the README within the patch for instructions on using the generic
'installpatch' and 'backoutpatch' scripts provided with each patch.

For Solaris 7 release, refer to the man pages for instructions on
using 'patchadd' and 'patchrm' scripts provided with Solaris.
Any other special or non-generic installation instructions should be
described below as special instructions.  The following example
installs a patch to a standalone machine:

       example# patchadd /var/spool/patch/104945-02

The following example removes a patch from a standalone system:

       example# patchrm 104945-02

For additional examples please see the appropriate man pages.

Special Install Instructions: 
----------------------------- 
None.

