## System Timeout Settings Page

This page displays system timeout parameters. Items marked with an asterisk (*) represent mandatory fields.

Field/Button | Description
*Ping | Time after which an unsuccessful ping attempt is considered failed.
*Email | Time after which an unsuccessful email attempt is considered failed.
*Sun Storage Arrays (http tokens) | Time after which an unsuccessful receipt of token data is considered failed.
*SNMP Access | Time after which an unsuccessful SNMP access attempt is considered failed.
*Inband Discovery | Time after which an unsuccessful attempt to discover in-band devices is considered failed.
*luxadm (Sun A5000) | Time after which an unsuccessful attempt to discover Sun A5000 devices is considered failed.
*RM6 (Sun A3500FC) | Time after which an unsuccessful attempt to discover Sun A3500FC devices is considered failed.
*sccli (Sun 3510) | Time after which an unsuccessful attempt to discover Sun 3510 devices is considered failed.

### Related Topics

- Viewing and Editing System Timeout Settings
- Resetting System Timeout Settings