## Setting Up Volume Verify

You can set up the Volume Verify function to run manual parity checks on Sun T3, Sun T4, and Sun StorEdge 6120 array volumes.

To set up volume verify to run on all Sun T3, Sun T4, and Sun StorEdge 6120 arrays:

1. Click Storage Automated Diagnostic Environment > Inventory.

The Devices page is displayed showing summary information for each system device.

2. From the Actions drop-down menu, select Setup Volume Verify.

The Volume Verify Setup page is displayed.

3. Select the Activate Volume Verify check box.
4. To enable Continuous Volume Verify to automatically fix errors it encounters while running, select the Run with `fix' option check box.

Note -

This option may mistakenly fix parity on bad blocks. Contact your storage system representative for more information.

5. From the Run on same array at most every X days list, select how often, in days, you want Continuous Volume Verify to run on any one array.
6. From the day-of-the-week lists, choose a time period from at least one day at which that you want Continuous Volume Verify to run.
7. From the Execution Rate list, select the rate at which you want Continuous Volume Verify to run.
8. Enter the default array password, if configured, for the system.
9. Click OK.

### Related Topics

- Running a Diagnostic Test on a Device