## Archiving a Topology

To archive the current topology:

1. Click Storage Automated Diagnostic Environment > Topology.

The system configuration is displayed in the default topological view set in Preferences.

2. From the Actions drop-down menu, select Archive Current Topology.

A confirmation is displayed when the topology is successfully archived.

### Related Topics

- About Monitoring Topologies
- Changing Topology Views
- Viewing the Storage Network Topology
- Viewing Archived Topologies
- Viewing an Archived Topology Snapshot
- Deleting an Archived Topology Snapshot