## Volume Verify Setup Page

This page enables you to set up volume verify to run on all Sun T3, Sun T4, and Sun StorEdge 6120 arrays.

Field | Description
Activate Volume Verify | Select to enable the Volume Verify utility. Volumes are verified one at a time on a rotational basis for all enabled arrays.
Run with `fix' option | Select to allow Volume Verify to automatically fix volume errors. Note: The fix option might mistakenly fix parity on bad blocks. Consult your service representative for details.
Run on same array at most every X days | Select the maximum frequency at which you want Volume Verify to run on the same array.
Sunday, Monday, Tuesday, Wednesday, Thursday, Friday, Saturday | For each day of the week you want Volume Verify to run, select the hour during which Continuous Volume Verify will run. To run Volume Verify continuously during the corresponding day, select Anytime.
Execution Rate | Select the rate at which you want Volume Verify to run on all arrays. Higher execution rates result in lower array I/O performance.
Default Array Password | Enter the default password for arrays (if configured).

### Related Topics

- Running a Diagnostic Test on a Device