Patch-ID# 118779-01
Keywords: b10n application software image firmware sun fire
Synopsis: Firmware: Sun Fire B10n application software
Date: Jan/03/2005


Install Requirements: Additional instructions may be listed below                      
                      
Solaris Release: 

SunOS Release: 

Unbundled Product: Sun Fire B10n application software

Unbundled Release: N/A

Xref: 

Topic: 

Relevant Architectures: 

BugId's fixed with this patch: 6212005

Changes incorporated in this version: 6212005

Patches accumulated and obsoleted by this patch: 

Patches which conflict with this patch: 

Patches required with this patch: 

Obsoleted by: 

Files included with this patch: 

sunfire_b10n.1.3.6

Problem Description:

6212005 memory leak in http application monitoring

Patch Installation Instructions:
--------------------------------
 
The procedures for upgrading software for the Sun Fire B10n blade involve 
using TFTP. This means that to perform them you need to have a TFTP server 
available on your network.
 
1. Setup a TFTP Server (refer to the adminstration manual if necessary).
 
 
2. Access the Sun Fire B10n console. At the Sun Fire B1600 SC console SC> type:
 
	sc> console Sn
	Where n is the slot number of the B10n blade
 
3. Login to the B10n console.
 
	Login: admin
	password: admin
 
4. Verify the boot image and versions:
 
puma{admin}# show system
 
Boot Options:
================================================================================
Config Type   Config File   Boot Image         Diag Level   Verbose Mode
--------------------------------------------------------------------------------
running                 1   2 (1.3.5)                   0              0
next                    1   2 (1.3.5)                   0              0
================================================================================
 
 
Image Information Table:
================================================================================
Image   Blade   Image Type      Version      Build Date:Time      Size      
--------------------------------------------------------------------------------
1       B10n    Load Balancer   1.3.5        05/24/04 : 16:09     4166917   
2       B10n    Load Balancer   1.3.5        05/24/04 : 16:09     4166917   
diag    B10n    Diagnostics     1.3.5        05/24/04 : 16:10     2506350   
================================================================================
 
Flash FS /RFA0 free space = 17,072,128 bytes
 
puma{admin}# 
 
 
5. Determine which image to update (image 1 or 2), and update the empty or 
   oldest image.
 
6. Update the B10n application software. As admin, use the following command:
 
    puma{admin}# update image <tftp server> file <image_name> image <location>
 
   The <image_name> is the file located in this patch.
 
   The following example uses the TFTP server with the IP address of 
   192.50.50.201, the image name of sunfire_b10n.1.3.6, and the image 
   at location 1.
 
	puma{admin}# update image 192.50.50.201 file sunfire_b10n.1.3.6 image 1
 
   The system returns the following output, verifying the parameters entered:
 
	file exist! will overwrite /RFA0/BOOTIMAGE/boot_image_1
	Start downloading sunfire_b10n.1.3.6... using TFTP
	Transferring and writing to file /RFA0/BOOTIMAGE/boot_image_1...
	please wait.
 
	puma{admin}#
 
7. Set the new Images to be the Default Image as follows:
 
   a.  Configure the desired Boot Image. At the B10n console type:
 
	puma{admin}# config boot image x
 
	Where x is the image you just updated
 
   b. Save the updated image using the commit command:
 
	puma{admin}# commit
	commit : Are you sure to continue? [yes|no]yes
 
            Note: To power off any content load balancing blade,
            you must have access to the system controller and 
            r-level user permission. Refer to the Sun Fire B1600 
            Blade System Chassis Administration Guide for information 
            on system controller user permissions.
 
   c.  From the B1600 system controller , execute the following commands: 
 
	    Note: The poweroff, removefru, and poweron command can be 
            executed from the SC console or SC telnet session.
 
		SC> poweroff S<n>
 
		SC> removefru S<n>
 
		SC> poweron S<n>
 
	Where <n> is the number of the slot containing the blade when
	the Update B10n Software image has been installed.

Special Install Instructions:
----------------------------- 
 
After bringing up B10n 1.3.6  image, verify the running image by typing 
the following command:
 
 
puma{admin}# show system
 
Boot Options:
================================================================================
Config Type   Config File   Boot Image         Diag Level   Verbose Mode
--------------------------------------------------------------------------------
running                 1   1 (1.3.6)                   0              0
next                    1   1 (1.3.6)                   0              0
================================================================================
 
 
Image Information Table:
================================================================================
Image   Blade   Image Type      Version      Build Date:Time      Size      
--------------------------------------------------------------------------------
1       B10n    Load Balancer   1.3.6        12/24/04 : 08:23     4168058   
2       B10n    Load Balancer   1.3.5        05/24/04 : 16:09     4166917   
diag    B10n    Diagnostics     1.3.5        05/24/04 : 16:10     2506350   
================================================================================
 
Flash FS /RFA0 free space = 17,070,080 bytes

README -- Last modified date:  Monday, January 3, 2005

