Patch-ID# 108965-02
Keywords: mobile IP snoop services ILP MH MA
Synopsis: SunOS 5.8_x86: /usr/sbin/snoop patch
Date: 20/Mar/00

Solaris Release: 8_x86

SunOS release: 5.8_x86

Unbundled Product: 

Unbundled Release: 

Topic: SunOS 5.8_x86: /usr/sbin/snoop patch

	NOTE:	Refer to Special Install Instructions section for 
		IMPORTANT specific information on this patch.

BugId's fixed with this patch: 4297326 4297676 4313760 4315280 4317713 4321696 4321713 4321720 4321721 4321723 4321725 4321726 4322042 4322055 4322058 4322060 4322064 4322200 4322670 

Changes incorporated in this version: 4297326 4313760 4315280 4317713 4321696 4321713 4321720 4321721 4321723 4321725 4321726 4322042 4322055 4322058 4322060 4322064 4322200 4322670

Relevant Architectures: i386

Patches accumulated and obsoleted by this patch:  

Patches which conflict with this patch: 

Patches required with this patch: 

Obsoleted by: 

Files included with this patch:

/etc/inet/services
/usr/sbin/snoop

Problem Description:

4321726 When HA receives a regreq with a buffer overflowing extension, it core dumps
4321713 Granted lifetime keeps increasing as the registration is refreshed
4321721 FA shouldn't reject regreq with both MH and MA
4321725 FA expects to receive challenge-response extension before MH auth
4321720 FA should discard the message if it contains an unrecognized extension 0-127
4313760 Reg Request with same ILP for HA and Coaddr times out.
4321723 snoop parses agent advertisement wrong
4322200 mipagentconf and mipagentstat don't  setlocaled.
4322670 Pool addresses are wrong due to byte ordering when mipagent run on x86
4321696 After a succesful reg-dereg, HA core dumps
4317713 Sample mipagent.conf files have inconsistent info which might be confusing
4322042 AAA open session result was not getting propogated into registration response.
4322055 mipagent should accept an HA of 0xffffffff when the request comes from AAA
4322058 remove #if 0 code lines left in AAA code
4322060 Add aaaSPI per current AAA extension specification
4322064 dynamic key info from AAA server not being propogated to agents correctly
4297326 mipagentstat: command line option '-v' should be reserved for 'verbose'
4315280 Debug flag defined which includes test code NOT to be shipped to customers.

(from 108965-01)

4297676 Need Mobile IP support in Solaris

Patch Installation Instructions:
--------------------------------

For Solaris 2.0-2.6 releases, refer to the Install.info file and/or
the README within the patch for instructions on using the generic
'installpatch' and 'backoutpatch' scripts provided with each patch.

For Solaris 7-8 releases, refer to the man pages for instructions
on using 'patchadd' and 'patchrm' scripts provided with Solaris.
Any other special or non-generic installation instructions should be
described below as special instructions.  The following example
installs a patch to a standalone machine:

       example# patchadd /var/spool/patch/104945-02

The following example removes a patch from a standalone system:

       example# patchrm 104945-02

For additional examples please see the appropriate man pages.

Special Install Instructions: 
----------------------------- 

	NOTE:	To get the Mobile IP support, one needs to install the 
		following pkgs:

                SUNWmipr (Mobile-IP configuration and startup scripts)
                SUNWmipu (Mobile-IP daemon and utilities)
