Patch-ID# 108980-04
Keywords: Hotplug hotswap scsb PCI pcihp
Synopsis: SunOS 5.8_x86: PCI HotPlug framework patch
Date: 18/Apr/00

Solaris Release: 8_x86

SunOS release: 5.8_x86

Unbundled Product: 

Unbundled Release: 

Topic: SunOS 5.8_x86: PCI HotPlug framework patch

BugId's fixed with this patch: 4272737 4276021 4303126 4306367 4307062 4307080 4307747 4307827 4309011 4309802 4309818 4310864 4311126 4311134 4312937 4314121 4314936 4315098 4315100 4315101 4318351 4318747 4320440 4320471 4330429 4330774 

Changes incorporated in this version: 4318351 4330429 4330774

Relevant Architectures: i386

Patches accumulated and obsoleted by this patch:  

Patches which conflict with this patch: 

Patches required with this patch: 

Obsoleted by: 

Files included with this patch:

/kernel/misc/hpcsvc 
/kernel/misc/pcicfg
/kernel/misc/pcihp
/usr/include/sys/hotplug/hpcsvc.h
/usr/include/sys/hotplug/hpctrl.h
/usr/include/sys/hotplug/pci/pcicfg.h
/usr/include/sys/hotplug/pci/pcihp.h
/usr/lib/cfgadm/pci.so.1
/usr/lib/devfsadm/linkmod/SUNW_misc_link.so
/usr/lib/devfsadm/linkmod/SUNW_misc_link_i386.so

Problem Description:

4318351 scsb driver shall implement software control of LEDs
4330429 System hangs on boot if faulty fantray or powersupply present
4330774 change in hpctrl.h required for PCI HotPlug Framework

(from 108980-03)

4314121 pci plug-in library shows regression on attachment point's names
4303126 pci.so: pcisch# and like get munged to pci0 regardless of what #

(from 108980-02)

4320471 After a Basic Hotswap operation, cPCI board type information is missing!
4320440 Public API for control of SSB Slot LEDs
4318747 Unnecessary warning message "WARNING: i2c_0 forcing polled mode operation"

(from 108980-01)

4276021 Solaris Hotplug Framework requires complete support for both Basic & Full hotswap
4307062 Alarm card should have a unique product ID
4307080 Value being returned from Temperature device not correct
4307747 prtdiag does not work correctly on CompactPCI platforms
4309011 p1.0 obp: device node changes cause scsb devlinks to not be created
4309802 Need support to hotswap QuadFast Ethernet, SunSwift PCI together
4309818 PCI configurator module should be dynamically loadable
4311134 SCSB hsc module does need extensions to support full hotswap
4307827 Some #defines are defined in multiple .h with different values
4306367 env4test does not test env and i2c devices
4272737 db21554 bridge driver needs to program proper dvma address range
4310864 ENVC_IOC_GETFAN ioctl not supported in pcf8574 driver
4314936 p1.5 scsb: high interrupt line causes scsb driver to hang during attach
4311126 Need support for handling ENUM# interrupt event synchronously
4315101 Need to keep slots in reset during hotswap
4315100 Alarm Card Probe Support required in PCI Configurator during Hotswap
4315098 pcihp must use slot-flags for autoconfiguration during cPCI full hotswap
4312937 scsb_intr passes a null value to putnext(); scsb_rq uninitialized.

Patch Installation Instructions:
--------------------------------

For Solaris 2.0-2.6 releases, refer to the Install.info file and/or
the README within the patch for instructions on using the generic
'installpatch' and 'backoutpatch' scripts provided with each patch.

For Solaris 7-8 releases, refer to the man pages for instructions
on using 'patchadd' and 'patchrm' scripts provided with Solaris.
Any other special or non-generic installation instructions should be
described below as special instructions.  The following example
installs a patch to a standalone machine:

       example# patchadd /var/spool/patch/104945-02

The following example removes a patch from a standalone system:

       example# patchrm 104945-02

For additional examples please see the appropriate man pages.

Special Install Instructions: 
----------------------------- 

Reboot the system after patch installation.
