> ## Updating a Smart Card

> Solaris Smart Cards knows the current Answer to Reset values of the three smart card types it supports. By default, the ATRs for all three card times are activated when you first start up smart cards. If the manufacturer changes the ATR for a newer release of a card, you have to edit the ATR value of the card in the Smart Cards dialog box.

Sun Microsystems, Inc. http://www.sun.com

Copyright © 1999 Sun Microsystems, Inc.