Patch-ID# 109874-02
Keywords: AC-97 audio mixer audiots cpr interrupt audiocs sdtaudio
Synopsis: SunOS 5.8: audio patch
Date: 18/Jul/00

Solaris Release: 8

SunOS release: 5.8

Unbundled Product: 

Unbundled Release: 

Topic: SunOS 5.8: audio patch

	NOTE:   Refer to Special Install Instructions section for 
                IMPORTANT specific information on this patch.

BugId's fixed with this patch: 4271687 4291027 4304911 4305392 4307415 4327740 4329687 4332773 4333448 4339937 4350077 

Changes incorporated in this version: 4291027 4350077

Relevant Architectures: sparc

Patches accumulated and obsoleted by this patch: 109341-03 

Patches which conflict with this patch: 

Patches required with this patch: 

Obsoleted by: 

Files included with this patch:

/etc/driver_aliases
/etc/name_to_major
/usr/include/sys/ac97.h
/usr/include/sys/audiots.h
/usr/kernel/drv/audiocs
/usr/kernel/drv/audiots.conf
/usr/kernel/drv/sparcv9/audiocs
/usr/kernel/drv/sparcv9/audiots
/usr/kernel/misc/mixer
/usr/kernel/misc/sparcv9/mixer
/usr/lib/adb/sparcv9/audiots_state

Problem Description:

4350077 pause, mute and volume control functions do not work in sdtaudio
4291027 unclaimed audio interrupts on Sun4m using sunvts

(from 109874-01)

	This patch revision was generated to accumulate and obsolete
	the feature changes introduced in point patch 109341-03.

4271687 AC-97 compliant audio driver is needed for new platform using Acer South Bridge.
4304911 Switching modes while recording panics with a null pointer dereference
4307415 audio mixer panics when audio driver doesn't support monitor feature
4305392 new audio device set to high level interrupt when it should be low level
4327740 New platform OBP 4.0.166 requires the audiots driver to use the upper 2 gig addresses
4332773 Audio goes silent on a small percentage of new systems after a power cycle
4333448 audio mixer seems to cause panic during cpr
4339937 audiots: cpr panics during suspend operation on new platform

(from 109341-03)

4305392 new audio device set to high level interrupt when it should be low level
4333448 audio mixer seems to cause panic during cpr
4339937 audiots: cpr panics during suspend operation on new platform

(from 109341-02)

4327740 New platform OBP 4.0.166 requires the audiots driver to use the upper 2 gig addresses
4332773 Audio goes silent on a small percentage of new platform after a power cycle

(from 109341-01)

4271687 AC-97 compliant audio driver is needed for new platform using Acer South Bridge.
4304911 Switching modes while recording panics with a null pointer dereference
4307415 audio mixer panics when audio driver doesn't support monitor feature
4329687 Audio packages need depend files installed in packages

Patch Installation Instructions:
--------------------------------

For Solaris 2.0-2.6 releases, refer to the Install.info file and/or
the README within the patch for instructions on using the generic
'installpatch' and 'backoutpatch' scripts provided with each patch.

For Solaris 7-8 releases, refer to the man pages for instructions
on using 'patchadd' and 'patchrm' scripts provided with Solaris.
Any other special or non-generic installation instructions should be
described below as special instructions.  The following example
installs a patch to a standalone machine:

       example# patchadd /var/spool/patch/104945-02

The following example removes a patch from a standalone system:

       example# patchrm 104945-02

For additional examples please see the appropriate man pages.

Special Install Instructions: 

----------------------------- 

	NOTE:   To get the full support for following platforms:

                        SUNW,Sun-Blade-100
                        SUNW,Sun-Blade-1000

                one needs to install the following new packages:

                SUNW1394h       Sun IEEE1394 Framework Header Files
                SUNW1394x       Sun IEEE1394 Framework
                SUNWeridx       Sun RIO 10/100 Mb Ethernet Drivers (64-bit)
                SUNWiscr        Sun ISCRI OCF CT Driver
                SUNWiscrx       Sun ISCRI OCF CT Driver (64-bit)
                SUNWstcx        SUN ISCRI Kernel Driver - (64-bit)
                SUNWusx.u       UltraSPARC CPU Device Driver (64-bit)
                SUNWpiclh       PICL Header Files
                SUNWpiclr       PICL Framework (Root)
                SUNWpiclu       PICL Libraries, and Plugin Modules (Usr)
                SUNWpiclx       PICL Libraries (64-bit)

		AND the following patches:

		108528-03 (or newer)    kernel update patch
		108979-08 (or newer)    devfsadm, platform nexus, I2C and 
                                        Netra ct patch
		109883-01 (or newer)    ecppsys.h patch
		109877-01 (or newer)    dma_i8237A.h patch
		109793-02 (or newer)    su driver patch
		109872-01 (or newer)    vis driver patch
		109873-01 (or newer)    prtdiag patch
		108974-05 (or newer)	dada, uata, dad, sd and scsi patch
		109874-01 (or newer)    audio patch
		108725-02 (or newer)    st patch
		109876-01 (or newer)    fd patch	
		109885-01 (or newer)    glm patch
		109879-01 (or newer)    isadma patch
		109880-01 (or newer)    forthdebug patch
		109881-01 (or newer)    1394 adb macros patch
		109882-01 (or newer)    eri header files patch
		109892-01 (or newer)    ecpp patch
		109888-01 (or newer)    platform drivers patch
		109889-01 (or newer)    usr platform and libc_psr patch
		109887-01 (or newer)    smartcard patch
