> ## Basic Configuration Folder

> The basic configuration folder includes these properties:

> - Unique Card Terminal Name - Contains a unique name to identify this reader.
> - Model Name - Contains the manufacturer's model name for the card reader you selected from the Add Reader Dialog Box.

>   Note: | Do not change the model name unless you are upgrading to a version of the card reader with a new model name.

> - Device Port - Requires the fully-qualified device name for the port where the reader is attached, for example /dev/cua/b for serial port b.

> ##### To Define Basic Properties for Your Card Reader

> 1. Type a unique name for your card reader in the Unique Card Terminal Name property, or accept the default name in the field.

>    If you have more than one card reader of the same type attached to the host, you must type unique card terminal names for each reader.

> 2. Type the model name for the card reader only if you are using a newer version of the card reader than the one with the model name displayed.
> 3. Type the name of the device port where the reader is attached.

Sun Microsystems, Inc. http://www.sun.com

Copyright © 1999 Sun Microsystems, Inc.