Patch-ID# 109815-03
Keywords: Card, hotswappable, SCSB, scsb, se, se_async_softint obp
Synopsis: SunOS 5.8: se driver patch
Date: 02/Nov/00

Solaris Release: 8

SunOS release: 5.8

Unbundled Product: 

Unbundled Release: 

Topic: SunOS 5.8: se driver patch

        **********************************************************************
        NOTE: This patch may contain one or more OEM-specific platform ports.
              See the appropriate OEM_NOTES file within the patch for
              information specific to these platforms.
              DO NOT INSTALL this patch on an OEM system if a corresponding
              OEM_NOTES file is not present (or is present, but instructs not
              to install the patch), unless the OEM vendor directs otherwise.
        **********************************************************************

BugId's fixed with this patch: 4304938 4308769 4319571 4320055 4335099 4342866 4343601 4345375 4346323 4354219 4365262 4367981 4368931 

Changes incorporated in this version: 4342866 4365262 4367981

Relevant Architectures: sparc

Patches accumulated and obsoleted by this patch: 109731-02 110334-01 

Patches which conflict with this patch: 

Patches required with this patch: 

Obsoleted by: 

Files included with this patch:

/kernel/drv/se
/kernel/drv/sparcv9/se
/platform/SUNW,UltraSPARC-IIi-Netract/kernel/drv/se.conf
/platform/SUNW,UltraSPARC-IIi-Netract/kernel/drv/sparcv9/acebus
/platform/SUNW,UltraSPARC-IIi-Netract/kernel/drv/sparcv9/scsb

Problem Description:

4342866 Hotswap Drivers need to adopt fix for 4338633
4367981 Need to bring up system in Full Hotswap  mode by default
4365262 Should not warn about  not getting HEALTHY# at insertion

(from 109815-02)

        This patch revision was generated to accumulate and obsolete
        the feature changes introduced in point patch 110334-01 and
        109731-02.
         

4319571 Alarm Card should be hotswappable
4346323 SCSB driver needs support for a ioctl to upload/download Alarm relay
4368931 scsb needs to deliver an event for SCB hot removal
4320055 se driver needs support for DDI_DETACH and hence dynamic unloading

(from 109815-01)

4343601 replacement powersupply left in standby mode
4335099 CTC should not be showing up as cPCI card
4345375 scsb_leddata kstat must present user interface slot numbers for prtdiag

(from 109731-02)

4354219 OS returns tty ports to default mode regardless of obp settings

(from 109731-01)

4308769 se_async_softint called canputnext without checking for valid q_next
4304938 "stty 0" freeze system

(from 110334-01)

4319571 Alarm Card should be hotswappable
4346323 SCSB driver needs support for a ioctl to upload/download Alarm relay
4368931 scsb needs to deliver an event for SCB hot removal
4320055 se driver needs support for DDI_DETACH and hence dynamic unloading

Patch Installation Instructions:
--------------------------------

For Solaris 2.0-2.6 releases, refer to the Install.info file and/or
the README within the patch for instructions on using the generic
'installpatch' and 'backoutpatch' scripts provided with each patch.

For Solaris 7-8 releases, refer to the man pages for instructions
on using 'patchadd' and 'patchrm' scripts provided with Solaris.
Any other special or non-generic installation instructions should be
described below as special instructions.  The following example
installs a patch to a standalone machine:

       example# patchadd /var/spool/patch/104945-02

The following example removes a patch from a standalone system:

       example# patchrm 104945-02

For additional examples please see the appropriate man pages.

Special Install Instructions: 
----------------------------- 
Reboot the system after patch installation.

