> ## Configuring a Card Reader

> The first task in setting Solaris Smart Cards is to set up a card reader for the host. When you select Configure Card Reader from the Navigation pane, the icons that appear in the Console pane enable you to:

> - Add a new card reader.
> - View and modify properties set up for an already configured card reader, as explained in To Define Basic Properties for Your Card Reader.

> #### To Add a New Card Reader

> 1. Ensure that you have already attached the smart card reader to the local host.
> 2. Change permissions on the port where the card reader is attached, as explained in the Solaris Smart Cards Administration Guide.
> 3. Click Card Readers on the Navigation pane, if you have not done this already.
> 4. Double-click the Add Reader icon and display the Add New Reader Dialog Box.

Sun Microsystems, Inc. http://www.sun.com

Copyright © 1999 Sun Microsystems, Inc.