#
#pragma ident "@(#)Config-Reader4uwg-ruletext-d.x	1.5 01/02/13 Sun Microsystems"
#

_rules = {
        rulemsg:ircr4u209msg = "Memory Error"
        rulemsg:ircr4u209longmsg = "%s on %s"

        rulemsg:ircr4u210msg = "Hardware Error"
        rulemsg:ircr4u210longmsg = "Hardware Error: %s"

        rulemsy:ircr4u211msr = "Fatal Error"
        rulemsg:ircr4u211longmsg = "Fatal Error: %s"

        rulemsg:ircr4u212msg = "Memory Error"
        rulemsg:ircr4u212longmsg = "Hardware corrected error in %s on %s"

        rulemsg:ircr4u214msg = "Error"
        rulemsg:ircr4u214longmsg = "failing: %s"

        rulemsg:ircr4u216msg = "cpu error"
        rulemsg:ircr4u216longmsg = "cpu panic: %s: %s"

        rulemsg:ircr4u217msg = "tape Error"
        rulemsg:ircr4u217longmsg = "tape Error: %s: error rate: %s%%"

        rulemsg:ircr4u219msg = "disk removed"
        rulemsg:ircr4u219longmsg = "disk removed: %s"

        rulemsg:ircr4u220msg = "disk inserted"
        rulemsg:ircr4u220longmsg = "disk inserted: %s"

        rulemsg:ircr4u205msg = "Board temperature"
        rulemsg:ircr4u205longmsg = "%s temperature is %s: boardtype is %s "

        rulemsg:ircr4u204msg = " Fan Status"
        rulemsg:ircr4u204longmsg = "Fan Status is: %s"

        rulemsg:ircr4u213msg = "Notice"
        rulemsg:ircr4u213longmsg = "Hotplug: %s removed"

        rulemsg:ircr4u215msg = "Notice"
        rulemsg:ircr4u215longmsg = "Hotplug: %s inserted"

        rulemsg:ircr4u224msg = "Warning"
        rulemsg:ircr4u224longmsg = "hot plug installed: %s"

        rulemsg:ircr4u221msg = "Warning"
        rulemsg:ircr4u221longmsg = "redundant power status: %s"

        rulemsg:ircr4u225msg = "st status"
        rulemsg:ircr4u225longmsg = "%s st status is: %s"

	rulemsg:ircr4u230msg = "Temperature Status"
	rulemsg:ircr4u230highfmsg = "critically high"
	rulemsg:ircr4u230highwmsg = "high"
	rulemsg:ircr4u230lowfmsg = "critically low"
	rulemsg:ircr4u230lowfmsg = "low"
        rulemsg:ircr4u230longmsg = "Device %s has a %s temperature: %s"

        rulemsg:ircr4u218msg = "bank-0-status status"
        rulemsg:ircr4u218longmsg = "%s bank-0-status status is: %s"

        rulemsg:ircr4u203msg = "power supply status"
        rulemsg:ircr4u203longmsg = "%s power supply status is: %s"

        rulemsg:ircr4u200msg = "DIMM status"
        rulemsg:ircr4u200longmsg = "%s DIMM status is: %s"

        rulemsg:ircr4u201msg = "hot plug charge/precharge status"
        rulemsg:ircr4u201longmsg = "%s hot plug charge/precharge status is: %s"

        rulemsg:ircr4u207msg = "general status"
        rulemsg:ircr4u207longmsg = "%s general status is: %s"

        rulemsg:irpfa300msg = "PFA: SIMM Error"
        rulemsg:irpfa300longmsg = "%s: PFA: errors detected on SIMM. Immediately re-seat the SIMM or replace if necessary"

        rulemsg:irpfa301msg = "PFA: DISK Error"
        rulemsg:irpfa301longmsg = "%s: PFA: errors detected on DISK. Immediately investigate and replace if necessary"

        rulemsg:irpfa302msg = "SMART/PFA: DISk Error"
        rulemsg:irpfa302longmsg = "%s: SMART/PFA: Disk needs service immediately"

}
