Patch-ID# 109701-01
Keywords: dpti2o dptmgr dptutil dptelog 3754sm02.fwi dpt_send SRC/P dpt_reset_hba panic
Synopsis: SunOS 5.7: SRC/P Mandatory Maintenance Update Patch I
Date: Aug/09/00

Solaris Release: 7

SunOS Release: 5.7

Unbundled Product: Sun StorEdge SRC/P SCSI RAID Controller Driver

Unbundled Release: 1.0

NOTE:
**************************************************************************
**************************************************************************
**WARNING:****WARNING:****WARNING:****WARNING:****WARNING:****WARNING:****
*                                                                        *
* - Patch 109701-01 is for SRC/P on Solaris 7 only!                      *
*                                                                        *
* - You must follow ALL the "Special Install Instructions" listed below  *
*   for this patch to be properly applied including flashing the SRC/P   *
*   controller firmware!                                                 *
*                                                                        *
**WARNING:****WARNING:****WARNING:****WARNING:****WARNING:****WARNING:****
**************************************************************************
**************************************************************************


Relevant Architectures: sparc

BugId's fixed with this patch:
4239871 4239984 4240108 4240899 4242887 4242893 4243592 4244745 4245127
4245486 4245844 4246599 4246602 4247329 4248897 4250031 4250032 4250980
4251035 4251144 4252227 4252839 4252936 4253011 4253355 4253369 4253449
4254060 4254098 4254336 4254500 4255152 4255982 4257922 4259572 4260313 
4260858 4260859 4261249 4261649 4261729 4262098 4262292 4262318 4262640
4266033 4266496 4266991 4267632 4267728 4268596 4268628 4269552 4269743
4271225 4271236 4271238 4271491 4271948 4275835 4276137 4276623 4277457
4281582 4282901 4283942 4284453 4285806 4286019 4289659 4290134 4291821
4292938 4295387 4295392 4295430 4296188 4296342 4296647 4296734 4296738
4297193 4297400 4297565 4298251 4299194 4299294 4299305 4300002 4300006
4300041 4300068 4300346 4300371 4300680 4300904 4300908 4301245 4301289
4301290 4301318 4301505 4301545 4301548 4301788 4302255 4302325 4302469
4302654 4302662 4302663 4302665 4302676 4302703 4302715 4302775 4303257
4303444 4304079 4304646 4305320 4305516 4305549 4305642 4305900 4305903
4305911 4305926 4306244 4306358 4306364 4306424 4306651 4306970 4307455
4307457 4307936 4309834 4309836 4309838 4309841 4309843 4309847 4309850
4309853 4309975 4310780 4310965 4311182 4311253 4311637 4311645 4311897
4312336 4313881 4313927 4314020 4315164 4316890 4316891 4317244 4317245
4317246 4317247 4317248 4317250 4317251 4317252 4321055 4321494 4324468
4324699 4324700 4324701 4324740 4326831 4330518 4332761 4333005 4333499
4334143 4336048 4336737 4336819 4337093 4337613 4337774 4338126 4339189
4339651 4340294 4340295 4340297 4340298 4340299 4340301 4340303 4340305
4340307 4340308 4340309 4340310 4340311 4340313 4340314 4340315 4340316
4340317 4340318 4340319 4340324 4340394 4341386 4341924 4342215 4342576
4342584 4343742 4344009 4344277 4344813 4347070 4349107 4351852 4352034


Changes incorporated in this version: 

Patches accumulated and obsoleted by this patch: 

Patches which conflict with this patch: 

Patches required with this patch: 

Obsoleted by: 

Files included with this patch: 

/kernel/drv/dpti2o
/kernel/drv/sparcv9/dpti2o
/opt/SUNWhwrdg/3754smea.ima
/opt/SUNWhwrdg/dptelog
/opt/SUNWhwrdg/dptelog.ini
/opt/SUNWhwrdg/dptelog.rc
/opt/SUNWhwrdg/dpteng
/opt/SUNWhwrdg/dptmgr
/opt/SUNWhwrdg/dptmgr.hlp
/opt/SUNWhwrdg/dptmgr.ini
/opt/SUNWhwrdg/dptmgr.rsc
/opt/SUNWhwrdg/dptsig
/opt/SUNWhwrdg/dptutil
/usr/share/man/man1m/dptutil.1m
/usr/share/man/man7d/dpti2o.7d
Docs/patch_docs.tar.Z


Problem Description: 


See the end of this README for the Problem Descriptions.


Patch Installation Instructions: 
-------------------------------- 
Refer to the Install.info file for instructions on using the
generic 'installpatch' and 'backoutpatch' scripts provided with
each patch.  Any other special or non-generic installation
instructions should be described below as special instructions.

Special Install Instructions: 
----------------------------- 

There is a special "dpt_flashupdate" process that must be followed
to correctly upgrade the target machine.

1. Before starting the patch process backup all your data.  See the
   Answerbook2 online documentation for information about backing up
   data.

2. Copy the compressed file from the "Doc" directory located
   in the patch directory
   (i.e. "109701-01/Docs/patch_docs.tar.Z") to a SRC/P "Doc"
   destination directory.  The compressed file contains
   PostScript versions of updated SRC/P documentation.
   Uncompress and untar this file to get the PostScript files
   (i.e "uncompress patch_docs.tar.Z" and
   "tar xvf patch_docs.tar").  The PostScript files can be
   viewed and printed via "imagetool".

3. Login as root and install the patch via the "installpatch"
   utility (see Install.info) (i.e. "109701-01/installpatch 109701-01").

4. Shutdown the the target machine via "shutdown" or "uadmin"
   and boot in to single-user mode.

5. Make sure "/opt/SUNWhwrdg" is accessible (i.e. you may have to run 
   "mount /opt") and flash the SRC/P firmware by running
   "/opt/SUNWhwrdg/dpt_flashupdate".  The machine will be shutdown when
   the flash process is complete.

6. Boot the machine into multi-user mode and run
   "/opt/SUNWhwrdg/dptutil -L all" and verify that the firmware level
   has been upgraded to "SMEA".  Also, run
  "/usr/bin/showrev -p | grep hwrd" to confirm the patch has been
   applied.  Here's what the output should look like:
	# /usr/bin/showrev -p | grep hwrd
	Patch: 109701-01 Obsoletes:  Requires:  Incompatibles:  Packages:
        SUNWhwrd, SUNWhwrdf, SUNWhwrdg, SUNWhwrdm, SUNWhwrdx

7. It is recommended that after applying the patch (along with updating
   the firmware) and before using your SRC/P RAID arrays that you first
   run the "Verify" option from the SRC/P Storage Manager (NOTE: The "Verify"    
   process can be time consuming, particularly with multiple large arrays).
   This should detect and fix any RAID-5 parity or RAID-1 "mirror"
   inconsistencies.  Any inconsistencies will be reported in the Event Log.  If
   inconsistencies are detected, then it is recommended that you restore your
   data from backup.



------------ SAMPLE FLASH AND INSTALL SESSION START -----------------

Sample "dpt_flashupdate" session:

# 109701-01/installpatch 109701-01
# showrev -p |grep hwrd
Patch: 109701-01 Obsoletes:  Requires:  Incompatibles:  Packages: SUNWhwrd, 
SUNWhwrdf, SUNWhwrdg, SUNWhwrdm, SUNWhwrdx
# sync
# uadmin 2 0
syncing file systems... done
Program terminated
{3} ok boot -s
Resetting ... 


Sun Enterprise 450 (4 X UltraSPARC-II 296MHz), No Keyboard
OpenBoot 3.12, 1024 MB memory installed, Serial #11265262.
Ethernet address 8:0:20:ab:e4:ee, Host ID: 80abe4ee.



Rebooting with command: boot -s                                       
Boot device: /pci@1f,4000/scsi@3/disk@2,0:a  File and args: -s
SunOS Release 5.7 Version Generic_106541-08 64-bit [UNIX(R) System V Release 4.0]
Copyright (c) 1983-1999, Sun Microsystems, Inc.
configuring network interfaces: hme0.
Hostname: wgs40-51

INIT: SINGLE USER MODE

Type control-d to proceed with normal startup,
(or give root password for system maintenance): 
single-user privilege assigned to /dev/console.
Entering System Maintenance Mode

Jun 12 10:21:27 su: 'su root' succeeded for root on /dev/console
Sun Microsystems Inc.   SunOS 5.7       Generic October 1998
You have mail.
# mount /opt
mount: mount point cannot be determined
# /opt/SUNWhwrdg/dpt_flashupdate



Setup environment for SRC/P Flash Update - Please wait...



Checking for Installed SRC/P RAID Controllers - Please wait...



Installed SRC/P RAID Controllers:

#  b0 b1 b2  Controller     Cache  FW    NVRAM     Serial     Status
---------------------------------------------------------------------------
d0 c6 -- c5  DPT PM3755U2B  64MB   SM02  SUN V1.5  12-001953  Optimal

NOTE: SRC/P Controller Firmware (FW) should be at Revision "SMEA" or greater.

Type "y" to update all cards to "SMEA" firmware or "n" to skip update (y/n)? y


About to update all cards to "SMEA" firmware via the following command:

        /opt/SUNWhwrdg/dptutil -F ./3754smea.ima

Your system will be shutdown when the firmware update is complete!

WARNING: Do not interrupt the flash update process!

Type "y" to continue with firmware update or "n" to skip update (y/n)? y

Flashing SRC/P RAID Controller(s) - Please wait...


Downloading flash firmware is completed.


Your system will now be shutdown.


Hit "Enter" key to continue: 


Your system is being shutdown - Please wait...

syncing file systems... done
Program terminated
{0} ok
------------ SAMPLE FLASH AND INSTALL SESSION END -----------------

If the patch has been applied, but "dpt_flashupdate" has not been run, a
warning message like the following will be displayed on the console and in
/var/adm/messages:

dptelog: Installed SRC/P RAID Controllers:
dptelog: #  b0 b1 b2  Controller     Cache  FW    NVRAM     Serial     Status
dptelog: ---------------------------------------------------------------------
dptelog: d0 c6 -- c5  DPT PM3755U2B  64MB   SM02  SUN V1.5  12-001953  Optimal
dptelog:
dptelog: Flash SRC/P Controller(s) with "/opt/SUNWhwrdg/dpt_flashupdate"

Follow the "dpt_flashupdate" process listed in "Special Install Instructions"
to update the SRC/P controller to the proper firmware level. 

If "backoutpatch" must be run, the firmware can be flashed back to
the original version by running:
"/opt/SUNWhwrdg/dptutil -F /opt/SUNWhwrdf/3754sm02.fwi".



Problem Description: 


4239871 "silent" data corruption during NotesBench
4239984 dpt_usr_cmd hangs in dpt driver causing dpteng to hang
4240108 Log file corrupted with master FCS CD release (SM02 FW, 2.0L GUI + Engine)
4240899 Data corruption running mtscsirw
4242887 delete of RAID-5 w/ missing components causes illegal MsgOffset in dpt_getReply
4242893 "recursive mutex_enter" panic on delete of RAID-5 w/ missing components
4243592 PCI SERR running dptutil -L all in loop (3060th loop), LED #8 stuck on
4244745 need to remove GHD driver performance HACK from ghd_waitq.c
4245127 "dptutil -Z" does not work on RAID-5 w/ missing components
4245486 Solaris install shell drvconfig's from GUI/CLI/engine make GUI/CLI unusable
4245844 Array failures appear to be coincident with cache state change
4246599 Convert dpt_usr_cmd() to use ghd_transport() instead of dpt_send().
4246602 Make driver DDI compliant
4247329 RAID-5 with 1 failed drive corrupts files.
4248897 system panic while running newfs on a raid50 array
4250031 CPU(1) panic running 6/25 driver in 32 bit
4250032 DSM file RAID array creation does not build parity or mirror drives
4250980 failed RAID-0 array at boot cannot be made optimal via GUI (needs reboot)
4251035 delay needed after I2O SysEnable
4251144 PCI SERR - System Panic while running VTS with 6/29 package
4252227 panic in mutex_init during boot
4252839 After deleting arrays FAILED message frame bad index (MsgOffset=2f900)
4252936 Miscompares in run_io on newly created RAID-1
4253011 "dptutil -d# -H all" deletes arrays not hot spare drives - data can be lost
4253355 SRC/P User Guide uses different disk numbering scheme from dptutil usage screen
4253369 dptutil man page - '-D all' does *not* delete hot spare drives - poss data loss
4253449 delete of RAID-10 causes device to be unusable until reboot -r
4254060 need to update mscsi.conf to create devices for dpti2o
4254098 SRC/P does not initialise properly on first reboot after changing scsi speed
4254336 PSARC 1998/511 says all events must go to /var/adm/messages
4254500 False low-voltage shutdown causes "Priv Timeout" panic when RAID-5 drive pulled
4255152 dptcli returns bogus "Incorrect HBA designation" message
4255982 Must add functionality to dptutil to detect missing scsi channels
4257922 Sun log file selection in event broadcast window not documented
4259572 PSARC 1998/511 says all user commands must be installed in /usr/sbin
4260313 dptutil allows user to delete boot disk
4260858 Controller BLINKLEDs after installing 1.A7 driver
4260859 unknown drive type appearing in format after deleting/creating arrays
4261249 GUI and CLI should label unlabeled drives before exiting
4261649 HWRAID bootup message apppears 1 char per line in /var/adm/messages
4261729 cannot rebuild a failed array using the dptcfg utility
4262098 dptutil needs to be able to delete Hot Spare if d?b?t?d? device name
4262292 When partitioning a RAID-50 using format, entire array fails
4262318 dptcfg needs "maintenance shell" menu selection to run dptutil
4262640 PCI SERR: "Set System Config" causes commands to be lost to boot RAID controller
4266033 dpti2o: PCI SERR during boot of RAID5
4266496 RAID-5 set to Optimal prematurely - RAID-5 fails Verify
4266991 dpti2o: WARNING: interrupt level 4 not serviced while running sunvts
4267632 dpti2o: dpt_reset_hba only resets bus 0 on a scsi bus reset
4267728 remove d?b?t?d? naming from GUI (seen w/ "Set Sys Config" of deleted array)
4268596 need "premature Optimal" condition flagged by firmware
4268628 Internal cable cannot be attached to hwraid SX daughter card
4269552 dpti2o has dependency on year 1999
4269743 2.1GB Seagate drives may cause panics
4271225 cpu panic, possibly resulting from pci serr.
4271236 After getting ghd_timer_reset, was able to delete boot device from GUI
4271238 Logger must capture messages during installation of RAID boot device
4271491 blink_led 43, card sn 12-001028
4271948 Recoverable drive errors are marked Unrecoverable by SM02 FW
4275835 timeout of GUI/CLI commands hangs system
4276137 Disk status reported by firmware needs to match status reported by GUI
4276623 Recoverable errors cause drives to be marked "Failed" - SM02 FW
4277457 Flashing boot hwraid HBA with SM03 disables the controller
4281582 Reassign Block reassigns to wrong LUN - SM02
4282901 Sybase on RAID-5 or RAID-1 w/ 18GB drives hangs E450 - FCS pkg
4283942 dptelog: HBA: 0 reports controller error (Selection Timeout [10], 0)
4284453 privilege timeout error
4285806 FCODE probe-scsi-all does not "see" 3-channel RAID-10 - CD0 can't boot
4286019 SRC/P + Sybase11.9.2: WriteBack Cache Hangs Initializing DB
4289659 dptutil 2.0T no longer shows all conponent drives for RAID-10
4290134 You cannot build a raid 1 LSU with dptmgr if it is built from 10000 rpm drives.
4291821 dptmgr GUI dumps core when LANG env string > 12 chars
4292938 PCI SERR Panic with the latest Rev 6 of the HARDWARE RAID DPT SRC-P CARD
4295387 Data miscompares while using diskomizer with Hardware Raid PCI
4295392 WARNING messages when running dptutil or dptmgr
4295430 Unable to start dptmgr or run dptutil bogus exit messages/status's
4296188 need to increase delay after resetIOP in 1.B3 driver
4296342 Fixes needed to GUI online help.
4296647 TERM Power Voltage Low errors in dmesg & dptlog on (re)boot
4296734 Cannot use mouse when building RAID 5+0
4296738 32 bit driver package fails if pkgadd before 64bit driver package
4297193 dptutil help screen displays unsupported option
4297400 On-line help incorrectly states that warning condition is indicated by blue flag
4297565 Clicking "Build" button on failed RAID-5 gets BLINKLED 7 w/ dex 32 - SM0A
4298251 BLINKLED 0xE2 running dex32 and "dd"s with SM02
4299194 console is constantly filled with osdIOrequest messages...
4299294 SM02 - dptutil cached off command causes BLINKLED 7
4299305 data corruption running diskomizer after FW issues REASSIGN BLOCKS scsi command
4300002 dptutil needs "-a build" switch for CD0
4300006 RAID array(s) must be failed if DPT card cache line cannot be written out
4300041 Need to remove prefetch options from dptutil
4300068 Hotspare drive not being pulled in on impacted Raid 1 array
4300346 data corruption on drive with "Sense Key 4" errors - SM0C - BLINKLED 7
4300371 Nested timeouts can cause the driver to enter an indefinite wait.
4300680 PCI SERR panic with diskomizer and dptutil
4300904 SM0C/SM0D Privledge Timeout Panic with same-channel RAID-50 on boot
4300908 command dptutil from SRC/P card hangs
4301245 dptcfg while using CD0 install does not verify if disks selected exist
4301289 Get many "dpt_timeout_action" , cards fail to initialize
4301290 BLINKLED 7 with SM0D w/ "new verify" fix - running diskomizer on 3 RAID-5s
4301318 firmware hangs trying to spin up a drive
4301505 RAID-1 can't failover to Hot-Spare of same drive type - need FIN (FCS pkg)
4301545 2.0U dptutil and 2.0S dpteng cannot be opened under heavy load
4301548 system deadlock after command timeout
4301788 data miscompares with diskomizer on hwraid after drive failure
4302255 diskomizer reports data miscompares with hwraid after scsi recoverable errors
4302325 Priveleged Timeout Error during DEX32 script
4302469 dptutil verify option does not fix data inconsistencies
4302654 SM0C f/w dies with BLINK LED=3C after triggering bug 4301788
4302662 pulling drive from RAID-5 causes Privlege Timeout panic
4302663 If drive capacity can't be read, drive ID changed
4302665 Failed RAID-10 with MB06 cannot be brought back online without reboot
4302676 Privelege Timeout when RAID 1+0 fails
4302703 need Sun special error handling for ALL unrecoverable errors
4302715 Running dptutil or dptmgr will abort any formatting in progress on any card
4302775 Failed drive reinserted in RAID5 would not rebuild or associate properly in RAID
4303257 an array with a disk that was corrupted in format, dptutil and dptmgr will fail
4303444 BLINKLED 7 on SM0E+fixes (MB09) on 3-drive RAID-5 and diskomizer
4304079 "dpt_timeout_action" errors with MB09 on 14 drive RAID-5 and diskomizer
4304646 SRC/P + Sybase11.9.2: WriteBack Cache Hangs Initializing DB
4305320 Diskomizer misompares on SM0E while changing cache policy
4305516 cannot boot with src/p card installed
4305549 BLINKLED 7 when pulling drive from 3-drive RAID-5 & diskomizer - JH0E FW
4305642 "Phantom RAID" when adding 6 X 18GB drives to system.
4305900 Data corruption is seen almost immediately on a RAID 0 array
4305903 Sensekey 4 does not cause RAID 5/50 drive failure.
4305911 dptmgr can not delete an array with a drive marked as failed
4305926 diskomizer terminated with data corruption
4306244 NMI Proto board "hung" in constant NMI loop - latest JH0E FW
4306358 RAID 1+0 claims reconstructing, but no disk activity
4306364 1.B3 driver does not recover from forced blinkled 7 from UART
4306424 Change blinkled settings for codes 1F and lower from hard to soft - SM0E
4306651 BLINKLED 'BB'/SM0E running diskomizer on multiple raids concurrently on 1 board
4306970 PCI SERR on "max" config running JH0E and DEX32
4307455 dual level arrays do not start rebuilds after 1st reboot on SM0E and SME1
4307457 RAID50's go immediately optimal on reboot with SM0E and SME1
4307936 gui fails to initialize with fcs driver/gui and sm0e firmware
4309834 Reassign block command does not work
4309836 Event Log incomplete
4309838 Valid hotspares identical to array components are not protecting the arrays
4309841 Missing HRS in firmware after SM02
4309843 SUN:  new  HDM queue wraparound
4309847 rebuild rate while I/O is going on is too long on multilevel arrays!
4309850 Reassign Block event log block number is misleading
4309853 RAID-5 set to Optimal prematurely - RAID-5 fails
4309975 Profiling process breaks SM0E blinkled recover routine
4310780 Silent Data Miscompares with SME2 f/w and diskomizer & FCS packages
4310965 Synchronize cache does not flush all dirty pages in cache - SME2
4311182 BBU code needs to be fixed to tolerate minor configuration changes - SME2
4311253 Battery status never returns from Maintenance calibration
4311637 Have the controller hang on a BlinkLED when in degraded mode
4311645 put controller in write through mode when a redundant array goes degraded
4311897 data corruption on DS0A firmware
4312336 multiple drive failure on RAID5
4313881 miscompares in diskomizer after drive reinserted, post IOP reset - SME2
4313927 Panic in DPTI2o HBA driver
4314020 SME2 can hang with a blinking 1 if messaging unit is disabled
4315164 SME3 can produce IRQ solid and Blinking 1 when driver/FW in deadlock condition
4316890 Stack overflow in IO Error Recovery Task
4316891 Blinkled 0x3E due to parity error during LockDrive
4317244 errors during reconstruction of errored RAID5 read command corrupt PCB list
4317245 firmware hangs trying to spin up a drive
4317246 Blinkled E3 on MB09TC.ima code
4317247 1564U3 Hangs on 128k Random Reads (due to Scatter-Gather known issue)
4317248 Build and Rebuilds take too long during heavy I/O
4317250 Verify doesn't detect corruption past first 16 blocks of stripe for a RAID-1
4317251 Verify with repair now causes data corruption
4317252 RAID-1 or RAID-5 reassign can corrupt I/O error recovery PCB list
4321055 Leap year bug in firmware
4321494 data corruption due to task sleeping on RP allocation
4324468 failed RAID-0 drive with driver dpti2o.112.b will cause system crash
4324699 RAID-1 data corruption because of Domino errata - "CPQ bug"
4324700 FCS driver needs modifications to deal with Interim FW timing changes
4324701 1.B4 driver needs modifications to deal with Interim FW timing changes
4324740 On a RAID-0 when a drive is pulled datat corruption occures in 5 to 7 minutes
4326831 src/p board causes a timeout panic
4330518 Event logger is not reporting all events/status changes
4332761 I can't get out of the GUI, and the pulldown menu doesn't work.
4333005 Data Corruption on SRC/P card
4333499 dptutil CLI does not delete LUNs
4334143 Data corruption when swapping a smaller drive for a larger failed drive
4336048 Drive kicked out of array
4336737 Format cannot access dpt devices
4336819 SME4 data corruption on retry in presence of a medium or recoverable error
4337093 Blinkled7 with SME5
4337613 random files written to HW Raid controller filesystems have CRC errors
4337774 When we create a RAID1 it displays one of the drives as failed.
4338126 Random flagging of drives
4339189 DPT Raid 5 hot spare swap will not automatically rebuild failed drive.
4339651 when we fail a drive in R5 array, GUI displays two hotspares failed
4340294 Failure of 2nd parity group in a dual level array does not fail array
4340295 Broken arrays reported in GUI or card hang when pulling drives
4340297 RAID1 pending build shows target device as failed:  SetLogicalRaidState bug
4340298 Online-offline-online
4340299 Card hang with UART in looping HDM mailbox command timeouts
4340301 SME4 data corruption on in presence of a medium or recoverable error
4340303 Blinkled D5 on SME4 based code
4340305 Data corruption if reassign block command fails
4340307 TIDs changing across IOP reset
4340308 Blinkled 7 upon hotspare creation due to not deleting cache page
4340309 data corruption due to flush task sleeping on RP allocation
4340310 Leap year bug in firmware
4340311 errors occuring during reconstruction of errored RAID5 cause data corruption
4340313 reassign block to optimal raid-1 or 5 arrays corrupt the I/O error recovery
4340314 Stack overflow in IO Error Recovery Task
4340315 Blinkled 0x3E due to parity error during LockDrive
4340316 Disable interrupts while Event Log is transferred to host
4340317 SME3 can produce IRQ solid and Blinking 1 when driver/FW in deadlock condition
4340318 SME2 can hang with a blinking 1
4340319 SME3 Broken link causes miscompares in diskomizer
4340324 BBU bug allows dirty data to be lost after a power cycle or iop reset
4340394 Array does not restart build after power killed to disk pack
4341386 SRC/P panics system when under heavy load
4341924 Silent Data Corruption with SME6
4342215 DPT array not reporting correct capacity
4342576 Unable to extract stripe size info from a created array
4342584 Need to Document why card my be offlined and User Action that needs to be taken
4343742 BLINKLED 1,3 hang with SME7
4344009 Blinkled 1,3-hang
4344277 Unsupported option in dptutil man page
4344813 After strange display, can't clear raid configuration with "dptutil -Z".
4347070 Data Corruption with SME7 with 3 disk raid 5
4349107 Data inconsistencies when initiating rebuild
4351852 SME7 State hole problem:  IOP reset before failed drives can be updated
4352034 Dead Beef on SME7 under uneven read/write load

		- END -


