
         Ghostscript-2.6.1 Driver for Epson Stylus Color Printer

                                                     Kubo, Hiroshi



This is a Ghostscript-2.6.1 driver for MJ-700V2C. This may also work with
Epson Stylus color printer, though I have not tried.

This version supports micro-weave and shrink-dot mode.

LICENSE
-------

Please distribute this driver under GPL (GNU Public LICENSE).

How to install
--------------

1.  Append gdevmjc.mak to Makefile. If you want to set the default page 
    size to A4, follow the comments and rewrite the gdevmjc.mak.

2. Write 'mjc180', 'mjc360' and/or 'mjc720' at DEVICE_DEVS entry 
   in Makefile as:

  DEVICE_DEVS=mjc180.dev mjc360.de.dev mjc720.dev mj500c.dev

3. Just make as ordinary.

Examples
-------

% gs -sDEVICE=mjc360 -sOutputFile=tiger.mj gdevmjc.ps tiger.ps

% gs -sDEVICE=mjc360 -dMicroWeave=1 -dDotSize=1 -sOutputFile=tiger.mj gdevmjc.ps tiger.ps

% gs -sDEVICE=mjc720 -dMicroWeave=1 -dDotSize=0 -sOutputFile=tiger.mj gdevmjc.ps tiger.ps

% gs -sDEVICE=mjc360 -dColorComponent=3 -sOutputFile=tiger.mj gdevmjc.ps tiger.ps

% gs -sDEVICE=mj500c -sOutputFile=tiger.mj gdevmjc.ps tiger.ps

% gs -sDEVICE=mjc720 -dColorComponent=1 -sOutputFile=tiger.mj gdevmjc.ps tiger.ps


Comments, Suggestion and Bug Reports
------------------------------------

are welcomed. Please send E-mail to 'h-kubo@kuee.kyoto-u.ac.jp'.


Thanks
------

This driver can not exist without Ghostscript-2.6.1 distribution.
Especially, many parts of the driver are quoted from George Cameron's 
gdevcdj.c and Richard Brown's gdevescp.c . I thank you very much.

Mr. Tetsuya Nozaki and Mr. Kouichi Higashi told me how to control micro-weave
and shrink-dot mode.

Mr. Kwato sent me a K&R patch.

Mr. Kazutaka Kaga and Mr. Tetsuya Nozaki contributed 
"crystallizing algorithm" codes.

I also appriciate all the people who sent me bug reports and comments.


