Patch-ID# 113566-02
Keywords: StorEdge Enterprise Backup EBS 7.0 NetWorker Solstice
Synopsis: StorEdge EBS 7.0: Product Patch
Date: May/14/2003

Install Requirements: None                      
                      
Solaris Release: 7 8 9

SunOS Release: 5.7 5.8 5.9

Unbundled Product: StorEdge Enterprise Backup EBS

Unbundled Release: 7.0

Xref: 

Topic: StorEdge Enterprise Backup 7.0: Product Patch

Relevant Architectures: sparc

BugId's fixed with this patch: 4834837 4847536 4851406

Changes incorporated in this version: 4851406

Patches accumulated and obsoleted by this patch: 113563-01

Patches which conflict with this patch: 

Patches required with this patch: 

Obsoleted by: 

Files included with this patch: 

/usr/kernel/drv/lus
/usr/kernel/drv/lus32
/usr/kernel/drv/sparcv9/lus
/usr/lib/nsr/libscsi.so
/usr/lib/nsr/libscsi.so.1
/usr/lib/nsr/libscsi27.so.1
/usr/lib/nsr/libsji.so
/usr/lib/nsr/libsji.so.1
/usr/sbin/nsr/changers
/usr/sbin/nsr/dpy120
/usr/sbin/nsr/dpy210
/usr/sbin/nsr/hpflip
/usr/sbin/nsr/inquire
/usr/sbin/nsr/jbconfig
/usr/sbin/nsr/relem

Problem Description:

4851406 Need to combine the LTO-Gen2 and barcode reader fixes into one patch
 
(from 113566-01)
4847536 EBS 7.0 does not work with a L8/LTO Gen2 drive
 
(from 113563-01)
4834837 Labeling Op failed with L7/L8 autoloader when a barcode reader is installed

Patch Installation Instructions:
-------------------------------------------------------------------------
Refer to the Install.info file within the patch for instructions on
using the generic 'installpatch'/patchadd and 'backoutpatch'/patchrm 
scripts/binaries provided with each patch.  Any other special or 
non-generic installation instructions should be described below.
-------------------------------------------------------------------------

Special Install Instructions:
------------------------------------------------------------------------------
 
Configuring Sun StorEdge L7 and StorEdge L8 Tape Libraries in Sun StorEdge(TM) 
Enterprise Backup software (EBS) 7.0
 
Chapter 3 of the Sun StorEdge EBS Version 7 Installation Guide covers the 
procedure for installing and configuring an "Autochanger" device with EBS.
As noted in the documentation, the "jbconfig" command is used to perform the
configuration.  Both the StorEdge L7 and StorEdge L8 tape libraries can be
ordered with an optional bar code reader (i.e., Option# SG-XBARCODE-L7 or 
SG-XBARCODE-L8).  With this patch installed, Sun StorEdge EBS will be able
to accurately detect the presence of a barcode reader and set the appropriate
defaults during jukebox configuration.  After the installation of this patch
it may be necessary to re-run "jbconfig;" this will be true, if you have a 
StorEdge L7 or L8 tape library with the barcode reader option.
 
------------------------------------------------------------------------------
 
The following are BugTraq IDs considered fixed in this patch:
 
Sun Bug ID   Legato Bug ID   Description
----------   -------------   ---------------------------------------------------
4851406      LGTpa53708      PORT of LGTpa49931 into LGTpa53482
 
(from 113566-01)
4847536      LGTpa53482      jbconfig incorrectly detects LTO ultrium drive type
 
(from 113563-01)
4834837      LGTpa49931      L8 jbconfig message "barcode reading to on . . ." in all cases

README -- Last modified date:  Wednesday, May 14, 2003

