## About the Default State of the System

After you complete the basic configuration tasks described in the Sun StorEdge 6920 System Getting Started Guide, your system has the following characteristics:

- The Ethernet connection is cabled to a host or a gateway on the local area network (LAN).
- A service console is connected.
- The system is powered up.
- The IP address and netmask has been entered.
- Initial setup of the system has been completed.
- One data host, an initiator, is assigned to the DEFAULT storage domain.
- The DEFAULT storage domain uses one storage pool named Default.
- All storage ports are assigned to the Default storage pool.
- The Default storage pool uses the specifications of the Default storage profile:

Storage Attribute | Value
--- | ---
RAID level | RAID-5
Segment size | 64 Kbyte
Read-ahead mode | On/Enabled
Number of drives | Variable
Array type | Best Available Match: Bandwidth
Dedicated hot spare | No
Virtualization strategy | Stripe
Stripe size | 1 Mbyte

### Related Topics

- About Provisioning Storage
- About Physical Storage Elements
- About Logical Storage Elements