## Restoring the System After a Full Shutdown

If the system has been powered off using the full shutdown procedure, you must go to the location of the system and perform the following procedure:

1. Open the front door and back door of the base cabinet and any expansion cabinets.
2. Remove the front trim panel from each cabinet.
3. Verify that the key switches located at the bottom front of each cabinet are in the Standby position.
4. At the bottom front and bottom back of each cabinet, press the AC power sequencer circuit breaker to Off.
5. Verify that the AC power cables are connected to the correct AC outlets.
6. At the bottom front and bottom back of the each cabinet, press the Local/Off/Remote switch to Remote.
7. At the bottom front and bottom back of the each cabinet, press the AC power sequencer circuit breakers to On.

The power status LEDs on both the front and back panel illuminate in the following order, showing the status of the front power sequencer:

- The main AC power LED lights when the power is applied to the cabinet.
- Sequencer Stage 1
- Sequencer Stage 2

8. Wait approximately one minute.
9. Go to the back of the system and locate the power switch for the Storage Service Processor.
10. Press the power switch off and then press it on again.
11. Verify that all components have only green LEDs lit.
12. Replace the front trim panels and close all doors.

The system is now operating and supports the remote power-on procedure.

### Related Topics

- Powering the System On and Off