## Continuous Volume Verify Page

This page allows you to schedule or stop the Continuous Volume Verify utility and to display a device summary of Continuous Volume Verify results for all arrays on which Continuous Volume Verify is enabled.

This page includes the following sections:

- Select Function
- Schedule Volume Verify
- Stop Verify
- Device Summary

### Select Function

This drop-down list enables you to select the continuous volume verify function to be performed.

Field | Description
Schedule Volume Verify | Select to configure options to schedule Continuous Volume Verify to run.
Stop Verify | Select to stop Continuous Volume Verify operations on all arrays.
Device Summary | Click to display Continuous Volume Verify results for each monitored array.

### Schedule Volume Verify

This page enables you to define parameters to schedule continuous volme verify operations.

Field | Description
Activate vol-verify | Select to enable the Continuous Volume Verify utility. Volumes are verified one at a time on a rotational basis for all enabled arrays.
Run with `fix' option | Select to allow Continuous Volume Verify to automatically fix volume errors. Note: The fix option might mistakenly fix parity on bad blocks. Consult your service representative for details.
Run on same array at most every X days | Select the maximum frequency at which you want Continuous Volume Verify to run on the same array.
Start volVerify only in these time periods | For each day of the week you want Continuous Volume Verify to run, select the hour during which Continuous Volume Verify will run. To run Volume Verify continuously during the corresponding day, select ALL THE TIME.
Execution Rate | Select the rate at which you want Continuous Volume Verify to run on all arrays. Higher execution rates result in lower array I/O performance.
Default Array Password | Enter the default password for system arrays. The default password is defined using the Configuration Options function.
Reset Time Periods | Click to clear all selected time periods.
Save Options | Click to save newly configured settings.

### Stop Verify

This function allows you to stop all Continuous Volume Verify processes.

Field | Description
Status | The current status of the Stop Verify function: Not Running, Running, Done.
Log: Display Process-Stop Log | Click to display the log file for the Stop Verify function.
Stop All Vol-Verify Processes | Click to stop all Continuous Volume Verify processes.

### Device Summary

This function allows you to display Continuous Volume Verify results for all arrays on which it is enabled.

Field | Description
Host | The name of the host device for the array.
Device | The name of the array. Click to display the Maintain Decice page for the array.
Verify | Whether Continuous Volume Verify is enabled for the device.
Volume | The name of the volume for which results are displayed.
Start Date | The date and time when Continuous Volume Verify started on the volume.
End Date | The date and time when Continuous Volume Verify ended on the volume.
Duration | The length of time required to complete Continuous Volume Verify on the volume.
Errors | The number of errors detected.
Status | The current status of Continuous Volume Verify on the device.

### Related Topics

- Using Continuous Volume Verify
- Scheduling Continuous Volume Verify
- Starting and Stopping Continuous Volume Verify for a Specific Array
- Stopping Continuous Volume Verify for All Devices
- Displaying Continuous Volume Verify Results