## Switch Data Page

This page allows you to display Fibre Channel (FC) counter values.

Field | Description
--- | ---
Select Switch | Select the Fibre Channel device for which you want to display counter values.
Display | Click to display counter values for the selected Fibre Channel device.
Set Baseline | Click to store the current counter values as the reference values from which the counters will increment.
Total | Click to display the sum of the baseline counter values and the current counter values.

### Switch Counter Values Table

This table displays various counters for the Fibre Channel (FC) ports.

Field | Description
--- | ---
Name | The IP address of the device in which the Fibre Channel ports reside.
Component | The Fibre Channel port number.
Link | The number of Fibre Channel link resets.
Sig | The number of Fibre Channel signal errors.
Seq | The number of Fibre Channel sequence delimiter errors.
CRC | The number of Fibre Channel Cyclic Redundancy Check errors.
Sync | The number of times that the Fibre Channel has lost synchronization.
InvTxW | The number of times that an invalid transmission has been detected on the Fibre Channel using 8b/10b encoded-word detection.
Inframes | The number of frames received by the Fibre Channel port.
Outframes | The number of frames sent by the Fibre Channel port.

### Related Topics

- Displaying Switch Counter Values