## Using an External Modem for the Sun StorEdge Remote Response Service

You might find that in your country the modem on the Storage Service Processor accessory tray does not work. To use an external modem:

1. Disconnect the RJ-45 cable (#530-3205-01) from the Management Interface Card (MIC) #2 DB-9/RJ-45 serial port of the Storage Service Processor.

Note -

Leave the other end of this cable attached to the AUX port on the Storage Service Processor accessory tray.

2. Reconnect the RJ-45 cable to the AUX port on the interior face of the Storage Service Processor panel.
3. Connect the external modem to the AUX port of the Storage Service Processor panel.

### Related Topics

- About the Sun StorEdge Remote Response Service
- Enabling the Sun StorEdge Remote Response Service