## FC Port Details Page

This page displays the properties associated with the selected FC port, including statistics and subreports.

Field | Indicates
--- | ---
Link State | The current link state: Online, Failure, or Offline.
Hardware State | The current state of the hardware: Active Link Down Unknown Failed Loopback No Media Bypassed Transmit Fault
Port ID | The Fibre Channel nPort identifier (ID).
WWN | The port worldwide name (WWN).
Node WWN | The node worldwide name (WWN).
Port Type | The Fibre Channel port type: nPort or nlPort.
FC Unit Type | The Fibre Channel unit type, typically HBA (host bus adapter).
Module Type | The module type: 1 GBIC, 2 GBIC, or Missing GBIC.
Uptime | The current Fibre Channel port uptime, in days, hours, minutes, and seconds.
FC ID Configured | The configured Fibre Channel identifier.
FC ID Operational | The operational Fibre Channel identifier.
FC Speed Configured | The configured Fibre Channel speed: Auto, 1 Gbyte, or 2 Gbytes. If this setting is Auto, the operational speed is either 1 or 2, depending on the installed hardware (GBIC). If this setting is 2, and the GBIC supports 1 only, the operational speed is 1. Storage users can change this setting.
FC Speed Operational | The operational Fibre Channel speed: 1 Gbyte/second or 2 Gbytes/second.
GBIC Class Capable | The Fibre Channel class capabilities, consisting of a combination of: Class 1 Class 2 Class 3 Class 4 Class 5 Class 6
FC Class Operational | The operational Fibre Channel class, consisting of: Class 1 Class 2 Class 3 Class 4 Class 5 Class 6
Protocol Capable | The protocol support for this Fibre Channel. This can be Loop, Fabric, or SCSI (small computer system interface), in one of the following combinations: IP over FC SCSI - FCP FC - VI
Protocol Operational | The currently configured protocols, including Loop, Fabric, and SCSI, in one of the following combinations: IP over FC SCSI - FCP FC - VI

The Statistics table displays the following information for the specified FC port:

Field | Indicates
--- | ---
Error Count | The current error count associated with this Fibre Channel port.
Write Commands | The current number of write commands to this Fibre Channel port.
Read Commands | The current number of read commands from this Fibre Channel port.
Bytes Written | The total number of bytes written from this Fibre Channel port.
Bytes Read | The total number of bytes read to this Fibre Channel port.
Loop Reset Events | The number of loop-reset events on this Fibre Channel port.
Loop Down Events | The number of loop-down events on this Fibre Channel port.

The subreports table provides additional information on initiators. Click an item to see its details.

Type | Quantity
--- | ---
Initiators | The number of initiators associated with this Fibre Channel port.

### Related Topics

- About FC Ports