## Running Tests From a Topology View

To initiate tests from a topological view:

1. Go to the Sun Web Console and click Storage Automated Diagnostic Environment.
2. Click Diagnose > Diagnostic Tests > Test from Topology.

The Test from Topology page is displayed.

3. Click the device you want to test.

A list of tests for the selected device is displayed.

4. Click the name of the test you want to run on the device.

Required test parameters are displayed for the selected test. For parameter descriptions, see Reference: Diagnostic Test Options.

5. Complete the required test parameter fields.
6. Click Start Test.

A confirmation request is displayed.

7. Click OK to proceed with the test.

While a test is running, the Test Manager window reports the status of the test. See Using Test Manager for more information.

After the test has completed its run, an email message is sent to the specified email recipient.

### Related Topics

- About Diagnostic Tests
- Running Tests From a Device List
- Reference: Diagnostic Test Options
- Managing Diagnostic Tests
- Setting Test Defaults