## FRU Reports Page

You can use the FRU Reports page to generate each of the following FRU report types:

- Detailed FRU Report
- FRU Summary (Health Concerns) Report
- FRU Model Summary (by Device Name) Report
- FRU Model Summary (by Device Type) Report
- Sun Storage 6020 Array Uptime Report
- Temperature Report

Field | Description
--- | ---
Report-Set Status | The status and the date and time of the last generated report; for example, Done/Wed Oct 29 09:40:09 MST 2003
Generate New Report-Set | Click to update all available reports. From the reports list, you can select and display a report, archive it for future retrieval, or send it to an email recipient.
Select | Select the check box that corresponds to the report you want to archive or send to an email recipient.
Report Name | List of the reports that are available. Reports include: Detailed FRU - A detailed list of FRUs. You can filter the FRU report by administration group, device type, or FRU type. FRU Summary (Health Concerns) - Displays only FRUs that are not in a normal state. FRU Model Summary (by Device Name) - Displays FRU models by device name. FRU Model Summary (by Device Type) - Displays FRU models by device type. Sun Storage 6020 Array Uptime - Displays the number of days since each array was rebooted. Temperature Report - Displays the FRU temperature distribution. It can be used to identify and isolate hot FRUs.
Email Selected | Type the address of the email recipient for a selected report, and click Email Selected.

### Detailed FRU Report

The elements of the Detailed FRU report are as follows.

Field | Description
--- | ---
Name | Name of the host device.
Device | Type of the host device; for example, array00 device type might be 6020.
FRU Type | Component FRU; for example, controller, disk, loop card.
FRU | FRU identifier number.
Vendor | FRU vendor; for example, Seagate disks.
Model | The model number of the FRU.
Serial | The serial number of the FRU.
Revision | `SUNWstade` or `SUNWstads` package revision number.
Status | Current device status; for example, ready-enabled, normal, or Standing By

### FRU Summary (Health Concerns) Report

The elements of the FRU Summary (Health Concerns) report are as follows.

Field | Description
--- | ---
Name | Name of the host device.
Device | Type of the host device; for example, array00 device type may be 6020.
FRU Type | Component FRU; for example, controller, disk, loop card.
FRU | FRU identifier number.
Vendor | FRU vendor: for example, Seagate disks.
Model | The model number of the FRU.
Serial | The serial number of the FRU.
Revision | `SUNWstade` or `SUNWstads` package revision number.
Status | Current device status; for example, ready-enabled, normal or Standing By.

### FRU Model Summary (by Device Name) Report

The elements of the FRU Model Summary (by Device Name) report are as follows.

Field | Description
--- | ---
Name | Name of the host device.
Device | Type of the host device; for example, array00 device type might be 6020.
FRU Type | Component FRU; for example, controller, disk, loop card.
Vendor | FRU vendor; for example, Seagate disks.
Model | The model number of the FRU.
Revision | `SUNWstade` or `SUNWstads` package revision number.
Count | The number of events associated with the FRU.

### FRU Model Summary (by Device Type) Report

The elements of the FRU Model Summary (by Device Type) report are as follows.

Field | Description
--- | ---
Device | Type of the host device; for example, array00 device type might be 6020.
FRU Type | Component FRU; for example, controller, disk, loop card.
Vendor | FRU vendor; for example, Seagate disks.
Model | The model number of the FRU.
Revision | `SUNWstade` or `SUNWstads` package revision number.
Count | The number of events associated with the FRU.

### Sun Storage 6020 Array Uptime Report

The elements of the Sun Storage 6020 Array Uptime report are as follows.

Field | Description
--- | ---
Type | Type of the host device; for example, 6020.
Device Name | The name of the host device.
Days Since Last Reboot | The number of days since the array was rebooted.

### Temperature Report

The elements of the Temperature report are as follows.

Field | Description
--- | ---
Device Name | The name of the host device.
Low | The lowest temperature of the device since the last Temperature report.
High | The highest temperature of the device since the last Temperature report.
Spread | The difference between the low and high temperatures since the last Temperature report.

### Related Topics

- Using FRU Reports
- Displaying a FRU Report
- Sending a FRU Report to an Email Recipient
- Archiving a FRU Report
- Customizing a FRU Report
- Scheduling a FRU Report
- Displaying an Archived FRU Report
- Deleting an Archived FRU Report
- Comparing Archived FRU Reports