## Test from List Page

This page allows you to initiate a diagnostic test for a listed system device.

Field | Description
--- | ---
Device | The device for which the test is to be run.
Diag Type | The communication method used for the test. InBand is performed in the data path; OutOfBand is performed in the non-data Ethernet channel.
Status | The status of the device test.
Run Test | A list of tests that you can run for each system device. Click a test name to initiate that test.

### Related Topics

- Reference: Diagnostic Test Options
- se2_configcheck Test Options
- 6020-VolVerify Test Options
- 6020-loop Test Options
- About Diagnostic Tests
- Running Tests From a Topology View
- Running Tests From a Device List
- Managing Diagnostic Tests
- Setting Test Defaults