Patch-ID# 118216-01
Keywords: storedge 5210
Synopsis: StorEdge 5210 NAS software update
Date: Sep/02/2004


Install Requirements: None                      
                      
Solaris Release: 

SunOS Release: 

Unbundled Product: StorEdge 5210

Unbundled Release: 4.02

Xref: 

Topic: StorEdge 5210 NAS
NOTE:   This patch updates the StorEdge 5120 NAS system software

Relevant Architectures: 

BugId's fixed with this patch: 5032231 5043211 5043485 5043915 5043941 5044940 5046060 5051146 5051432 5053915 5055817 5057720 5060256 5062400 5062401 5064710 5065380 5065523 5066146 5066161 5066287

Changes incorporated in this version: 5044940 5046060 5051432 5065380 5065523 5032231 5055817 5060256 5064710 5066146 5066161 5066287 5043211 5043485 5043915 5043941 5051146 5053915 5057720 5062400 5062401

Patches accumulated and obsoleted by this patch: 

Patches which conflict with this patch: 

Patches required with this patch: 

Obsoleted by: 

Files included with this patch: 

	verdeGEN.rom
NF402B160.IMG

Problem Description:

5044940 During fstress the unit was unable to handle the load.
 
5046060 Unit CPU went to 100% during testing
 
5051432 Fstress from four hosts ... causes the ethernet to stop
 
5065380 fstress udp mode msg_extract_opaque: offset + len > mlen
 
5065523 TCP mode in fstress causes NFS server 5210-2 not responding
 
5032231 Logical drive 1 hot-spare fail when JBOD is removed.
 
5055817 Performance issue with SNMP GETs/Walks
 
5060256 em_refill_mbufs_daemon: mbuf allocation failed.
 
5064710 System crashed while changing NTP configuration
 
5066146 fstress latency time
 
5066161 NAS looses connection during high iops in fstress...
 
5066287 system activity on the NAS is suspended in fstress specsfs97 tcp mode
 
5043211 Add a legend indicating what the different color/shadings of the
	HDD icons mean
 
5043485 Change the "Failed not rebuilt" status indicator in the gui from
	amber to red
 
5043915 Change the 'Failed not rebuilt' tag to 'Unconfigured'
 
5043941 Sync the status tags between the table and the graphical
	representation.
 
5051146 Packet counters are negative
 
5053915 Head rebooted while disconnected from the JBOD can't recover via
	the web GUI.
 
5057720 smbtorture RW3 test fails
 
5062400 System displays cache message on boot up
 
5062401 After using the menu silence alarm it remains unavailable after
	reboot.

Patch Installation Instructions:
--------------------------------
 
Installation instructions are in file install.txt
in the same directory as this file.

Special Install Instructions:
-----------------------------
 
None.

README -- Last modified date:  Thursday, September 2, 2004

