ATM-FORUM-MIB




DEFINITIONS ::= BEGIN

IMPORTS
        Counter, IpAddress              FROM RFC1155-SMI
        DisplayString                   FROM RFC1213-MIB
        TRAP-TYPE                       FROM RFC-1215
        OBJECT-TYPE                     FROM RFC-1212
        enterprises                     FROM RFC1155-SMI;



TruthValue ::= INTEGER { true(1), false(2) }

ClnpAddress ::= OCTET STRING (SIZE (1..21))

AtmServiceCategory ::=
        INTEGER {
                other(1),
                cbr(2),
                rtVbr(3),
                nrtVbr(4),
                abr(5),
                ubr(6)
        }


NetPrefix ::= OCTET STRING (SIZE (8 .. 13))




atmForum                OBJECT IDENTIFIER ::= { enterprises 353 }

atmForumAdmin           OBJECT IDENTIFIER ::= { atmForum 1 }
atmfTransmissionTypes   OBJECT IDENTIFIER ::= { atmForumAdmin 2 }
atmfMediaTypes          OBJECT IDENTIFIER ::= { atmForumAdmin 3 }
atmfTrafficDescrTypes   OBJECT IDENTIFIER ::= { atmForumAdmin 4 }
atmfSrvcRegTypes        OBJECT IDENTIFIER ::= { atmForumAdmin 5 }

atmForumUni             OBJECT IDENTIFIER ::= { atmForum 2 }
atmfPhysicalGroup       OBJECT IDENTIFIER ::= { atmForumUni 1 }
atmfAtmLayerGroup       OBJECT IDENTIFIER ::= { atmForumUni 2 }
atmfAtmStatsGroup       OBJECT IDENTIFIER ::= { atmForumUni 3 }
atmfVpcGroup            OBJECT IDENTIFIER ::= { atmForumUni 4 }
atmfVccGroup            OBJECT IDENTIFIER ::= { atmForumUni 5 }
atmfAddressGroup        OBJECT IDENTIFIER ::= { atmForumUni 6 }
atmfNetPrefixGroup      OBJECT IDENTIFIER ::= { atmForumUni 7 }
atmfSrvcRegistryGroup   OBJECT IDENTIFIER ::= { atmForumUni 8 }
atmfVpcAbrGroup         OBJECT IDENTIFIER ::= { atmForumUni 9 }
atmfVccAbrGroup         OBJECT IDENTIFIER ::= { atmForumUni 10 }
atmfAddressRegistrationAdminGroup OBJECT IDENTIFIER ::= { atmForumUni 11 }



atmfUnknownType         OBJECT IDENTIFIER ::= { atmfTransmissionTypes 1}
atmfSonetSTS3c          OBJECT IDENTIFIER ::= { atmfTransmissionTypes 2 }
atmfDs3                 OBJECT IDENTIFIER ::= { atmfTransmissionTypes 3 }
atmf4B5B                OBJECT IDENTIFIER ::= { atmfTransmissionTypes 4 }
atmf8B10B               OBJECT IDENTIFIER ::= { atmfTransmissionTypes 5 }
atmfSonetSTS12c         OBJECT IDENTIFIER ::= { atmfTransmissionTypes 6 }
atmfE3                  OBJECT IDENTIFIER ::= { atmfTransmissionTypes 7 }
atmfT1                  OBJECT IDENTIFIER ::= { atmfTransmissionTypes 8 }
atmfE1                  OBJECT IDENTIFIER ::= { atmfTransmissionTypes 9 }

atmfMediaUnknownType    OBJECT IDENTIFIER ::= { atmfMediaTypes 1 }
atmfMediaCoaxCable      OBJECT IDENTIFIER ::= { atmfMediaTypes 2 }
atmfMediaSingleMode     OBJECT IDENTIFIER ::= { atmfMediaTypes 3 }
atmfMediaMultiMode      OBJECT IDENTIFIER ::= { atmfMediaTypes 4 }
atmfMediaStp            OBJECT IDENTIFIER ::= { atmfMediaTypes 5 }
atmfMediaUtp            OBJECT IDENTIFIER ::= { atmfMediaTypes 6 }


atmfNoDescriptor        OBJECT IDENTIFIER ::= { atmfTrafficDescrTypes 1 }
atmfPeakRate            OBJECT IDENTIFIER ::= { atmfTrafficDescrTypes 2 }

atmfNoClpNoScr          OBJECT IDENTIFIER ::= { atmfTrafficDescrTypes 3 }
        -- Parameter #1 - peak cell rate in cells/second for CLP=0+1 traffic
        -- Parameter #2 - CDVT in tenths of microseconds
        -- Parameters #3, #4 and #5 are unused

atmfClpNoTaggingNoScr   OBJECT IDENTIFIER ::= { atmfTrafficDescrTypes 4 }
atmfClpTaggingNoScr     OBJECT IDENTIFIER ::= { atmfTrafficDescrTypes 5 }

atmfNoClpScr            OBJECT IDENTIFIER ::= { atmfTrafficDescrTypes 6 }
        -- Parameter #1 - peak cell rate in cells/second for CLP=0+1 traffic
        -- Parameter #2 - sustainable cell rate in cells/second for CLP=0+1 traffic
        -- Parameter #3 - maximum burst size in cells
        -- Parameter #4 - CDVT in tenths of microseconds
        -- Parameter #5 - unused

atmfClpNoTaggingScr     OBJECT IDENTIFIER ::= { atmfTrafficDescrTypes 7 }
        -- Parameter #1 - peak cell rate in cells/second for CLP=0+1 traffic
        -- Parameter #2 - sustainable cell rate in cells/second for CLP=0 traffic
        -- Parameter #3 - maximum burst size in cells
        -- Parameter #4 - CDVT in tenths of microseconds
        -- Parameter #5 - unused

atmfClpTaggingScr       OBJECT IDENTIFIER ::= { atmfTrafficDescrTypes 8 }
        -- Parameter #1 - peak cell rate in cells/second for CLP=0+1 traffic
        -- Parameter #2 - sustainable cell rate in cells/second for CLP=0
        --      traffic, excess tagged as CLP=1
        -- Parameter #3 - maximum burst size in cells
        -- Parameter #4 - CDVT in tenths of microseconds
        -- Parameter #5 - unused

atmfClpNoTaggingMcr      OBJECT IDENTIFIER ::= { atmfTrafficDescrTypes 9 }
        -- Parameter #1 - peak cell rate in cells/second
        -- parameter #2 - CDVT in tenths of microseconds
        -- Parameter #3 - minimum cell rate in cells/second
        -- Parameter #4 - unused
        -- Parameter #5 - unused



AtmAddress ::= OCTET STRING (SIZE (0 .. 32))



atmfPortTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF AtmfPortEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
                "A table of physical layer status and parameter
                information for the ATM Interface's physical interface."
        ::= { atmfPhysicalGroup 1 }

atmfPortEntry OBJECT-TYPE
        SYNTAX  AtmfPortEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
                "An entry in the table, containing information about
                the physical layer of an ATM Interface."
        INDEX   { atmfPortIndex }
        ::= { atmfPortTable 1 }

AtmfPortEntry ::=
        SEQUENCE {
                atmfPortIndex
                        INTEGER,
                atmfPortAddress
                        AtmAddress,
                atmfPortTransmissionType
                        OBJECT IDENTIFIER,
                atmfPortMediaType
                        OBJECT IDENTIFIER,
                atmfPortOperStatus
                        INTEGER,
                atmfPortSpecific
                        OBJECT IDENTIFIER,
                atmfPortMyIfName
                        DisplayString,
                atmfPortMyIfIdentifier
                        INTEGER

        }

atmfPortIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..2147483647)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The value of 0 which has the special meaning of
                identifying the ATM Interface over which this message
                was received."
        ::= { atmfPortEntry 1 }

atmfPortAddress OBJECT-TYPE
        SYNTAX  AtmAddress
        ACCESS  read-only
        STATUS  obsolete
        DESCRIPTION
                "This object should not be implemented except as
                required for backward compatibility with version 2.0
                of the UNI specification. The Address Group, defined
                in theAddress Registration MIB should be used instead."
        ::= { atmfPortEntry 2 }

atmfPortTransmissionType OBJECT-TYPE
        SYNTAX  OBJECT IDENTIFIER
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
                "This object should not be implemented except as
                required for backward compatibility with version 3.1
                of the UNI specification. Appropriate Network Management
                MIBs should be used instead."
        ::= { atmfPortEntry 3 }

atmfPortMediaType OBJECT-TYPE
        SYNTAX  OBJECT IDENTIFIER
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
                "This object should not be implemented except as
                required for backward compatibility with version 3.1
                of the UNI specification. Appropriate Network Management
                MIBs should be used instead."
        ::= { atmfPortEntry 4 }

atmfPortOperStatus OBJECT-TYPE
        SYNTAX  INTEGER {
                        other(1),
                        inService(2),
                        outOfService(3),
                        loopBack(4)
                }
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
                "This object should not be implemented except as
                required for backward compatibility with version 3.1
                of the UNI specification. Appropriate Network Management
                MIBs should be used instead."
        ::= { atmfPortEntry 5 }

atmfPortSpecific OBJECT-TYPE
        SYNTAX  OBJECT IDENTIFIER
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
                "This object should not be implemented except as
                required for backward compatibility with version 3.1
                of the UNI specification. Appropriate Network Management
                MIBs should be used instead."
        ::= { atmfPortEntry 6 }

atmfPortMyIfName OBJECT-TYPE
        SYNTAX  DisplayString
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "A textual name of this interface. If this system is
                manageable through SNMP, and supports the object
                ifName, the value of this object must be identical
                with that of ifName for the ifEntry of the lowest
                level physical interface for this port. This interface
                must be uniquely named on this system to distinguish
                parallel links with a neighboring system.  If this
                interface does not have a textual name, the value of
                this object is a zero length string."
        ::= { atmfPortEntry 7 }

atmfPortMyIfIdentifier OBJECT-TYPE
        SYNTAX INTEGER (0..2147483647)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "A unique value for each ATM interface. The scheme used to
                number the ATM interfaces on an ATM device is
                implementation specific. One way to generate this value is
                to use the ifIndex that an SNMP manager would use to
                identify the port. This interface must be uniquely numbered
                on this system to distinguish parallel links with a
                neighboring system."
        ::= { atmfPortEntry 8 }

atmfMyIpNmAddress OBJECT-TYPE
        SYNTAX  IpAddress
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "An IP Address to which a Network Management Station
                can send Network Management protocol messages, e.g. SNMP
                messages to UDP port 161, in order to access network
                management information concerning the operation of the
                ATM device local to this IME. If this object is supported,
                but the Network Management Agent has not been configured with
                an IP Address, the IME should return 0.0.0.0."
        ::= { atmfPhysicalGroup 2 }

atmfMyOsiNmNsapAddress OBJECT-TYPE
        SYNTAX  ClnpAddress
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "An NSAP Address to which a Network Management Station
                can send Network Management protocol messages in order
                to access network management information concerning
                the operation of the ATM device local to this IME.
                If this object is supported,
                but the Network Management Agent has not been configured with
                an NSAP Address, the IME should return 0.0.0.0"
         ::= { atmfPhysicalGroup 3 }

atmfMySystemIdentifier OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE (6))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "A 48 bit identifier, taken from the IEEE universally
                administered MAC address space, which uniquely
                identifies the ATM device local to this IME."
         ::= { atmfPhysicalGroup 4 }



atmfAtmLayerTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF AtmfAtmLayerEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
                "A table of ATM layer status and parameter information
                for the ATM Interface."
        ::= { atmfAtmLayerGroup 1 }

atmfAtmLayerEntry OBJECT-TYPE
        SYNTAX  AtmfAtmLayerEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
                "An entry in the table, containing information about
                the ATM layer of an ATM Interface."
        INDEX   { atmfAtmLayerIndex }
        ::= { atmfAtmLayerTable 1 }

AtmfAtmLayerEntry ::=
        SEQUENCE {
                atmfAtmLayerIndex
                        INTEGER,
                atmfAtmLayerMaxVPCs
                        INTEGER,
                atmfAtmLayerMaxVCCs
                        INTEGER,
                atmfAtmLayerConfiguredVPCs
                        INTEGER,
                atmfAtmLayerConfiguredVCCs
                        INTEGER,
                atmfAtmLayerMaxVpiBits
                        INTEGER,
                atmfAtmLayerMaxVciBits
                        INTEGER,
                atmfAtmLayerUniType
                        INTEGER,
                atmfAtmLayerUniVersion
                        INTEGER,
                atmfAtmLayerDeviceType
                        INTEGER,
                atmfAtmLayerIlmiVersion
                        INTEGER,
                atmfAtmLayerNniSigVersion
                        INTEGER,
                atmfAtmLayerMaxSvpcVpi
                        INTEGER,
                atmfAtmLayerMaxSvccVpi
                        INTEGER,
                atmfAtmLayerMinSvccVci
                        INTEGER
        }

atmfAtmLayerIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..2147483647)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The value of 0 which has the special meaning of
                identifying the ATM Interface over which this message
                was received."
        ::= { atmfAtmLayerEntry 1 }

atmfAtmLayerMaxVPCs OBJECT-TYPE
        SYNTAX  INTEGER (0..4096)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The maximum number of switched and permanent VPCs
                supported on this ATM Interface. For virtual interfaces
                (i.e. Virtual Path Connections), the maximum number of VPCs
                PNNI may communicate over is set to zero."
        ::= { atmfAtmLayerEntry 2 }

atmfAtmLayerMaxVCCs OBJECT-TYPE
        SYNTAX  INTEGER (0..268435456)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The maximum number of switched and permanent VCCs
                supported on this ATM Interface."
        ::= { atmfAtmLayerEntry 3 }

atmfAtmLayerConfiguredVPCs OBJECT-TYPE
        SYNTAX  INTEGER (0..4096)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The number of permanent VPCs configured for use on
                this ATM Interface. For virtual interfaces (i.e. Virtual Path
                Connections used by PNNI), the maximum number of VPCs
                is set to zero."
       ::= { atmfAtmLayerEntry 4 }

atmfAtmLayerConfiguredVCCs OBJECT-TYPE
        SYNTAX  INTEGER (0.. 268435456)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The number of permanent VCCs configured for use on
                this ATM Interface."
        ::= { atmfAtmLayerEntry 5 }

atmfAtmLayerMaxVpiBits OBJECT-TYPE
        SYNTAX  INTEGER (0..12)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The maximum number of active VPI bits on this ATM Interface.
                For virtual interfaces (i.e. Virtual Path Connections used by PNNI),
                this value has no meaning and is set to zero."
        ::= { atmfAtmLayerEntry 6 }

atmfAtmLayerMaxVciBits OBJECT-TYPE
        SYNTAX  INTEGER (0..16)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The maximum number of active VCI bits on this ATM Interface."
       ::= { atmfAtmLayerEntry 7 }

atmfAtmLayerUniType OBJECT-TYPE
        SYNTAX  INTEGER { public(1), private(2) }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The type of the ATM device, either public or private."
        ::= { atmfAtmLayerEntry 8 }

atmfAtmLayerUniVersion OBJECT-TYPE
        SYNTAX  INTEGER {
                        version2point0(1),
                        version3point0(2),
                        version3point1(3),
                        version4point0(4),
                        unsupported(5)
                }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "An indication of the latest version of the ATM Forum UNI
                Signalling Specification that is supported on this ATM
                Interface.  If this value is not present, a version of the UNI
                earlier than 3.1 is supported.

                If the peer IME's value of this object is the same as,
                or later than the local IME's value, then the version
                corresponding to the local IME's value should be
                attempted.  Otherwise, if the peer IME's value of this
                object is earlier, and supported locally, then the
                local IME should attempt the version corresponding to
                the peer IME's value.  Otherwise, compatibility of the
                two IMEs cannot be assumed."
        ::= { atmfAtmLayerEntry 9 }

atmfAtmLayerDeviceType OBJECT-TYPE
        SYNTAX  INTEGER { user(1), node(2) }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "This object determines the type of the ATM device. This
                object is used in automatic ATM Interface-Type determination
                procedure such that a correct operational ATM
                Interface-type can be determined. An ATM End System
                shall take the value of user(1), and an ATM network
                node shall take the value of node(2)."
        ::= { atmfAtmLayerEntry 10 }

atmfAtmLayerIlmiVersion OBJECT-TYPE
        SYNTAX  INTEGER { unsupported(1), version4point0(2) }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "An indication of the latest version of the ATM Forum
                ILMI Specification that is supported on this ATM Interface.

                If the peer IME's value of this object is the same as,
                or later than the local IME's value, then the version
                corresponding to the local IME's value should be
                attempted.  Otherwise, if the peer IME's value of this
                object is earlier, and supported locally, then the
                local IME should attempt the version corresponding to
                the peer IME's value.  Otherwise, compatibility of the
                two IMEs cannot be assumed.

                If this object is not present, a version of the ILMI earlier
                than 4.0 is supported."
        ::= { atmfAtmLayerEntry 11 }

atmfAtmLayerNniSigVersion OBJECT-TYPE
        SYNTAX  INTEGER { unsupported(1), iisp(2),
                          pnniVersion1point0(3) }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "An indication of the latest version of the ATM Forum
                PNNI Signalling Specification that is supported on this
                ATM Interface. Note that the PNNI routing version is not
                determined through ILMI.

                If the peer IME's value of this object is the same as,
                or later than the local IME's value, then the version
                corresponding to the local IME's value should be
                attempted.  Otherwise, if the peer IME's value of this
                object is earlier, and supported locally, then the
                local IME should attempt the version corresponding to
                the peer IME's value.  Otherwise, compatibility of the
                two IMEs cannot be assumed."
        ::= { atmfAtmLayerEntry 12 }

atmfAtmLayerMaxSvpcVpi OBJECT-TYPE
        SYNTAX  INTEGER (0..4096)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
               "The maximum VPI that the signalling stack on the ATM
                interface is configured to support for allocation to
                switched virtual path connections."
        ::= { atmfAtmLayerEntry 13 }

atmfAtmLayerMaxSvccVpi OBJECT-TYPE
        SYNTAX  INTEGER (0..4096)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The maximum VPI that the signalling stack on the ATM
                interface is configured to support for allocation to
                switched virtual channel connections."
        ::= { atmfAtmLayerEntry 14 }

atmfAtmLayerMinSvccVci OBJECT-TYPE
        SYNTAX  INTEGER (0..65536)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "This is the minimum VCI value that the
                signalling stack is configured to support for
                allocation to switched virtual channel connections.  The same
                value applies to all SVCC VPI values for which the
                signalling stack is configured."
        ::= { atmfAtmLayerEntry 15 }



atmfAtmStatsTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF AtmfAtmStatsEntry
        ACCESS  not-accessible
        STATUS  deprecated
        DESCRIPTION
                "This group is deprecated and should not be implemented
                 except as required for backward compatibility with version
                 3.1 of the UNI specification."
        ::= { atmfAtmStatsGroup 1 }

atmfAtmStatsEntry OBJECT-TYPE
        SYNTAX  AtmfAtmStatsEntry
        ACCESS  not-accessible
        STATUS  deprecated
        DESCRIPTION
                "This object should not be implemented except as
                required for backward compatibility with version 3.1
                of the UNI specification."
        INDEX   { atmfAtmStatsIndex }
        ::= { atmfAtmStatsTable 1 }

AtmfAtmStatsEntry ::=
        SEQUENCE {
                atmfAtmStatsIndex
                        INTEGER,
                atmfAtmStatsReceivedCells
                        Counter,
                atmfAtmStatsDroppedReceivedCells
                        Counter,
                atmfAtmStatsTransmittedCells
                        Counter
        }

atmfAtmStatsIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..2147483647)
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
                "This object should not be implemented except as
                required for backward compatibility with version 3.1
                of the UNI specification."
        ::= { atmfAtmStatsEntry 1 }

atmfAtmStatsReceivedCells OBJECT-TYPE
        SYNTAX  Counter
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
                "This object should not be implemented except as
                required for backward compatibility with version 3.1
                of the UNI specification."
       ::= { atmfAtmStatsEntry 2 }

atmfAtmStatsDroppedReceivedCells OBJECT-TYPE
        SYNTAX  Counter
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
                "This object should not be implemented except as
                required for backward compatibility with version 3.1
                of the UNI specification."
        ::= { atmfAtmStatsEntry 3 }

atmfAtmStatsTransmittedCells OBJECT-TYPE
        SYNTAX  Counter
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
                "This object should not be implemented except as
                required for backward compatibility with version 3.1
                of the UNI specification."
       ::= { atmfAtmStatsEntry 4 }



atmfVpcTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF AtmfVpcEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
                "A table of status and parameter information on the
                virtual path connections which cross this ATM
                Interface. There is one entry in this table for each
                permanent virtual path connection."
        ::= { atmfVpcGroup 1 }

atmfVpcEntry OBJECT-TYPE
        SYNTAX  AtmfVpcEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
                "An entry in the table, containing information about a
                particular virtual path connection."
        INDEX   { atmfVpcPortIndex, atmfVpcVpi }
        ::= { atmfVpcTable 1 }

AtmfVpcEntry ::=
        SEQUENCE {
                atmfVpcPortIndex
                        INTEGER,
                atmfVpcVpi
                        INTEGER,
                atmfVpcOperStatus
                        INTEGER,
                atmfVpcTransmitTrafficDescriptorType
                        OBJECT IDENTIFIER,
                atmfVpcTransmitTrafficDescriptorParam1
                        INTEGER,
                atmfVpcTransmitTrafficDescriptorParam2
                        INTEGER,
                atmfVpcTransmitTrafficDescriptorParam3
                        INTEGER,
                atmfVpcTransmitTrafficDescriptorParam4
                        INTEGER,
                atmfVpcTransmitTrafficDescriptorParam5
                        INTEGER,
                atmfVpcReceiveTrafficDescriptorType
                        OBJECT IDENTIFIER,
                atmfVpcReceiveTrafficDescriptorParam1
                        INTEGER,
                atmfVpcReceiveTrafficDescriptorParam2
                        INTEGER,
                atmfVpcReceiveTrafficDescriptorParam3
                        INTEGER,
                atmfVpcReceiveTrafficDescriptorParam4
                        INTEGER,
                atmfVpcReceiveTrafficDescriptorParam5
                        INTEGER,
                atmfVpcQoSCategory
                        INTEGER,
                atmfVpcTransmitQoSClass
                        INTEGER,
                atmfVpcReceiveQoSClass
                        INTEGER,
                atmfVpcBestEffortIndicator
                        TruthValue,
                atmfVpcServiceCategory
                        AtmServiceCategory
        }

atmfVpcPortIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..2147483647)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The value of 0 which has the special meaning of
                identifying the ATM Interface over which this message
                was received."
        ::= { atmfVpcEntry 1 }

atmfVpcVpi OBJECT-TYPE
        SYNTAX  INTEGER (0..4095)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The VPI value of this Virtual Path Connection at the
                local ATM Interface."
        ::= { atmfVpcEntry 2 }

atmfVpcOperStatus OBJECT-TYPE
        SYNTAX  INTEGER {
                        unknown(1),
                        end2endUp(2),
                        end2endDown(3),
                        localUpEnd2endUnknown(4),
                        localDown(5)
                }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The present actual operational status of the VPC.

                A value of end2endUp(2) or end2endDown(3) would be
                used if the end-to-end status is known. If only local
                status information is available, a value of
                localUpEnd2endUnknown(4) or localDown(5) would be
                used."
        ::= { atmfVpcEntry 3 }

atmfVpcTransmitTrafficDescriptorType OBJECT-TYPE
        SYNTAX  OBJECT IDENTIFIER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The type of traffic management, applicable to the
                transmit direction of this VPC. The type may indicate
                none, or a type with one or more parameters. These
                parameters are specified as a parameter vector, in the
                corresponding instances of the objects:
                        atmfVpcTransmitTrafficDescriptorParam1,
                        atmfVpcTransmitTrafficDescriptorParam2,
                        atmfVpcTransmitTrafficDescriptorParam3,
                        atmfVpcTransmitTrafficDescriptorParam4, and
                        atmfVpcTransmitTrafficDescriptorParam5."
        ::= { atmfVpcEntry 4 }

atmfVpcTransmitTrafficDescriptorParam1 OBJECT-TYPE
        SYNTAX  INTEGER (0..2147483647)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The first parameter of the transmit parameter vector
                for this VPC, used according to the value of
                atmfVpcTransmitTrafficDescriptorType."
        ::= { atmfVpcEntry 5 }

atmfVpcTransmitTrafficDescriptorParam2 OBJECT-TYPE
        SYNTAX  INTEGER (0..2147483647)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The second parameter of the transmit parameter vector
                for this VPC, used according to the value of
                atmfVpcTransmitTrafficDescriptorType."
        ::= { atmfVpcEntry 6 }

atmfVpcTransmitTrafficDescriptorParam3 OBJECT-TYPE
        SYNTAX  INTEGER (0..2147483647)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The third parameter of the transmit parameter vector
                for this VPC, used according to the value of
                atmfVpcTransmitTrafficDescriptorType."
        ::= { atmfVpcEntry 7 }

atmfVpcTransmitTrafficDescriptorParam4 OBJECT-TYPE
        SYNTAX  INTEGER (0..2147483647)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The fourth parameter of the transmit parameter vector
                for this VPC, used according to the value of
                atmfVpcTransmitTrafficDescriptorType."
        ::= { atmfVpcEntry 8 }

atmfVpcTransmitTrafficDescriptorParam5 OBJECT-TYPE
        SYNTAX  INTEGER (0..2147483647)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The fifth parameter of the transmit parameter vector
                for this VPC, used according to the value of
                atmfVpcTransmitTrafficDescriptorType."
        ::= { atmfVpcEntry 9 }

atmfVpcReceiveTrafficDescriptorType OBJECT-TYPE
        SYNTAX  OBJECT IDENTIFIER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The type of traffic management, applicable to the
                traffic in the receive direction of this VPC. The type
                may indicate none, or a type with one or more
                parameters. These parameters are specified as a
                parameter vector, in the corresponding instances of
                the objects:
                        atmfVpcReceiveTrafficDescriptorParam1,
                        atmfVpcReceiveTrafficDescriptorParam2,
                        atmfVpcReceiveTrafficDescriptorParam3,
                        atmfVpcReceiveTrafficDescriptorParam4, and
                        atmfVpcReceiveTrafficDescriptorParam5."
       ::= { atmfVpcEntry 10 }

atmfVpcReceiveTrafficDescriptorParam1 OBJECT-TYPE
        SYNTAX  INTEGER (0..2147483647)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The first parameter of the receive parameter vector
                for this VPC, used according to the value of
                atmfVpcReceiveTrafficDescriptorType."
        ::= { atmfVpcEntry 11 }

atmfVpcReceiveTrafficDescriptorParam2 OBJECT-TYPE
        SYNTAX  INTEGER (0..2147483647)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The second parameter of the receive parameter vector
                for this VPC, used according to the value of
                atmfVpcReceiveTrafficDescriptorType."
       ::= { atmfVpcEntry 12 }

atmfVpcReceiveTrafficDescriptorParam3 OBJECT-TYPE
        SYNTAX  INTEGER (0..2147483647)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The third parameter of the receive parameter vector
                for this VPC, used according to the value of
                atmfVpcReceiveTrafficDescriptorType."
        ::= { atmfVpcEntry 13 }

atmfVpcReceiveTrafficDescriptorParam4 OBJECT-TYPE
        SYNTAX  INTEGER (0..2147483647)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The fourth parameter of the receive parameter vector
                for this VPC, used according to the value of
                atmfVpcReceiveTrafficDescriptorType."
       ::= { atmfVpcEntry 14 }

atmfVpcReceiveTrafficDescriptorParam5 OBJECT-TYPE
        SYNTAX  INTEGER (0..2147483647)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The fifth parameter of the receive parameter vector
                for this VPC, used according to the value of
                atmfVpcReceiveTrafficDescriptorType."
       ::= { atmfVpcEntry 15 }

atmfVpcQoSCategory OBJECT-TYPE
        SYNTAX  INTEGER {
                        other(1),
                        deterministic (2),
                        statistical (3),
                        unspecified (4)
                }
        ACCESS  read-only
        STATUS  obsolete
        DESCRIPTION
                "This object should not be implemented except as
                required for backward compatibility with version 2.0
                of the UNI specification."
        ::= { atmfVpcEntry 16 }

atmfVpcTransmitQoSClass OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
                "This object should not be implemented except as
                required for backward compatibility with version 3.1
                of the UNI specification."
        ::= { atmfVpcEntry 17 }

atmfVpcReceiveQoSClass OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
                "This object should not be implemented except as
                required for backward compatibility with version 3.1
                of the UNI specification."
        ::= { atmfVpcEntry 18 }

atmfVpcBestEffortIndicator OBJECT-TYPE
        SYNTAX  TruthValue
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The object is examined when
                atmfVpcTransmitTrafficDescriptorType or
                atmfVpcReceiveTrafficDescriptorType for the associated
                connection is equal to atmfNoClpNoScr.
                If this object is set to false(2), the network is requested
                to apply the CBR.1 conformance definition. If this object
                is set to true(1), the network is requested to apply the
                UBR.1 conformance definition."
        ::= { atmfVpcEntry 19 }

atmfVpcServiceCategory OBJECT-TYPE
        SYNTAX  AtmServiceCategory
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The service category of this virtual path connection."
        ::= { atmfVpcEntry 20 }



atmfVccTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF AtmfVccEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
                "A table of status and parameter information on the
                virtual channel connections which are visible at this
                ATM Interface. There is one entry in this table for
                each permanent virtual channel connection, including
                reserved VCCs that are supported; e.g., signalling,
                OAM flows, and ILMI, but not unassigned cells."
        ::= { atmfVccGroup 1 }

atmfVccEntry OBJECT-TYPE
        SYNTAX  AtmfVccEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
                "An entry in the table, containing information about a
                particular virtual channel connection."
        INDEX   { atmfVccPortIndex, atmfVccVpi, atmfVccVci }
        ::= { atmfVccTable 1 }

AtmfVccEntry ::=
        SEQUENCE {
                atmfVccPortIndex
                        INTEGER,
                atmfVccVpi
                        INTEGER,
                atmfVccVci
                        INTEGER,
                atmfVccOperStatus
                        INTEGER,
                atmfVccTransmitTrafficDescriptorType
                        OBJECT IDENTIFIER,
                atmfVccTransmitTrafficDescriptorParam1
                        INTEGER,
                atmfVccTransmitTrafficDescriptorParam2
                        INTEGER,
                atmfVccTransmitTrafficDescriptorParam3
                        INTEGER,
                atmfVccTransmitTrafficDescriptorParam4
                        INTEGER,
                atmfVccTransmitTrafficDescriptorParam5
                        INTEGER,
                atmfVccReceiveTrafficDescriptorType
                        OBJECT IDENTIFIER,
                atmfVccReceiveTrafficDescriptorParam1
                        INTEGER,
                atmfVccReceiveTrafficDescriptorParam2
                        INTEGER,
                atmfVccReceiveTrafficDescriptorParam3
                        INTEGER,
                atmfVccReceiveTrafficDescriptorParam4
                        INTEGER,
                atmfVccReceiveTrafficDescriptorParam5
                        INTEGER,
                atmfVccQoSCategory
                        INTEGER,
                atmfVccTransmitQoSClass
                        INTEGER,
                atmfVccReceiveQoSClass
                        INTEGER,
                atmfVccBestEffortIndicator
                        TruthValue,
                atmfVccTransmitFrameDiscard
                        TruthValue,
                atmfVccReceiveFrameDiscard
                        TruthValue,
                atmfVccServiceCategory
                        AtmServiceCategory
        }

atmfVccPortIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..2147483647)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The value of 0 which has the special meaning of
                identifying the ATM Interface over which this message
                was received."
        ::= { atmfVccEntry 1 }

atmfVccVpi OBJECT-TYPE
        SYNTAX  INTEGER (0..4095)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The VPI value of this Virtual Channel Connection at
                the local ATM Interface. For virtual interfaces (i.e.
                Virtual Path Connections), this value has no meaning
                and is set to zero "
        ::= { atmfVccEntry 2 }

atmfVccVci OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The VCI value of this Virtual Channel Connection at
                the local ATM Interface."
       ::= { atmfVccEntry 3 }

atmfVccOperStatus OBJECT-TYPE
        SYNTAX  INTEGER {
                        unknown(1),
                        end2endUp(2),
                        end2endDown(3),
                        localUpEnd2endUnknown(4),
                        localDown(5)
                }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The present actual operational status of the VCC. A
                value of end2endUp(2) or end2endUp(3) is used if the
                end to end status is known.

                If only local status is known a value of
                localUpEnd2endUnknown(4) or localDown(5) is used."
        ::= { atmfVccEntry 4 }

atmfVccTransmitTrafficDescriptorType OBJECT-TYPE
        SYNTAX  OBJECT IDENTIFIER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The type of traffic management, applicable to the
                transmit direction of this VCC. The type may indicate
                none, or a type with one or more parameters. These
                parameters are specified as a parameter vector, in the
                corresponding instances of the objects:
                        atmfVccTransmitTrafficDescriptorParam1,
                        atmfVccTransmitTrafficDescriptorParam2,
                        atmfVccTransmitTrafficDescriptorParam3,
                        atmfVccTransmitTrafficDescriptorParam4, and
                        atmfVccTransmitTrafficDescriptorParam5."
        ::= { atmfVccEntry 5 }

atmfVccTransmitTrafficDescriptorParam1 OBJECT-TYPE
        SYNTAX  INTEGER (0..2147483647)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The first parameter of the transmit parameter vector
                for this VCC, used according to the value of
                atmfVccTransmitTrafficDescriptorType."
        ::= { atmfVccEntry 6 }

atmfVccTransmitTrafficDescriptorParam2 OBJECT-TYPE
        SYNTAX  INTEGER (0..2147483647)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The second parameter of the transmit parameter vector
                for this VCC, used according to the value of
                atmfVccTransmitTrafficDescriptorType."
       ::= { atmfVccEntry 7 }

atmfVccTransmitTrafficDescriptorParam3 OBJECT-TYPE
        SYNTAX  INTEGER (0..2147483647)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The third parameter of the transmit parameter vector
                for this VCC, used according to the value of
                atmfVccTransmitTrafficDescriptorType."
       ::= { atmfVccEntry 8 }

atmfVccTransmitTrafficDescriptorParam4 OBJECT-TYPE
        SYNTAX  INTEGER (0..2147483647)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The fourth parameter of the transmit parameter vector
                for this VCC, used according to the value of
                atmfVccTransmitTrafficDescriptorType."
       ::= { atmfVccEntry 9 }

atmfVccTransmitTrafficDescriptorParam5 OBJECT-TYPE
        SYNTAX  INTEGER (0..2147483647)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The fifth parameter of the transmit parameter vector
                for this VCC, used according to the value of
                atmfVccTransmitTrafficDescriptorType."
       ::= { atmfVccEntry 10 }

atmfVccReceiveTrafficDescriptorType OBJECT-TYPE
        SYNTAX  OBJECT IDENTIFIER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The type of traffic management, applicable to the
                traffic in the receive direction of this VCC. The type
                may indicate none, or a type with one or more
                parameters. These parameters are specified as a
                parameter vector, in the corresponding instances of
                the objects:
                        atmfVccReceiveTrafficDescriptorParam1,
                        atmfVccReceiveTrafficDescriptorParam2,
                        atmfVccReceiveTrafficDescriptorParam3,
                        atmfVccReceiveTrafficDescriptorParam4, and
                        atmfVccReceiveTrafficDescriptorParam5."
        ::= { atmfVccEntry 11 }

atmfVccReceiveTrafficDescriptorParam1 OBJECT-TYPE
        SYNTAX  INTEGER (0..2147483647)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The first parameter of the receive parameter vector
                for this VCC, used according to the value of
                atmfVccReceiveTrafficDescriptorType."
     ::= { atmfVccEntry 12 }

atmfVccReceiveTrafficDescriptorParam2 OBJECT-TYPE
        SYNTAX  INTEGER (0..2147483647)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The second parameter of the receive parameter vector
                for this VCC, used according to the value of
                atmfVccReceiveTrafficDescriptorType."
        ::= { atmfVccEntry 13 }

atmfVccReceiveTrafficDescriptorParam3 OBJECT-TYPE
        SYNTAX  INTEGER (0..2147483647)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The third parameter of the receive parameter vector
                for this VCC, used according to the value of
                atmfVccReceiveTrafficDescriptorType."
      ::= { atmfVccEntry 14 }

atmfVccReceiveTrafficDescriptorParam4 OBJECT-TYPE
        SYNTAX  INTEGER (0..2147483647)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The fourth parameter of the receive parameter vector
                for this VCC, used according to the value of
                atmfVccReceiveTrafficDescriptorType."
      ::= { atmfVccEntry 15 }

atmfVccReceiveTrafficDescriptorParam5 OBJECT-TYPE
        SYNTAX  INTEGER (0..2147483647)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The fifth parameter of the receive parameter vector
                for this VCC, used according to the value of
                atmfVccReceiveTrafficDescriptorType."
      ::= { atmfVccEntry 16 }

atmfVccQoSCategory OBJECT-TYPE
        SYNTAX  INTEGER {
                        other(1),
                        deterministic(2),
                        statistical(3),
                        unspecified(4)
                }
        ACCESS  read-only
        STATUS  obsolete
        DESCRIPTION
                "This object should not be implemented except as
                required for backward compatibility with version 2.0
                of the UNI specification."
       ::= { atmfVccEntry 17 }

 atmfVccTransmitQoSClass OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
                "This object should not be implemented except as
                required for backward compatibility with version 3.1
                of the UNI specification."
       ::= { atmfVccEntry 18 }

atmfVccReceiveQoSClass OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
                "This object should not be implemented except as
                required for backward compatibility with version 3.1
                of the UNI specification."
       ::= { atmfVccEntry 19 }

atmfVccBestEffortIndicator OBJECT-TYPE
        SYNTAX  TruthValue
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The object is examined when
                atmfVccTransmitTrafficDescriptorType or
                atmfVccReceiveTrafficDescriptorType for the associated
                connection is equal to atmfNoClpNoScr.
                If this object is set to false(2), the network is requested
                to apply the CBR.1 conformance definition. If this object
                is set to true(1), the network is requested to apply the
                UBR.1 conformance definition."
        ::= { atmfVccEntry 20 }

atmfVccTransmitFrameDiscard OBJECT-TYPE
        SYNTAX  TruthValue
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "If set to true(1), this object indicates that the network
                is requested to treat data for this connection (in the
                transmit direction) as frames (e.g. AAL5 CPCS_PDU's) rather
                than as individual cells.  While the precise
                implementation is network-specific, this treatment may
                for example involve discarding entire frames during
                congestion, rather than a few cells from many frames.
                The default value is false(2)."
        ::= { atmfVccEntry 21 }

atmfVccReceiveFrameDiscard OBJECT-TYPE
        SYNTAX  TruthValue
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "If set to true(1), this object indicates that the network
                is requested to treat data for this connection (in the
                receive direction) as frames (e.g. AAL5 CPCS_PDU's) rather
                than as individual cells.  While the precise
                implementation is network-specific, this treatment may
                for example involve discarding entire frames during
                congestion, rather than a few cells from many frames.
                The default value is false(2)."
       ::= { atmfVccEntry 22 }

atmfVccServiceCategory OBJECT-TYPE
        SYNTAX  AtmServiceCategory
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The service category of this virtual channel connection."
        ::= { atmfVccEntry 23 }


atmfVpcChange TRAP-TYPE
        ENTERPRISE      atmForum
        VARIABLES       { atmfVpcPortIndex, atmfVpcVpi, atmfVpcOperStatus }
        DESCRIPTION
                "An atmfVpcChange trap indicates that a permanent VPC has been
                added or deleted at this ATM Interface or that the attributes
                of an existing VPC have been modified. The variables
                included in the trap identify the VPI value of the
                reconfigured VPC at this ATM Interface."
        ::= 1

atmfVccChange TRAP-TYPE
        ENTERPRISE      atmForum
        VARIABLES       { atmfVccPortIndex, atmfVccVci, atmfVccVpi,
                          atmfVccOperStatus }
        DESCRIPTION
                "An atmfVccChange trap indicates that a permanent VCC has been 
                added or deleted at this ATM Interface or that the attributes
                of an existing VCC have been modified.. The variables
                included in the trap identify the VCI and VPI values
                of the reconfigured VCC at this ATM
                Interface."
        ::= 2



atmfNetPrefixTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF AtmfNetPrefixEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
                "A table implemented by the user-side IME, containing the
                network-prefix(es) for ATM-layer addresses in effect on
                the user side of the UNI."
        ::= { atmfNetPrefixGroup 1 }

atmfNetPrefixEntry OBJECT-TYPE
        SYNTAX  AtmfNetPrefixEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
                "Information about a single network-prefix for
                ATM-layer addresses in effect on the user-side IME.
                Note that the index variable atmNetPrefixPrefix is a
                variable-length string, and as such the rule for
                variable-length strings in section 4.1.6 of RFC 1212
                applies."

        INDEX   { atmfNetPrefixPort, atmfNetPrefixPrefix }
        ::= { atmfNetPrefixTable 1 }

AtmfNetPrefixEntry ::=
        SEQUENCE {
                atmfNetPrefixPort
                        INTEGER,
                atmfNetPrefixPrefix
                        NetPrefix,
                atmfNetPrefixStatus
                        INTEGER
        }

atmfNetPrefixPort OBJECT-TYPE
        SYNTAX  INTEGER (0..2147483647)
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
                "A unique value which identifies the UNI port for
                which the network prefix for ATM addresses is in
                effect.  The value of 0 has the special meaning of
                identifying the local UNI."
        ::= { atmfNetPrefixEntry 1 }

atmfNetPrefixPrefix  OBJECT-TYPE
        SYNTAX  NetPrefix
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
                "The network prefix for ATM addresses which is in
                effect on the user side of the ATM UNI port."
        ::= { atmfNetPrefixEntry 2 }

atmfNetPrefixStatus  OBJECT-TYPE
        SYNTAX  INTEGER { valid(1), invalid(2) }
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
                "An indication of the validity of the network prefix
                for ATM addresses on the user side of the UNI port.
                To configure a new network prefix in this table, the
                network-side IME must set the appropriate instance of this
                object to the value valid(1).  To delete an existing
                network prefix in this table, the network-side IME must
                set the appropriate instance of this object to the
                value invalid(2).

                If circumstances occur on the user-side IME which cause a
                prefix to become invalid, the user-side IME modifies the
                value of the appropriate instance of this object to invalid(2).

                Whenever the value of this object for a particular
                prefix becomes invalid(2), the conceptual row for that
                prefix may be removed from the table at any time,
                either immediately or subsequently."
       ::= { atmfNetPrefixEntry 3 }



atmfAddressTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF AtmfAddressEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
                "A table implemented by the network-side IME, containing the
                ATM-layer addresses in effect on the user side of the UNI."
        ::= { atmfAddressGroup 1 }

atmfAddressEntry OBJECT-TYPE
        SYNTAX  AtmfAddressEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
                "Information about a single ATM-layer address in effect
                on the user-side IME.  Note that the index variable
                atmAddressAtmAddress is a variable-length string, and as
                such the rule for variable-length strings in section
                4.1.6 of RFC 1212 applies."
        INDEX   { atmfAddressPort, atmfAddressAtmAddress }
        ::= { atmfAddressTable 1 }

AtmfAddressEntry ::=
        SEQUENCE {
                atmfAddressPort
                        INTEGER,
                atmfAddressAtmAddress
                        AtmAddress,
                atmfAddressStatus
                        INTEGER,
                atmfAddressOrgScope
                        INTEGER
        }

atmfAddressPort OBJECT-TYPE
        SYNTAX  INTEGER (0..2147483647)
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
                "A unique value which identifies the UNI port for
                which the ATM address is in effect.  The value of 0
                has the special meaning of identifying the local UNI."
        ::= { atmfAddressEntry 1 }

atmfAddressAtmAddress  OBJECT-TYPE
        SYNTAX  AtmAddress
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
                "The ATM address which is in effect on the user side
                of the ATM UNI port."
        ::= { atmfAddressEntry 2 }

atmfAddressStatus  OBJECT-TYPE
        SYNTAX  INTEGER { valid(1), invalid(2) }
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
                "An indication of the validity of the ATM address at
                the user side of the UNI port.  To configure a new
                address in this table, the user-side IME must set the
                appropriate instance of this object to the value
                valid(1).  To delete an existing address in this table,
                the user-side IME must set the appropriate instance of
                this object to the value invalid(2).

                If circumstances occur on the network-side IME which cause
                an address to become invalid, the network-side IME
                modifies the value of the appropriate instance of this
                object to invalid(2).

                Whenever the value of this object for a particular
                address becomes invalid(2), the conceptual row for
                that address may be removed from the table at any
                time, either immediately or subsequently."
         ::= { atmfAddressEntry 3 }

atmfAddressOrgScope OBJECT-TYPE
        SYNTAX  INTEGER {
                localNetwork(1),
                localNetworkPlusOne(2),
                localNetworkPlusTwo(3),
                siteMinusOne(4),
                intraSite(5), 
                sitePlusOne(6),
                organizationMinusOne(7),
                intraOrganization(8),
                organizationPlusOne(9),
                communityMinusOne(10),
                intraCommunity(11),
                communityPlusOne(12),
                regional(13),
                interRegional(14),
                global(15)
        }
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION 
                "This object indicates the organizational
                scope for the referenced address. The information of
                the referenced address shall not be distributed
                outside the indicated scope. If the user-side IME does
                not specify a value for the atmfAddressOrgScope object,
                the network shall set the value of this object to
                localNetwork(1), if the registered address is an ATM group
                address, or to global(15), if the registered address is 
                an individual address.  Refer to Annex 6.0
                of ATM Forum UNI Signalling 4.0 for guidelines regarding
                the use of organizational scopes.

                This organization hierarchy may be mapped to ATM network's
                routing hierarchy such as PNNI's routing level and
                the mapping shall be configurable in
                nodes. Use of this object in a public network is for
                further study.
                The default values for organizational scope are
                localNetwork(1) for ATM group addresses, and global(15)
                for individual addresses."
       ::= { atmfAddressEntry 4 }



atmfAddressRegistrationAdminTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF AtmfAddressRegistrationAdminEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
                "A table of Address Registration administrative
                information for the ATM Interface."
    ::= { atmfAddressRegistrationAdminGroup 1 }

atmfAddressRegistrationAdminEntry OBJECT-TYPE
        SYNTAX  AtmfAddressRegistrationAdminEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
                "An entry in the table, containing Address
                Registration administrative information for the ATM
                Interface."
        INDEX   { atmfAddressRegistrationAdminIndex }
        ::= { atmfAddressRegistrationAdminTable 1 }


AtmfAddressRegistrationAdminEntry ::=
        SEQUENCE {
                atmfAddressRegistrationAdminIndex
                        INTEGER,
                atmfAddressRegistrationAdminStatus
                        INTEGER
        }

atmfAddressRegistrationAdminIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..2147483647)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "The value of 0 which has the special meaning of
                identifying the ATM Interface over which this message
                was received."
         ::= { atmfAddressRegistrationAdminEntry 1 }

atmfAddressRegistrationAdminStatus OBJECT-TYPE
        SYNTAX  INTEGER { supported(1), unsupported(2) }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "An indication of whether or not Address Registration
                is supported on this ATM Interface. Supported(1)
                indicates that this ATM Interface supports address
                registration. Unsupported(2) indicates that this ATM
                Interface does not support address registration."
         ::= { atmfAddressRegistrationAdminEntry 2 }



atmfSrvcRegLecs         OBJECT IDENTIFIER ::= { atmfSrvcRegTypes 1 }

atmfSrvcRegAns         OBJECT IDENTIFIER ::= { atmfSrvcRegTypes 2 }


END

