All utilities are located in /opt/SUNWstade, see the man pages for more details

Program | Description
--- | ---
bin/checkcron | If executed from the command line, this executable program verifies that the executable program "rasagent" is entered in the `crontab(1M)` file. Note: You must be root to run this program.
bin/clearcache | If executed from the command line, this executable program will remove the instrumentation information for all the configured devices from the CACHE. This is typically used during testing purposes so that a DiscoveryEvent can be forced to occur upon the next execution of the Storage Automated Diagnostic Environment Agent.
disk_inquiry | Used by Storage Automated Diagnostic Environment to discover devices on the data-path that are using SCSI commands.
bin/ras_admin | performs common Storage Automated Diagnostic Environment administrative tasks from the command line interface (CLI).
bin/ras_install | This program will set-up the HTTP service, add a cron and register with the master Storage Automated Diagnostic Environment Agent in the case of a slave install. It must be run manually upon completing the 'pkgadd'. This program can be executed anytime after the initial execution and setup when a modification to the cron is desired or to change the Master/Slave title of a Host agent. Refer to the User's Guide before making changes.
bin/ras_revcheck | Checks the software, hardware, and firmware revision levels of all user-selected modules. The report displays the current revision, the expected revision, and upgrade information.
bin/ras_fccheck | Utility is used to provide a check of available Fibre Channel counters to verify link integrity. ras_fccheck utility probes the device counters and creates an initial baseline for comparison. After a short period of time, the ras_fccheck utility again compares the device counters and compares them to the baseline to determine if problems exist.
bin/rasagent | This is the executable program that calls the modules for the different Network Storage Devices supported by this monitoring agent. It is executed automatically by cron or can be run manually from the command line. Keep in mid however, if run from the command line, rasagent will first check that another process for rasagent is not already running.
bin/save_password | Utility used by the system administrator to change the password to Storage Automated Diagnostic Environment's graphical user interface. Changing the password can also be performed in the GUI itself. However this utility would be used from the command line when the administrator forgot the password. Usage: save_password <password>
bin/sanbox | Utility used by Storage Automated Diagnostic Environment to gather Fibre Channel Switch information.
bin/testt3 | Verify that the tokens of a specific T3 are working. T3 token files elemprop.html and sysprop.html must be available for the Storage Automated Diagnostic Environment probing capabilities to work properly. Running this utility from the command will require that the IP Address of the T3 being probed is known. Usage: testt3 <ip_address>